;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Size##OTHER##;Shape##OTHER##;ProductInformation##OTHER##;ModelReference##OTHER##;Material##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Length##LENGTH##MILLIMETERS;Description##OTHER##;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP_Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;CreatedOn##OTHER##;Control Gear##OTHER##;Color##OTHER##;Body##OTHER##;BarCode##OTHER##;BIMObjectName##OTHER##;ArticleNumber##OTHER##;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;ColorRenderingIndex##Other##;Vik Big##OTHER##
VIK SMALL LED CLEAR LL 830_65700;225;2.2;3000;L 220 mm + W 225 mm + H 244 mm;Rectangle;Body of aluminium. Diffuser of impact resistant opal or clear acrylic.;Vik LED;aluminium;939;Wall;Surface;220;A wall mounted luminaire in two sizes with a timeless design suitable for most environments. The opal diffuser creates a well-balanced luminance on wall, while the clear shade offers a more direct light.;939;3000;3000;44;244;106;Created 22/08/2018;Standard;Grey (NCS 6000);Fagerhult_Alugrey_Aluminium;7320046697570;Vik LED;65700;9;min. 80;0
VIK SMALL LED CLEAR HL 830_65701;225;2.2;3000;L 220 mm + W 225 mm + H 244 mm;Rectangle;Body of aluminium. Diffuser of impact resistant opal or clear acrylic.;Vik LED;aluminium;1780;Wall;Surface;220;A wall mounted luminaire in two sizes with a timeless design suitable for most environments. The opal diffuser creates a well-balanced luminance on wall, while the clear shade offers a more direct light.;1780;3000;3000;44;244;129;Created 22/08/2018;Standard;Grey (NCS 6000);Fagerhult_Alugrey_Aluminium;7320046697587;Vik LED;65701;14;min. 80;0
VIK SMALL LED CLEAR LL 840_65702;225;2.2;4000;L 220 mm + W 225 mm + H 244 mm;Rectangle;Body of aluminium. Diffuser of impact resistant opal or clear acrylic.;Vik LED;aluminium;958;Wall;Surface;220;A wall mounted luminaire in two sizes with a timeless design suitable for most environments. The opal diffuser creates a well-balanced luminance on wall, while the clear shade offers a more direct light.;958;4000;4000;44;244;108;Created 22/08/2018;Standard;Grey (NCS 6000);Fagerhult_Alugrey_Aluminium;7320046697594;Vik LED;65702;9;min. 80;0
VIK SMALL LED CLEAR HL 840_65703;225;2.2;4000;L 220 mm + W 225 mm + H 244 mm;Rectangle;Body of aluminium. Diffuser of impact resistant opal or clear acrylic.;Vik LED;aluminium;1816;Wall;Surface;220;A wall mounted luminaire in two sizes with a timeless design suitable for most environments. The opal diffuser creates a well-balanced luminance on wall, while the clear shade offers a more direct light.;1816;4000;4000;44;244;132;Created 22/08/2018;Standard;Grey (NCS 6000);Fagerhult_Alugrey_Aluminium;7320046700522;Vik LED;65703;14;min. 80;0
VIK SMALL LED OPAL LL 830_65704;225;2.2;3000;L 220 mm + W 225 mm + H 244 mm;Rectangle;Body of aluminium. Diffuser of impact resistant opal or clear acrylic.;Vik LED;aluminium;661;Wall;Surface;220;A wall mounted luminaire in two sizes with a timeless design suitable for most environments. The opal diffuser creates a well-balanced luminance on wall, while the clear shade offers a more direct light.;661;3000;3000;44;244;56;Created 22/08/2018;Standard;Grey (NCS 6000);Fagerhult_Alugrey_Aluminium;7320046700607;Vik LED;65704;12;min. 80;0
VIK SMALL LED OPAL HL 830_65705;225;2.2;3000;L 220 mm + W 225 mm + H 244 mm;Rectangle;Body of aluminium. Diffuser of impact resistant opal or clear acrylic.;Vik LED;aluminium;1022;Wall;Surface;220;A wall mounted luminaire in two sizes with a timeless design suitable for most environments. The opal diffuser creates a well-balanced luminance on wall, while the clear shade offers a more direct light.;1022;3000;3000;44;244;69;Created 22/08/2018;Standard;Grey (NCS 6000);Fagerhult_Alugrey_Aluminium;7320046700614;Vik LED;65705;15;min. 80;0
VIK SMALL LED OPAL LL 840_65706;225;2.2;4000;L 220 mm + W 225 mm + H 244 mm;Rectangle;Body of aluminium. Diffuser of impact resistant opal or clear acrylic.;Vik LED;aluminium;674;Wall;Surface;220;A wall mounted luminaire in two sizes with a timeless design suitable for most environments. The opal diffuser creates a well-balanced luminance on wall, while the clear shade offers a more direct light.;674;4000;4000;44;244;57;Created 22/08/2018;Standard;Grey (NCS 6000);Fagerhult_Alugrey_Aluminium;7320046700621;Vik LED;65706;12;min. 80;0
VIK SMALL LED OPAL HL 840_65707;225;2.2;4000;L 220 mm + W 225 mm + H 244 mm;Rectangle;Body of aluminium. Diffuser of impact resistant opal or clear acrylic.;Vik LED;aluminium;1043;Wall;Surface;220;A wall mounted luminaire in two sizes with a timeless design suitable for most environments. The opal diffuser creates a well-balanced luminance on wall, while the clear shade offers a more direct light.;1043;4000;4000;44;244;70;Created 22/08/2018;Standard;Grey (NCS 6000);Fagerhult_Alugrey_Aluminium;7320046700638;Vik LED;65707;15;min. 80;0
VIK BIG LED CLEAR 2800LM 830_65708;287;4.3;3000;L 280 mm + W 287 mm + H 310 mm;Rectangle;Body of aluminium. Diffuser of impact resistant opal or clear acrylic.;Vik LED;aluminium;2829;Wall;Surface;280;A wall mounted luminaire in two sizes with a timeless design suitable for most environments. The opal diffuser creates a well-balanced luminance on wall, while the clear shade offers a more direct light.;2829;3000;3000;44;310;115;Created 22/08/2018;Standard;Grey (NCS 6000);Fagerhult_Alugrey_Aluminium;7320046700645;Vik LED;65708;25;min. 80;1
VIK BIG LED CLEAR 2800LM 840_65709;287;4.3;4000;L 280 mm + W 287 mm + H 310 mm;Rectangle;Body of aluminium. Diffuser of impact resistant opal or clear acrylic.;Vik LED;aluminium;2887;Wall;Surface;280;A wall mounted luminaire in two sizes with a timeless design suitable for most environments. The opal diffuser creates a well-balanced luminance on wall, while the clear shade offers a more direct light.;2887;4000;4000;44;310;117;Created 22/08/2018;Standard;Grey (NCS 6000);Fagerhult_Alugrey_Aluminium;7320046700652;Vik LED;65709;25;min. 80;1
