;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Installation##OTHER##
NOTOR 36 L LEFT PEND D DALI HL OPAL 840_16085-20237;563;1.4;4000;2566;Acrylic - Fagerhult - Opal;563;2566;4000;4000;20;36;118;White;Aluminium - Fagerhult - White;7320049576643;16085-20237;23;23;Notor 36 pendant Opal;Individual or system installation by means of wire suspension. Can also be wall mounted using the wall bracket. Wire brackets and friction locks are included in the delivery. Use Configure for wire suspension and mounting options.;"Luminaire with Opal louvre for pendent installation, individually or in a system. 
Choose between linear modules and shapes X, T, L, ceiling-to-wall and spotlight modules to freely create the system that best suits your project.";min. 80;C;1;1
NOTOR 36 L RIGHT PEND  DALI HL OPAL 840_16085-20238;563;1.4;4000;2566;Acrylic - Fagerhult - Opal;563;2566;4000;4000;20;36;118;White;Aluminium - Fagerhult - White;7320049576674;16085-20238;23;23;Notor 36 pendant Opal;Individual or system installation by means of wire suspension. Can also be wall mounted using the wall bracket. Wire brackets and friction locks are included in the delivery. Use Configure for wire suspension and mounting options.;"Luminaire with Opal louvre for pendent installation, individually or in a system. 
Choose between linear modules and shapes X, T, L, ceiling-to-wall and spotlight modules to freely create the system that best suits your project.";min. 80;C;1;1
