;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Type##OTHER##
NOTOR65 DYNAMIC BETAOPTI 1200 DI TW/TW WHT SINGLE_13677-402;65;4;4000;4227;Aluminium - Fagerhult - Beta Opti;1357;4227;4000;4000;20;190;95;White;Aluminium - Fagerhult - White;7316910589423;13677-402;47;47;Notor 65 Dynamic Beta Opti;"Single installation in wire suspension. For wire suspension installation, wire brackets are required for flexible c/c; ordered separately, see accessories.";Born out of research on Double Dynamic Lighting, Notor 65 Dynamic has a clear focus on lighting for humans. With diffuse direct/indirect light combined with directional light from a spotlight mounted in the side, dynamic and natural-like lighting is created. Beta Opti louvre shutters provide high efficiency and optimal light comfort and this, combined with the anti-glare spotlight, makes it possible to manage UGR16 and meet the maximum average luminance requirement at workplaces with monitors 3000cd/m2 at 65-90 degrees. Can be a good luminaire in your next WELL project.;min. 90;D/E;1;0
NOTOR65 DYNAMIC BETAOPTI 1200 DI TW/TW BLACK SINGLE_13678-402;65;4;4000;4200;Aluminium - Fagerhult - Beta Opti;1357;4200;4000;4000;20;190;95;Black;Aluminium - Fagerhult - Black;7316910589447;13678-402;47;47;Notor 65 Dynamic Beta Opti;"Single installation in wire suspension. For wire suspension installation, wire brackets are required for flexible c/c; ordered separately, see accessories.";Born out of research on Double Dynamic Lighting, Notor 65 Dynamic has a clear focus on lighting for humans. With diffuse direct/indirect light combined with directional light from a spotlight mounted in the side, dynamic and natural-like lighting is created. Beta Opti louvre shutters provide high efficiency and optimal light comfort and this, combined with the anti-glare spotlight, makes it possible to manage UGR16 and meet the maximum average luminance requirement at workplaces with monitors 3000cd/m2 at 65-90 degrees. Can be a good luminaire in your next WELL project.;min. 90;D/E;1;0
NOTOR65 DYNAMIC BETAOPTI 1200 DI 840/930 WHT SINGLE_13681-402;65;4;4000;4580;Aluminium - Fagerhult - Beta Opti;1357;4580;4000;4000;20;190;132;White;Aluminium - Fagerhult - White;7316910589584;13681-402;36;36;Notor 65 Dynamic Beta Opti;"Single installation in wire suspension. For wire suspension installation, wire brackets are required for flexible c/c; ordered separately, see accessories.";Born out of research on Double Dynamic Lighting, Notor 65 Dynamic has a clear focus on lighting for humans. With diffuse direct/indirect light combined with directional light from a spotlight mounted in the side, dynamic and natural-like lighting is created. Beta Opti louvre shutters provide high efficiency and optimal light comfort and this, combined with the anti-glare spotlight, makes it possible to manage UGR16 and meet the maximum average luminance requirement at workplaces with monitors 3000cd/m2 at 65-90 degrees. Can be a good luminaire in your next WELL project.;min. 80;C/E;1;0
NOTOR65 DYNAMIC BETAOPTI 1200 DI 840/930 WHT SINGLE_13681-533;65;4;4000;4580;Aluminium - Fagerhult - Beta Opti;1447;4580;4000;4000;20;190;131;White;Aluminium - Fagerhult - White;7316910589607;13681-533;36.5;36.5;Notor 65 Dynamic Beta Opti;"Single installation in wire suspension. For wire suspension installation, wire brackets are required for flexible c/c; ordered separately, see accessories.";Born out of research on Double Dynamic Lighting, Notor 65 Dynamic has a clear focus on lighting for humans. With diffuse direct/indirect light combined with directional light from a spotlight mounted in the side, dynamic and natural-like lighting is created. Beta Opti louvre shutters provide high efficiency and optimal light comfort and this, combined with the anti-glare spotlight, makes it possible to manage UGR16 and meet the maximum average luminance requirement at workplaces with monitors 3000cd/m2 at 65-90 degrees. Can be a good luminaire in your next WELL project.;min. 80;C/E;1;1
NOTOR65 DYNAMIC BETAOPTI 1200 DI 840/930 WHT SINGLE_13681-555;65;4;4000;4580;Aluminium - Fagerhult - Beta Opti;1392;4580;4000;4000;20;190;128;White;Aluminium - Fagerhult - White;7316910589621;13681-555;37;37;Notor 65 Dynamic Beta Opti;"Single installation in wire suspension. For wire suspension installation, wire brackets are required for flexible c/c; ordered separately, see accessories.";Born out of research on Double Dynamic Lighting, Notor 65 Dynamic has a clear focus on lighting for humans. With diffuse direct/indirect light combined with directional light from a spotlight mounted in the side, dynamic and natural-like lighting is created. Beta Opti louvre shutters provide high efficiency and optimal light comfort and this, combined with the anti-glare spotlight, makes it possible to manage UGR16 and meet the maximum average luminance requirement at workplaces with monitors 3000cd/m2 at 65-90 degrees. Can be a good luminaire in your next WELL project.;min. 80;C/E;1;2
NOTOR65 DYNAMIC BETAOPTI 1200 DI 840/930 BLACK SINGLE_13682-402;65;4;4000;4523;Aluminium - Fagerhult - Beta Opti;1357;4523;4000;4000;20;190;130;Black;Aluminium - Fagerhult - Black;7316910589645;13682-402;36;36;Notor 65 Dynamic Beta Opti;"Single installation in wire suspension. For wire suspension installation, wire brackets are required for flexible c/c; ordered separately, see accessories.";Born out of research on Double Dynamic Lighting, Notor 65 Dynamic has a clear focus on lighting for humans. With diffuse direct/indirect light combined with directional light from a spotlight mounted in the side, dynamic and natural-like lighting is created. Beta Opti louvre shutters provide high efficiency and optimal light comfort and this, combined with the anti-glare spotlight, makes it possible to manage UGR16 and meet the maximum average luminance requirement at workplaces with monitors 3000cd/m2 at 65-90 degrees. Can be a good luminaire in your next WELL project.;min. 80;C/E;1;0
NOTOR65 DYNAMIC BETAOPTI 1200 DI 840/930 BLACK SINGLE_13682-533;65;4;4000;4523;Aluminium - Fagerhult - Beta Opti;1447;4523;4000;4000;20;190;129;Black;Aluminium - Fagerhult - Black;7316910589669;13682-533;36.5;36.5;Notor 65 Dynamic Beta Opti;"Single installation in wire suspension. For wire suspension installation, wire brackets are required for flexible c/c; ordered separately, see accessories.";Born out of research on Double Dynamic Lighting, Notor 65 Dynamic has a clear focus on lighting for humans. With diffuse direct/indirect light combined with directional light from a spotlight mounted in the side, dynamic and natural-like lighting is created. Beta Opti louvre shutters provide high efficiency and optimal light comfort and this, combined with the anti-glare spotlight, makes it possible to manage UGR16 and meet the maximum average luminance requirement at workplaces with monitors 3000cd/m2 at 65-90 degrees. Can be a good luminaire in your next WELL project.;min. 80;C/E;1;1
NOTOR65 DYNAMIC BETAOPTI 1200 DI 840/930 BLACK SINGLE_13682-555;65;4;4000;4523;Aluminium - Fagerhult - Beta Opti;1392;4523;4000;4000;20;190;126;Black;Aluminium - Fagerhult - Black;7316910589683;13682-555;37;37;Notor 65 Dynamic Beta Opti;"Single installation in wire suspension. For wire suspension installation, wire brackets are required for flexible c/c; ordered separately, see accessories.";Born out of research on Double Dynamic Lighting, Notor 65 Dynamic has a clear focus on lighting for humans. With diffuse direct/indirect light combined with directional light from a spotlight mounted in the side, dynamic and natural-like lighting is created. Beta Opti louvre shutters provide high efficiency and optimal light comfort and this, combined with the anti-glare spotlight, makes it possible to manage UGR16 and meet the maximum average luminance requirement at workplaces with monitors 3000cd/m2 at 65-90 degrees. Can be a good luminaire in your next WELL project.;min. 80;C/E;1;2
NOTOR65 DYNAMIC BETAOPTI 1200 DI TW/930 WHT SINGLE_13685-533;65;4;3000;4385;Aluminium - Fagerhult - Beta Opti;1447;4385;3000;3000;20;190;98;White;Aluminium - Fagerhult - White;7316910589744;13685-533;46.5;46.5;Notor 65 Dynamic Beta Opti;"Single installation in wire suspension. For wire suspension installation, wire brackets are required for flexible c/c; ordered separately, see accessories.";Born out of research on Double Dynamic Lighting, Notor 65 Dynamic has a clear focus on lighting for humans. With diffuse direct/indirect light combined with directional light from a spotlight mounted in the side, dynamic and natural-like lighting is created. Beta Opti louvre shutters provide high efficiency and optimal light comfort and this, combined with the anti-glare spotlight, makes it possible to manage UGR16 and meet the maximum average luminance requirement at workplaces with monitors 3000cd/m2 at 65-90 degrees. Can be a good luminaire in your next WELL project.;min. 90;D/E;1;1
NOTOR65 DYNAMIC BETAOPTI 1200 DI TW/930 BLACK SINGLE_13686-533;65;4;3000;4358;Aluminium - Fagerhult - Beta Opti;1447;4358;3000;3000;20;190;98;Black;Aluminium - Fagerhult - Black;7316910589768;13686-533;46.5;46.5;Notor 65 Dynamic Beta Opti;"Single installation in wire suspension. For wire suspension installation, wire brackets are required for flexible c/c; ordered separately, see accessories.";Born out of research on Double Dynamic Lighting, Notor 65 Dynamic has a clear focus on lighting for humans. With diffuse direct/indirect light combined with directional light from a spotlight mounted in the side, dynamic and natural-like lighting is created. Beta Opti louvre shutters provide high efficiency and optimal light comfort and this, combined with the anti-glare spotlight, makes it possible to manage UGR16 and meet the maximum average luminance requirement at workplaces with monitors 3000cd/m2 at 65-90 degrees. Can be a good luminaire in your next WELL project.;min. 90;D/E;1;1
NOTOR65 DYNAMIC BETA 1200 DI TW/TW WHT SING DDL_13672-533;65;3.8;4000;4227;Aluminium - Fagerhult - Beta Opti;1447;4227;4000;4000;20;190;94;White;Aluminium - Fagerhult - White;7316910532443;13672-533;46.5;46.5;Notor 65 Dynamic Beta Opti;"Single installation in wire suspension. For wire suspension installation, wire brackets are required for flexible c/c; ordered separately, see accessories.";Born out of research on Double Dynamic Lighting, Notor 65 Dynamic has a clear focus on lighting for humans. With diffuse direct/indirect light combined with directional light from a spotlight mounted in the side, dynamic and natural-like lighting is created. Beta Opti louvre shutters provide high efficiency and optimal light comfort and this, combined with the anti-glare spotlight, makes it possible to manage UGR16 and meet the maximum average luminance requirement at workplaces with monitors 3000cd/m2 at 65-90 degrees. Can be a good luminaire in your next WELL project.;min. 90;D/E;1;1
NOTOR65 DYNAMIC BETA 1200 DI TW/TW BLACK SING DDL_13673-533;65;3.8;4000;4200;Aluminium - Fagerhult - Beta Opti;1447;4200;4000;4000;20;190;73;Black;Aluminium - Fagerhult - Black;7316910532450;13673-533;46.5;46.5;Notor 65 Dynamic Beta Opti;"Single installation in wire suspension. For wire suspension installation, wire brackets are required for flexible c/c; ordered separately, see accessories.";Born out of research on Double Dynamic Lighting, Notor 65 Dynamic has a clear focus on lighting for humans. With diffuse direct/indirect light combined with directional light from a spotlight mounted in the side, dynamic and natural-like lighting is created. Beta Opti louvre shutters provide high efficiency and optimal light comfort and this, combined with the anti-glare spotlight, makes it possible to manage UGR16 and meet the maximum average luminance requirement at workplaces with monitors 3000cd/m2 at 65-90 degrees. Can be a good luminaire in your next WELL project.;min. 90;D/E;1;1
