;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Type##OTHER##
NOTOR65 DYNAMIC DELTA 1200 DI TW/TW BLACK SINGLE_13676-402;65;4.5;4000;4169;Acrylic - Fagerhult - Delta Microprism;1346;4169;4000;4000;20;190;85;Black;Aluminium - Fagerhult - Black;7316910589409;13676-402;51;51;Notor 65 Dynamic Delta;"Single installation in wire suspension. For wire suspension installation, wire brackets are required for flexible c/c; ordered separately, see accessories.";Born out of research on Double Dynamic Lighting, Notor 65 Dynamic has a clear focus on lighting for humans. With diffuse direct/indirect light combined with directional light from a spotlight mounted in the side, dynamic and natural-like lighting is created. Delta louvre shutters provide high efficiency and optimal light comfort and this, combined with the anti-glare spotlight, makes it possible to manage UGR16 and meet the maximum average luminance requirement at workplaces with monitors 3000cd/m2 at 65-90 degrees. Can be a good luminaire in your next WELL project.;min. 90;D/E;1;0
NOTOR65 DYNAMIC DELTA 1200 DI TW/TW WHT SINGLE_13675-402;65;4.5;4000;4431;Acrylic - Fagerhult - Delta Microprism;1346;4431;4000;4000;20;190;91;White;Aluminium - Fagerhult - White;7316910589386;13675-402;51;51;Notor 65 Dynamic Delta;"Single installation in wire suspension. For wire suspension installation, wire brackets are required for flexible c/c; ordered separately, see accessories.";Born out of research on Double Dynamic Lighting, Notor 65 Dynamic has a clear focus on lighting for humans. With diffuse direct/indirect light combined with directional light from a spotlight mounted in the side, dynamic and natural-like lighting is created. Delta louvre shutters provide high efficiency and optimal light comfort and this, combined with the anti-glare spotlight, makes it possible to manage UGR16 and meet the maximum average luminance requirement at workplaces with monitors 3000cd/m2 at 65-90 degrees. Can be a good luminaire in your next WELL project.;min. 90;D/E;1;0
NOTOR65 DYNAMIC DELTA 1200 DI 840/930 WHT SINGLE_13679-402;65;4.5;4000;4781;Acrylic - Fagerhult - Delta Microprism;1346;4781;4000;4000;20;190;125;White;Aluminium - Fagerhult - White;7316910589461;13679-402;39.5;39.5;Notor 65 Dynamic Delta;"Single installation in wire suspension. For wire suspension installation, wire brackets are required for flexible c/c; ordered separately, see accessories.";Born out of research on Double Dynamic Lighting, Notor 65 Dynamic has a clear focus on lighting for humans. With diffuse direct/indirect light combined with directional light from a spotlight mounted in the side, dynamic and natural-like lighting is created. Delta louvre shutters provide high efficiency and optimal light comfort and this, combined with the anti-glare spotlight, makes it possible to manage UGR16 and meet the maximum average luminance requirement at workplaces with monitors 3000cd/m2 at 65-90 degrees. Can be a good luminaire in your next WELL project.;min. 80;C/E;1;0
NOTOR65 DYNAMIC DELTA 1200 DI 840/930 WHT SINGLE_13679-555;65;4.5;4000;4781;Acrylic - Fagerhult - Delta Microprism;1380;4781;4000;4000;20;190;125;White;Aluminium - Fagerhult - White;7316910589508;13679-555;40.5;40.5;Notor 65 Dynamic Delta;"Single installation in wire suspension. For wire suspension installation, wire brackets are required for flexible c/c; ordered separately, see accessories.";Born out of research on Double Dynamic Lighting, Notor 65 Dynamic has a clear focus on lighting for humans. With diffuse direct/indirect light combined with directional light from a spotlight mounted in the side, dynamic and natural-like lighting is created. Delta louvre shutters provide high efficiency and optimal light comfort and this, combined with the anti-glare spotlight, makes it possible to manage UGR16 and meet the maximum average luminance requirement at workplaces with monitors 3000cd/m2 at 65-90 degrees. Can be a good luminaire in your next WELL project.;min. 80;C/E;1;2
NOTOR65 DYNAMIC DELTA 1200 DI 840/930 BLACK SINGLE_13680-533;65;4.5;4000;4506;Acrylic - Fagerhult - Delta Microprism;1435;4506;4000;4000;20;190;117;Black;Aluminium - Fagerhult - Black;7316910589546;13680-533;39.5;39.5;Notor 65 Dynamic Delta;"Single installation in wire suspension. For wire suspension installation, wire brackets are required for flexible c/c; ordered separately, see accessories.";Born out of research on Double Dynamic Lighting, Notor 65 Dynamic has a clear focus on lighting for humans. With diffuse direct/indirect light combined with directional light from a spotlight mounted in the side, dynamic and natural-like lighting is created. Delta louvre shutters provide high efficiency and optimal light comfort and this, combined with the anti-glare spotlight, makes it possible to manage UGR16 and meet the maximum average luminance requirement at workplaces with monitors 3000cd/m2 at 65-90 degrees. Can be a good luminaire in your next WELL project.;min. 80;C/E;1;1
NOTOR65 DYNAMIC DELTA 1200 DI 840/930 WHT SINGLE_13679-533;65;4.5;4000;4781;Acrylic - Fagerhult - Delta Microprism;1435;4781;4000;4000;20;190;122;White;Aluminium - Fagerhult - White;7316910589485;13679-533;39.5;39.5;Notor 65 Dynamic Delta;"Single installation in wire suspension. For wire suspension installation, wire brackets are required for flexible c/c; ordered separately, see accessories.";Born out of research on Double Dynamic Lighting, Notor 65 Dynamic has a clear focus on lighting for humans. With diffuse direct/indirect light combined with directional light from a spotlight mounted in the side, dynamic and natural-like lighting is created. Delta louvre shutters provide high efficiency and optimal light comfort and this, combined with the anti-glare spotlight, makes it possible to manage UGR16 and meet the maximum average luminance requirement at workplaces with monitors 3000cd/m2 at 65-90 degrees. Can be a good luminaire in your next WELL project.;min. 80;C/E;1;1
NOTOR65 DYNAMIC DELTA 1200 DI 840/930 BLACK SINGLE_13680-402;65;4.5;4000;4506;Acrylic - Fagerhult - Delta Microprism;1346;4506;4000;4000;20;190;118;Black;Aluminium - Fagerhult - Black;7316910589522;13680-402;39.5;39.5;Notor 65 Dynamic Delta;"Single installation in wire suspension. For wire suspension installation, wire brackets are required for flexible c/c; ordered separately, see accessories.";Born out of research on Double Dynamic Lighting, Notor 65 Dynamic has a clear focus on lighting for humans. With diffuse direct/indirect light combined with directional light from a spotlight mounted in the side, dynamic and natural-like lighting is created. Delta louvre shutters provide high efficiency and optimal light comfort and this, combined with the anti-glare spotlight, makes it possible to manage UGR16 and meet the maximum average luminance requirement at workplaces with monitors 3000cd/m2 at 65-90 degrees. Can be a good luminaire in your next WELL project.;min. 80;C/E;1;0
NOTOR65 DYNAMIC DELTA 1200 DI 840/930 BLACK SINGLE_13680-555;65;4.5;4000;4506;Acrylic - Fagerhult - Delta Microprism;1380;4506;4000;4000;20;190;115;Black;Aluminium - Fagerhult - Black;7316910589560;13680-555;40.5;40.5;Notor 65 Dynamic Delta;"Single installation in wire suspension. For wire suspension installation, wire brackets are required for flexible c/c; ordered separately, see accessories.";Born out of research on Double Dynamic Lighting, Notor 65 Dynamic has a clear focus on lighting for humans. With diffuse direct/indirect light combined with directional light from a spotlight mounted in the side, dynamic and natural-like lighting is created. Delta louvre shutters provide high efficiency and optimal light comfort and this, combined with the anti-glare spotlight, makes it possible to manage UGR16 and meet the maximum average luminance requirement at workplaces with monitors 3000cd/m2 at 65-90 degrees. Can be a good luminaire in your next WELL project.;min. 80;C/E;1;2
NOTOR65 DYNAMIC DELTA 1200 DI TW/930 WHT SINGLE_13683-533;65;4.5;3000;4589;Acrylic - Fagerhult - Delta Microprism;1435;4589;3000;3000;20;190;94;White;Aluminium - Fagerhult - White;7316910589706;13683-533;50.5;50.5;Notor 65 Dynamic Delta;"Single installation in wire suspension. For wire suspension installation, wire brackets are required for flexible c/c; ordered separately, see accessories.";Born out of research on Double Dynamic Lighting, Notor 65 Dynamic has a clear focus on lighting for humans. With diffuse direct/indirect light combined with directional light from a spotlight mounted in the side, dynamic and natural-like lighting is created. Delta louvre shutters provide high efficiency and optimal light comfort and this, combined with the anti-glare spotlight, makes it possible to manage UGR16 and meet the maximum average luminance requirement at workplaces with monitors 3000cd/m2 at 65-90 degrees. Can be a good luminaire in your next WELL project.;min. 90;D/E;1;1
NOTOR65 DYNAMIC DELTA 1200 DI TW/930 BLACK SINGLE_13684-533;65;4.5;3000;4327;Acrylic - Fagerhult - Delta Microprism;1435;4327;3000;3000;20;190;88;Black;Aluminium - Fagerhult - Black;7316910589720;13684-533;50.5;50.5;Notor 65 Dynamic Delta;"Single installation in wire suspension. For wire suspension installation, wire brackets are required for flexible c/c; ordered separately, see accessories.";Born out of research on Double Dynamic Lighting, Notor 65 Dynamic has a clear focus on lighting for humans. With diffuse direct/indirect light combined with directional light from a spotlight mounted in the side, dynamic and natural-like lighting is created. Delta louvre shutters provide high efficiency and optimal light comfort and this, combined with the anti-glare spotlight, makes it possible to manage UGR16 and meet the maximum average luminance requirement at workplaces with monitors 3000cd/m2 at 65-90 degrees. Can be a good luminaire in your next WELL project.;min. 90;D/E;1;1
NOTOR65 DYNAMIC DELTA 1200 DI TW/TW WHT SING DDL_13670-533;65;4.3;4000;4431;Acrylic - Fagerhult - Delta Microprism;1435;4431;4000;4000;20;190;90;White;Aluminium - Fagerhult - White;7316910532429;13670-533;52.5;52.5;Notor 65 Dynamic Delta;"Single installation in wire suspension. For wire suspension installation, wire brackets are required for flexible c/c; ordered separately, see accessories.";Born out of research on Double Dynamic Lighting, Notor 65 Dynamic has a clear focus on lighting for humans. With diffuse direct/indirect light combined with directional light from a spotlight mounted in the side, dynamic and natural-like lighting is created. Delta louvre shutters provide high efficiency and optimal light comfort and this, combined with the anti-glare spotlight, makes it possible to manage UGR16 and meet the maximum average luminance requirement at workplaces with monitors 3000cd/m2 at 65-90 degrees. Can be a good luminaire in your next WELL project.;min. 90;D/E;1;1
NOTOR65 DYNAMIC DELTA 1200 DI TW/TW BLACK SING DDL_13671-533;65;4.3;4000;4169;Acrylic - Fagerhult - Delta Microprism;1435;4169;4000;4000;20;190;83;Black;Aluminium - Fagerhult - Black;7316910532436;13671-533;52.5;52.5;Notor 65 Dynamic Delta;"Single installation in wire suspension. For wire suspension installation, wire brackets are required for flexible c/c; ordered separately, see accessories.";Born out of research on Double Dynamic Lighting, Notor 65 Dynamic has a clear focus on lighting for humans. With diffuse direct/indirect light combined with directional light from a spotlight mounted in the side, dynamic and natural-like lighting is created. Delta louvre shutters provide high efficiency and optimal light comfort and this, combined with the anti-glare spotlight, makes it possible to manage UGR16 and meet the maximum average luminance requirement at workplaces with monitors 3000cd/m2 at 65-90 degrees. Can be a good luminaire in your next WELL project.;min. 90;D/E;1;1
