;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Tilt Angle##ANGLE##DEGREES;Temperature Color##OTHER##;Size##OTHER##;Shape##OTHER##;ServiceLifeDuration##OTHER##;ProductInformation##OTHER##;Photometric Web File##OTHER##;Optic##OTHER##;ModelReference##OTHER##;Material##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Length##LENGTH##MILLIMETERS;Description##OTHER##;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP_Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;DiffuserMaterial##OTHER##;Control Gear##OTHER##;Color##OTHER##;Body##OTHER##;BarCode##OTHER##;BIMObjectName##OTHER##;ArticleNumber##OTHER##;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;ColorRenderingIndex##Other##
CLARICO UP 600X600 3K 3KLM_23793;596;5.0;90;3000;L 596 mm + W 596 mm + H 86 mm;Square;LED 50,000 hrs;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;23793.IES;<By Category>;Clarico Up;aluminium;2719;Fagerhult_Opal;Ceiling;Recessed ;596;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;2719;3000;3000;40;86;113;<By Category>;Standard;White;Fagerhult_White_aluminium;7320043437704;Clarico Up;23793;24;830
CLARICO UP 600X600 3K 3KLM_23793-3;596;5.0;90;3000;L 596 mm + W 596 mm + H 86 mm;Square;LED 50,000 hrs;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;23793-3.IES;<By Category>;Clarico Up;aluminium;2719;Fagerhult_Opal;Ceiling;Recessed ;596;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;2719;3000;3000;40;86;113;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7320043437711;Clarico Up;23793-3;24;830
CLARICO UP 600X600 3K 3KLM_23793-402;596;5.0;90;3000;L 596 mm + W 596 mm + H 86 mm;Square;LED 50,000 hrs;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;23793-402.IES;<By Category>;Clarico Up;aluminium;2719;Fagerhult_Opal;Ceiling;Recessed ;596;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;2719;3000;3000;40;86;113;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320043437940;Clarico Up;23793-402;24;830
CLARICO HB UP 600X600 3K 3KLM_23794;596;5.0;90;3000;L 596 mm + W 596 mm + H 86 mm;Square;LED 50,000 hrs;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;23794.IES;<By Category>;Clarico Up;aluminium;2719;Fagerhult_Opal;Ceiling;Recessed ;596;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;2719;3000;3000;40;86;113;<By Category>;Standard;White;Fagerhult_White_aluminium;7320043437728;Clarico Up;23794;24;830
CLARICO HB UP 600X600 3K 3KLM_23794-3;596;5.0;90;3000;L 596 mm + W 596 mm + H 86 mm;Square;LED 50,000 hrs;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;23794-3.IES;<By Category>;Clarico Up;aluminium;2719;Fagerhult_Opal;Ceiling;Recessed ;596;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;2719;3000;3000;40;86;113;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7320043437957;Clarico Up;23794-3;24;830
CLARICO HB UP 600X600 3K 3KLM_23794-402;596;5.0;90;3000;L 596 mm + W 596 mm + H 86 mm;Square;LED 50,000 hrs;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;23794-402.IES;<By Category>;Clarico Up;aluminium;2719;Fagerhult_Opal;Ceiling;Recessed ;596;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;2719;3000;3000;40;86;113;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320043437964;Clarico Up;23794-402;24;830
CLARICO UP 600X600 4K 3KLM_23795;596;5.0;90;4000;L 596 mm + W 596 mm + H 86 mm;Square;LED 50,000 hrs;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;23795.IES;<By Category>;Clarico Up;aluminium;2862;Fagerhult_Opal;Ceiling;Recessed ;596;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;2862;4000;4000;40;86;119;<By Category>;Standard;White;Fagerhult_White_aluminium;7320043437735;Clarico Up;23795;24;840
CLARICO UP 600X600 4K 3KLM_23795-3;596;5.0;90;4000;L 596 mm + W 596 mm + H 86 mm;Square;LED 50,000 hrs;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;23795-3.IES;<By Category>;Clarico Up;aluminium;2862;Fagerhult_Opal;Ceiling;Recessed ;596;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;2862;4000;4000;40;86;119;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7320043437971;Clarico Up;23795-3;24;840
CLARICO UP 600X600 4K 3KLM_23795-402;596;5.0;90;4000;L 596 mm + W 596 mm + H 86 mm;Square;LED 50,000 hrs;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;23795-402.IES;<By Category>;Clarico Up;aluminium;2862;Fagerhult_Opal;Ceiling;Recessed ;596;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;2862;4000;4000;40;86;119;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320043437988;Clarico Up;23795-402;24;840
CLARICO HB UP 600X600 4K 3KLM_23796;596;5.0;90;4000;L 596 mm + W 596 mm + H 86 mm;Square;LED 50,000 hrs;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;23796.IES;<By Category>;Clarico Up;aluminium;2862;Fagerhult_Opal;Ceiling;Recessed ;596;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;2862;4000;4000;40;86;119;<By Category>;Standard;White;Fagerhult_White_aluminium;7320043437742;Clarico Up;23796;24;840
CLARICO HB UP 600X600 4K 3KLM_23796-3;596;5.0;90;4000;L 596 mm + W 596 mm + H 86 mm;Square;LED 50,000 hrs;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;23796-3.IES;<By Category>;Clarico Up;aluminium;2862;Fagerhult_Opal;Ceiling;Recessed ;596;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;2862;4000;4000;40;86;119;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7320043437995;Clarico Up;23796-3;24;840
CLARICO HB UP 600X600 4K 3KLM_23796-402;596;5.0;90;4000;L 596 mm + W 596 mm + H 86 mm;Square;LED 50,000 hrs;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;23796-402.IES;<By Category>;Clarico Up;aluminium;2862;Fagerhult_Opal;Ceiling;Recessed ;596;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;2862;4000;4000;40;86;119;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320043438008;Clarico Up;23796-402;24;840
CLARICO UP 600X600 3K 4,5KLM_23813;596;5.0;90;3000;L 596 mm + W 596 mm + H 86 mm;Square;LED 50,000 hrs;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;23813.IES;<By Category>;Clarico Up;aluminium;4169;Fagerhult_Opal;Ceiling;Recessed ;596;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;4169;3000;3000;40;86;116;<By Category>;Standard;White;Fagerhult_White_aluminium;7320043437780;Clarico Up;23813;36;830
CLARICO UP 600X600 3K 4,5KLM_23813-3;596;5.0;90;3000;L 596 mm + W 596 mm + H 86 mm;Square;LED 50,000 hrs;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;23813-3.IES;<By Category>;Clarico Up;aluminium;4169;Fagerhult_Opal;Ceiling;Recessed ;596;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;4169;3000;3000;40;86;116;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7320043438091;Clarico Up;23813-3;36;830
CLARICO UP 600X600 3K 4,5KLM_23813-402;596;5.0;90;3000;L 596 mm + W 596 mm + H 86 mm;Square;LED 50,000 hrs;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;23813-402.IES;<By Category>;Clarico Up;aluminium;4169;Fagerhult_Opal;Ceiling;Recessed ;596;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;4169;3000;3000;40;86;116;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320043438107;Clarico Up;23813-402;36;830
CLARICO HB UP 600X600 3K 4,5KLM_23814;596;5.0;90;3000;L 596 mm + W 596 mm + H 86 mm;Square;LED 50,000 hrs;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;23814.IES;<By Category>;Clarico Up;aluminium;4169;Fagerhult_Opal;Ceiling;Recessed ;596;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;4169;3000;3000;40;86;116;<By Category>;Standard;White;Fagerhult_White_aluminium;7320043437797;Clarico Up;23814;36;830
CLARICO HB UP 600X600 3K 4,5KLM_23814-3;596;5.0;90;3000;L 596 mm + W 596 mm + H 86 mm;Square;LED 50,000 hrs;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;23814-3.IES;<By Category>;Clarico Up;aluminium;4169;Fagerhult_Opal;Ceiling;Recessed ;596;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;4169;3000;3000;40;86;116;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7320043438114;Clarico Up;23814-3;36;830
CLARICO HB UP 600X600 3K 4,5KLM_23814-402;596;5.0;90;3000;L 596 mm + W 596 mm + H 86 mm;Square;LED 50,000 hrs;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;23814-402.IES;<By Category>;Clarico Up;aluminium;4169;Fagerhult_Opal;Ceiling;Recessed ;596;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;4169;3000;3000;40;86;116;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320043438121;Clarico Up;23814-402;36;830
CLARICO UP 600X600 4K 4,5KLM_23815;596;5.0;90;4000;L 596 mm + W 596 mm + H 86 mm;Square;LED 50,000 hrs;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;23815.IES;<By Category>;Clarico Up;aluminium;4388;Fagerhult_Opal;Ceiling;Recessed ;596;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;4388;4000;4000;40;86;122;<By Category>;Standard;White;Fagerhult_White_aluminium;7320043437803;Clarico Up;23815;36;840
CLARICO UP 600X600 4K 4,5KLM_23815-3;596;5.0;90;4000;L 596 mm + W 596 mm + H 86 mm;Square;LED 50,000 hrs;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;23815-3.IES;<By Category>;Clarico Up;aluminium;4388;Fagerhult_Opal;Ceiling;Recessed ;596;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;4388;4000;4000;40;86;122;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7320043438138;Clarico Up;23815-3;36;840
CLARICO UP 600X600 4K 4,5KLM_23815-402;596;5.0;90;4000;L 596 mm + W 596 mm + H 86 mm;Square;LED 50,000 hrs;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;23815-402.IES;<By Category>;Clarico Up;aluminium;4388;Fagerhult_Opal;Ceiling;Recessed ;596;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;4388;4000;4000;40;86;122;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320043438145;Clarico Up;23815-402;36;840
CLARICO HB UP 600X600 4K 4,5KLM_23816;596;5.0;90;4000;L 596 mm + W 596 mm + H 86 mm;Square;LED 50,000 hrs;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;23816.IES;<By Category>;Clarico Up;aluminium;4388;Fagerhult_Opal;Ceiling;Recessed ;596;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;4388;4000;4000;40;86;122;<By Category>;Standard;White;Fagerhult_White_aluminium;7320043437810;Clarico Up;23816;36;840
CLARICO HB UP 600X600 4K 4,5KLM_23816-3;596;5.0;90;4000;L 596 mm + W 596 mm + H 86 mm;Square;LED 50,000 hrs;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;23816-3.IES;<By Category>;Clarico Up;aluminium;4388;Fagerhult_Opal;Ceiling;Recessed ;596;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;4388;4000;4000;40;86;122;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7320043438152;Clarico Up;23816-3;36;840
CLARICO HB UP 600X600 4K 4,5KLM_23816-402;596;5.0;90;4000;L 596 mm + W 596 mm + H 86 mm;Square;LED 50,000 hrs;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;23816-402.IES;<By Category>;Clarico Up;aluminium;4388;Fagerhult_Opal;Ceiling;Recessed ;596;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;4388;4000;4000;40;86;122;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320043438169;Clarico Up;23816-402;36;840
CLARICO UP 600X600 3K 4KLM_23875;596;5.0;90;3000;L 596 mm + W 596 mm + H 86 mm;Square;LED 50,000 hrs;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;23875.IES;<By Category>;Clarico Up;aluminium;3625;Fagerhult_Opal;Ceiling;Recessed ;596;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;3625;3000;3000;40;86;117;<By Category>;Standard;White;Fagerhult_White_aluminium;7320043437865;Clarico Up;23875;31;830
CLARICO UP 600X600 3K 4KLM_23875-3;596;5.0;90;3000;L 596 mm + W 596 mm + H 86 mm;Square;LED 50,000 hrs;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;23875-3.IES;<By Category>;Clarico Up;aluminium;3625;Fagerhult_Opal;Ceiling;Recessed ;596;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;3625;3000;3000;40;86;117;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7320043438251;Clarico Up;23875-3;31;830
CLARICO UP 600X600 3K 4KLM_23875-402;596;5.0;90;3000;L 596 mm + W 596 mm + H 86 mm;Square;LED 50,000 hrs;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;23875-402.IES;<By Category>;Clarico Up;aluminium;3625;Fagerhult_Opal;Ceiling;Recessed ;596;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;3625;3000;3000;40;86;117;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320043438268;Clarico Up;23875-402;31;830
CLARICO HB UP 600X600 3K 4KLM_23876;596;5.0;90;3000;L 596 mm + W 596 mm + H 86 mm;Square;LED 50,000 hrs;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;23876.IES;<By Category>;Clarico Up;aluminium;3625;Fagerhult_Opal;Ceiling;Recessed ;596;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;3625;3000;3000;40;86;117;<By Category>;Standard;White;Fagerhult_White_aluminium;7320043437872;Clarico Up;23876;31;830
CLARICO HB UP 600X600 3K 4KLM_23876-3;596;5.0;90;3000;L 596 mm + W 596 mm + H 86 mm;Square;LED 50,000 hrs;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;23876-3.IES;<By Category>;Clarico Up;aluminium;3625;Fagerhult_Opal;Ceiling;Recessed ;596;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;3625;3000;3000;40;86;117;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7320043438275;Clarico Up;23876-3;31;830
CLARICO HB UP 600X600 3K 4KLM_23876-402;596;5.0;90;3000;L 596 mm + W 596 mm + H 86 mm;Square;LED 50,000 hrs;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;23876-402.IES;<By Category>;Clarico Up;aluminium;3625;Fagerhult_Opal;Ceiling;Recessed ;596;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;3625;3000;3000;40;86;117;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320043438282;Clarico Up;23876-402;31;830
CLARICO UP 600X600 4K 4KLM_23877;596;5.0;90;4000;L 596 mm + W 596 mm + H 86 mm;Square;LED 50,000 hrs;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;23877.IES;<By Category>;Clarico Up;aluminium;3816;Fagerhult_Opal;Ceiling;Recessed ;596;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;3816;4000;4000;40;86;123;<By Category>;Standard;White;Fagerhult_White_aluminium;7320043437889;Clarico Up;23877;31;840
CLARICO UP 600X600 4K 4KLM_23877-3;596;5.0;90;4000;L 596 mm + W 596 mm + H 86 mm;Square;LED 50,000 hrs;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;23877-3.IES;<By Category>;Clarico Up;aluminium;3816;Fagerhult_Opal;Ceiling;Recessed ;596;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;3816;4000;4000;40;86;123;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7320043438299;Clarico Up;23877-3;31;840
CLARICO UP 600X600 4K 4KLM_23877-402;596;5.0;90;4000;L 596 mm + W 596 mm + H 86 mm;Square;LED 50,000 hrs;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;23877-402.IES;<By Category>;Clarico Up;aluminium;3816;Fagerhult_Opal;Ceiling;Recessed ;596;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;3816;4000;4000;40;86;123;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320043438305;Clarico Up;23877-402;31;840
CLARICO HB UP 600X600 4K 4KLM_23878;596;5.0;90;4000;L 596 mm + W 596 mm + H 86 mm;Square;LED 50,000 hrs;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;23878.IES;<By Category>;Clarico Up;aluminium;3816;Fagerhult_Opal;Ceiling;Recessed ;596;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;3816;4000;4000;40;86;123;<By Category>;Standard;White;Fagerhult_White_aluminium;7320043437896;Clarico Up;23878;31;840
CLARICO HB UP 600X600 4K 4KLM_23878-3;596;5.0;90;4000;L 596 mm + W 596 mm + H 86 mm;Square;LED 50,000 hrs;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;23878-3.IES;<By Category>;Clarico Up;aluminium;3816;Fagerhult_Opal;Ceiling;Recessed ;596;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;3816;4000;4000;40;86;123;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7320043438312;Clarico Up;23878-3;31;840
CLARICO HB UP 600X600 4K 4KLM_23878-402;596;5.0;90;4000;L 596 mm + W 596 mm + H 86 mm;Square;LED 50,000 hrs;Luminaire body in natural anodised, extruded aluminium or white enamelled (RAL 9016). With continuous installation an unbroken line of light is achieved, even via a L-coupling.;23878-402.IES;<By Category>;Clarico Up;aluminium;3816;Fagerhult_Opal;Ceiling;Recessed ;596;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;3816;4000;4000;40;86;123;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320043438329;Clarico Up;23878-402;31;840
