;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Tilt Angle##ANGLE##DEGREES;Temperature Color##OTHER##;Size##OTHER##;Shape##OTHER##;ServiceLifeDuration##OTHER##;ProductInformation##OTHER##;Photometric Web File##OTHER##;Optic##OTHER##;ModelReference##OTHER##;Material##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Length##LENGTH##MILLIMETERS;Description##OTHER##;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP_Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;DiffuserMaterial##OTHER##;Control Gear##OTHER##;Color##OTHER##;Body##OTHER##;BarCode##OTHER##;BIMObjectName##OTHER##;ArticleNumber##OTHER##;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;ColorRenderingIndex##Other##
CLARICO DOWN 600X600 3K 3KLM_23797;596;5.0;90;3000;L 600 mm + W 600 mm + H 86 mm;Square;LED 50,000 hrs;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;23797.IES;<By Category>;Clarico Down;aluminium;2808;Fagerhult_Opal;Ceiling;Recessed ;596;Luminaire body in white enamelled sheet steel (RAL 9016). ;2808;3000;3000;40;86;117;<By Category>;Standard;White;Fagerhult_White_aluminium;7,32004E+12;Clarico Down;23797;24;830
CLARICO DOWN 600X600 3K 3KLM_23797-3;596;5.0;90;3000;L 600 mm + W 600 mm + H 86 mm;Square;LED 50,000 hrs;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;23797-3.IES;<By Category>;Clarico Down;aluminium;2808;Fagerhult_Opal;Ceiling;Recessed ;596;Luminaire body in white enamelled sheet steel (RAL 9016). ;2808;3000;3000;40;86;117;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7,32004E+12;Clarico Down;23797-3;24;830
CLARICO DOWN 600X600 3K 3KLM_23797-402;596;5.0;90;3000;L 600 mm + W 600 mm + H 86 mm;Square;LED 50,000 hrs;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;23797-402.IES;<By Category>;Clarico Down;aluminium;2808;Fagerhult_Opal;Ceiling;Recessed ;596;Luminaire body in white enamelled sheet steel (RAL 9016). ;2808;3000;3000;40;86;117;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7,32004E+12;Clarico Down;23797-402;24;830
CLARICO HB DOWN 600X600 3K 3KLM_23798;596;5.0;90;3000;L 600 mm + W 600 mm + H 86 mm;Square;LED 50,000 hrs;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;23798.IES;<By Category>;Clarico Down;aluminium;2808;Fagerhult_Opal;Ceiling;Recessed ;596;Luminaire body in white enamelled sheet steel (RAL 9016). ;2808;3000;3000;40;86;117;<By Category>;Standard;White;Fagerhult_White_aluminium;7,32004E+12;Clarico Down;23798;24;830
CLARICO HB DOWN 600X600 3K 3KLM_23798-3;596;5.0;90;3000;L 600 mm + W 600 mm + H 86 mm;Square;LED 50,000 hrs;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;23798-3.IES;<By Category>;Clarico Down;aluminium;2808;Fagerhult_Opal;Ceiling;Recessed ;596;Luminaire body in white enamelled sheet steel (RAL 9016). ;2808;3000;3000;40;86;117;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7,32004E+12;Clarico Down;23798-3;24;830
CLARICO HB DOWN 600X600 3K 3KLM_23798-402;596;5.0;90;3000;L 600 mm + W 600 mm + H 86 mm;Square;LED 50,000 hrs;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;23798-402.IES;<By Category>;Clarico Down;aluminium;2808;Fagerhult_Opal;Ceiling;Recessed ;596;Luminaire body in white enamelled sheet steel (RAL 9016). ;2808;3000;3000;40;86;117;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7,32004E+12;Clarico Down;23798-402;24;830
CLARICO DOWN 600X600 4K 3KLM_23799;596;5.0;90;4000;L 600 mm + W 600 mm + H 86 mm;Square;LED 50,000 hrs;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;23799.IES;<By Category>;Clarico Down;aluminium;2956;Fagerhult_Opal;Ceiling;Recessed ;596;Luminaire body in white enamelled sheet steel (RAL 9016). ;2956;4000;4000;40;86;123;<By Category>;Standard;White;Fagerhult_White_aluminium;7,32004E+12;Clarico Down;23799;24;840
CLARICO DOWN 600X600 4K 3KLM_23799-3;596;5.0;90;4000;L 600 mm + W 600 mm + H 86 mm;Square;LED 50,000 hrs;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;23799-3.IES;<By Category>;Clarico Down;aluminium;2956;Fagerhult_Opal;Ceiling;Recessed ;596;Luminaire body in white enamelled sheet steel (RAL 9016). ;2956;4000;4000;40;86;123;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7,32004E+12;Clarico Down;23799-3;24;840
CLARICO DOWN 600X600 4K 3KLM_23799-402;596;5.0;90;4000;L 600 mm + W 600 mm + H 86 mm;Square;LED 50,000 hrs;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;23799-402.IES;<By Category>;Clarico Down;aluminium;2956;Fagerhult_Opal;Ceiling;Recessed ;596;Luminaire body in white enamelled sheet steel (RAL 9016). ;2956;4000;4000;40;86;123;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7,32004E+12;Clarico Down;23799-402;24;840
CLARICO HB DOWN 600X600 4K 3KLM_23800;596;5.0;90;4000;L 600 mm + W 600 mm + H 86 mm;Square;LED 50,000 hrs;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;23800.IES;<By Category>;Clarico Down;aluminium;2956;Fagerhult_Opal;Ceiling;Recessed ;596;Luminaire body in white enamelled sheet steel (RAL 9016). ;2956;4000;4000;40;86;123;<By Category>;Standard;White;Fagerhult_White_aluminium;7,32004E+12;Clarico Down;23800;24;840
CLARICO HB DOWN 600X600 4K 3KLM_23800-3;596;5.0;90;4000;L 600 mm + W 600 mm + H 86 mm;Square;LED 50,000 hrs;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;23800-3.IES;<By Category>;Clarico Down;aluminium;2956;Fagerhult_Opal;Ceiling;Recessed ;596;Luminaire body in white enamelled sheet steel (RAL 9016). ;2956;4000;4000;40;86;123;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7,32004E+12;Clarico Down;23800-3;24;840
CLARICO HB DOWN 600X600 4K 3KLM_23800-402;596;5.0;90;4000;L 600 mm + W 600 mm + H 86 mm;Square;LED 50,000 hrs;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;23800-402.IES;<By Category>;Clarico Down;aluminium;2956;Fagerhult_Opal;Ceiling;Recessed ;596;Luminaire body in white enamelled sheet steel (RAL 9016). ;2956;4000;4000;40;86;123;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7,32004E+12;Clarico Down;23800-402;24;840
CLARICO DOWN 600X600 3K 4,5KLM_23817;596;5.0;90;3000;L 600 mm + W 600 mm + H 86 mm;Square;LED 50,000 hrs;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;23817.IES;<By Category>;Clarico Down;aluminium;4306;Fagerhult_Opal;Ceiling;Recessed ;596;Luminaire body in white enamelled sheet steel (RAL 9016). ;4306;3000;3000;40;86;120;<By Category>;Standard;White;Fagerhult_White_aluminium;7,32004E+12;Clarico Down;23817;36;830
CLARICO DOWN 600X600 3K 4,5KLM_23817-3;596;5.0;90;3000;L 600 mm + W 600 mm + H 86 mm;Square;LED 50,000 hrs;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;23817-3.IES;<By Category>;Clarico Down;aluminium;4306;Fagerhult_Opal;Ceiling;Recessed ;596;Luminaire body in white enamelled sheet steel (RAL 9016). ;4306;3000;3000;40;86;120;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7,32004E+12;Clarico Down;23817-3;36;830
CLARICO DOWN 600X600 3K 4,5KLM_23817-402;596;5.0;90;3000;L 600 mm + W 600 mm + H 86 mm;Square;LED 50,000 hrs;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;23817-402.IES;<By Category>;Clarico Down;aluminium;4306;Fagerhult_Opal;Ceiling;Recessed ;596;Luminaire body in white enamelled sheet steel (RAL 9016). ;4306;3000;3000;40;86;120;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7,32004E+12;Clarico Down;23817-402;36;830
CLARICO HB DOWN 600X600 3K 4,5KLM_23818;596;5.0;90;3000;L 600 mm + W 600 mm + H 86 mm;Square;LED 50,000 hrs;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;23818.IES;<By Category>;Clarico Down;aluminium;4306;Fagerhult_Opal;Ceiling;Recessed ;596;Luminaire body in white enamelled sheet steel (RAL 9016). ;4306;3000;3000;40;86;120;<By Category>;Standard;White;Fagerhult_White_aluminium;7,32004E+12;Clarico Down;23818;36;830
CLARICO HB DOWN 600X600 3K 4,5KLM_23818-3;596;5.0;90;3000;L 600 mm + W 600 mm + H 86 mm;Square;LED 50,000 hrs;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;23818-3.IES;<By Category>;Clarico Down;aluminium;4306;Fagerhult_Opal;Ceiling;Recessed ;596;Luminaire body in white enamelled sheet steel (RAL 9016). ;4306;3000;3000;40;86;120;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7,32004E+12;Clarico Down;23818-3;36;830
CLARICO HB DOWN 600X600 3K 4,5KLM_23818-402;596;5.0;90;3000;L 600 mm + W 600 mm + H 86 mm;Square;LED 50,000 hrs;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;23818-402.IES;<By Category>;Clarico Down;aluminium;4306;Fagerhult_Opal;Ceiling;Recessed ;596;Luminaire body in white enamelled sheet steel (RAL 9016). ;4306;3000;3000;40;86;120;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7,32004E+12;Clarico Down;23818-402;36;830
CLARICO DOWN 600X600 4K 4,5KLM_23819;596;5.0;90;4000;L 600 mm + W 600 mm + H 86 mm;Square;LED 50,000 hrs;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;23819.IES;<By Category>;Clarico Down;aluminium;4533;Fagerhult_Opal;Ceiling;Recessed ;596;Luminaire body in white enamelled sheet steel (RAL 9016). ;4533;4000;4000;40;86;126;<By Category>;Standard;White;Fagerhult_White_aluminium;7,32004E+12;Clarico Down;23819;36;840
CLARICO DOWN 600X600 4K 4,5KLM_23819-3;596;5.0;90;4000;L 600 mm + W 600 mm + H 86 mm;Square;LED 50,000 hrs;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;23819-3.IES;<By Category>;Clarico Down;aluminium;4533;Fagerhult_Opal;Ceiling;Recessed ;596;Luminaire body in white enamelled sheet steel (RAL 9016). ;4533;4000;4000;40;86;126;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7,32004E+12;Clarico Down;23819-3;36;840
CLARICO DOWN 600X600 4K 4,5KLM_23819-402;596;5.0;90;4000;L 600 mm + W 600 mm + H 86 mm;Square;LED 50,000 hrs;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;23819-402.IES;<By Category>;Clarico Down;aluminium;4533;Fagerhult_Opal;Ceiling;Recessed ;596;Luminaire body in white enamelled sheet steel (RAL 9016). ;4533;4000;4000;40;86;126;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7,32004E+12;Clarico Down;23819-402;36;840
CLARICO HB DOWN 600X600 4K 4,5KLM_23820;596;5.0;90;4000;L 600 mm + W 600 mm + H 86 mm;Square;LED 50,000 hrs;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;23820.IES;<By Category>;Clarico Down;aluminium;4533;Fagerhult_Opal;Ceiling;Recessed ;596;Luminaire body in white enamelled sheet steel (RAL 9016). ;4533;4000;4000;40;86;126;<By Category>;Standard;White;Fagerhult_White_aluminium;7,32004E+12;Clarico Down;23820;36;840
CLARICO HB DOWN 600X600 4K 4,5KLM_23820-3;596;5.0;90;4000;L 600 mm + W 600 mm + H 86 mm;Square;LED 50,000 hrs;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;23820-3.IES;<By Category>;Clarico Down;aluminium;4533;Fagerhult_Opal;Ceiling;Recessed ;596;Luminaire body in white enamelled sheet steel (RAL 9016). ;4533;4000;4000;40;86;126;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7,32004E+12;Clarico Down;23820-3;36;840
CLARICO HB DOWN 600X600 4K 4,5KLM_23820-402;596;5.0;90;4000;L 600 mm + W 600 mm + H 86 mm;Square;LED 50,000 hrs;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;23820-402.IES;<By Category>;Clarico Down;aluminium;4533;Fagerhult_Opal;Ceiling;Recessed ;596;Luminaire body in white enamelled sheet steel (RAL 9016). ;4533;4000;4000;40;86;126;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7,32004E+12;Clarico Down;23820-402;36;840
CLARICO DOWN 600X600 3K 4KLM_23879;596;5.0;90;3000;L 600 mm + W 600 mm + H 86 mm;Square;LED 50,000 hrs;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;23879.IES;<By Category>;Clarico Down;aluminium;3744;Fagerhult_Opal;Ceiling;Recessed ;596;Luminaire body in white enamelled sheet steel (RAL 9016). ;3744;3000;3000;40;86;121;<By Category>;Standard;White;Fagerhult_White_aluminium;7,32004E+12;Clarico Down;23879;31;830
CLARICO DOWN 600X600 3K 4KLM_23879-3;596;5.0;90;3000;L 600 mm + W 600 mm + H 86 mm;Square;LED 50,000 hrs;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;23879-3.IES;<By Category>;Clarico Down;aluminium;3744;Fagerhult_Opal;Ceiling;Recessed ;596;Luminaire body in white enamelled sheet steel (RAL 9016). ;3744;3000;3000;40;86;121;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7,32004E+12;Clarico Down;23879-3;31;830
CLARICO DOWN 600X600 3K 4KLM_23879-402;596;5.0;90;3000;L 600 mm + W 600 mm + H 86 mm;Square;LED 50,000 hrs;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;23879-402.IES;<By Category>;Clarico Down;aluminium;3744;Fagerhult_Opal;Ceiling;Recessed ;596;Luminaire body in white enamelled sheet steel (RAL 9016). ;3744;3000;3000;40;86;121;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7,32004E+12;Clarico Down;23879-402;31;830
CLARICO HB DOWN 600X600 3K 4KLM_23880;596;5.0;90;3000;L 600 mm + W 600 mm + H 86 mm;Square;LED 50,000 hrs;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;23880.IES;<By Category>;Clarico Down;aluminium;3744;Fagerhult_Opal;Ceiling;Recessed ;596;Luminaire body in white enamelled sheet steel (RAL 9016). ;3744;3000;3000;40;86;121;<By Category>;Standard;White;Fagerhult_White_aluminium;7,32004E+12;Clarico Down;23880;31;830
CLARICO HB DOWN 600X600 3K 4KLM_23880-3;596;5.0;90;3000;L 600 mm + W 600 mm + H 86 mm;Square;LED 50,000 hrs;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;23880-3.IES;<By Category>;Clarico Down;aluminium;3744;Fagerhult_Opal;Ceiling;Recessed ;596;Luminaire body in white enamelled sheet steel (RAL 9016). ;3744;3000;3000;40;86;121;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7,32004E+12;Clarico Down;23880-3;31;830
CLARICO HB DOWN 600X600 3K 4KLM_23880-402;596;5.0;90;3000;L 600 mm + W 600 mm + H 86 mm;Square;LED 50,000 hrs;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;23880-402.IES;<By Category>;Clarico Down;aluminium;3744;Fagerhult_Opal;Ceiling;Recessed ;596;Luminaire body in white enamelled sheet steel (RAL 9016). ;3744;3000;3000;40;86;121;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7,32004E+12;Clarico Down;23880-402;31;830
CLARICO DOWN 600X600 4K 4KLM_23881;596;5.0;90;4000;L 600 mm + W 600 mm + H 86 mm;Square;LED 50,000 hrs;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;23881.IES;<By Category>;Clarico Down;aluminium;3941;Fagerhult_Opal;Ceiling;Recessed ;596;Luminaire body in white enamelled sheet steel (RAL 9016). ;3941;4000;4000;40;86;127;<By Category>;Standard;White;Fagerhult_White_aluminium;7,32004E+12;Clarico Down;23881;31;840
CLARICO DOWN 600X600 4K 4KLM_23881-3;596;5.0;90;4000;L 600 mm + W 600 mm + H 86 mm;Square;LED 50,000 hrs;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;23881-3.IES;<By Category>;Clarico Down;aluminium;3941;Fagerhult_Opal;Ceiling;Recessed ;596;Luminaire body in white enamelled sheet steel (RAL 9016). ;3941;4000;4000;40;86;127;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7,32004E+12;Clarico Down;23881-3;31;840
CLARICO DOWN 600X600 4K 4KLM_23881-402;596;5.0;90;4000;L 600 mm + W 600 mm + H 86 mm;Square;LED 50,000 hrs;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;23881-402.IES;<By Category>;Clarico Down;aluminium;3941;Fagerhult_Opal;Ceiling;Recessed ;596;Luminaire body in white enamelled sheet steel (RAL 9016). ;3941;4000;4000;40;86;127;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7,32004E+12;Clarico Down;23881-402;31;840
CLARICO HB DOWN 600X600 4K 4KLM_23882;596;5.0;90;4000;L 600 mm + W 600 mm + H 86 mm;Square;LED 50,000 hrs;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;23882.IES;<By Category>;Clarico Down;aluminium;3941;Fagerhult_Opal;Ceiling;Recessed ;596;Luminaire body in white enamelled sheet steel (RAL 9016). ;3941;4000;4000;40;86;127;<By Category>;Standard;White;Fagerhult_White_aluminium;7,32004E+12;Clarico Down;23882;31;840
CLARICO HB DOWN 600X600 4K 4KLM_23882-3;596;5.0;90;4000;L 600 mm + W 600 mm + H 86 mm;Square;LED 50,000 hrs;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;23882-3.IES;<By Category>;Clarico Down;aluminium;3941;Fagerhult_Opal;Ceiling;Recessed ;596;Luminaire body in white enamelled sheet steel (RAL 9016). ;3941;4000;4000;40;86;127;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7,32004E+12;Clarico Down;23882-3;31;840
CLARICO HB DOWN 600X600 4K 4KLM_23882-402;596;5.0;90;4000;L 600 mm + W 600 mm + H 86 mm;Square;LED 50,000 hrs;A recessed luminaire for most types of suspended ceilings. A combination of microprism and opal surfaces in various levels produces direct light on the floor and ambient light on walls and ceilings. ;23882-402.IES;<By Category>;Clarico Down;aluminium;3941;Fagerhult_Opal;Ceiling;Recessed ;596;Luminaire body in white enamelled sheet steel (RAL 9016). ;3941;4000;4000;40;86;127;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7,32004E+12;Clarico Down;23882-402;31;840
