;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Installation##OTHER##;Miscellaneous##OTHER##
NOTOR36 REC D 600 DALI HL BETA 840_16087-20035;56;1.1;4000;1284;Aluminium - Fagerhult - Beta Opti Nano;589;1284;4000;4000;20;68;116;White;Aluminium - Fagerhult - White;7320048773777;16087-20035;11;11;Notor 36 recessed Beta Opti Nano;Recessed installation in suspended ceilings. Unventilated or ventilated ceilings. For installation in suspended ceilings with visible T-bars, VTB (24 mm) or one-piece suspended ceilings.;A recessed luminaire for installation in suspended ceilings with Beta Opti Nano louvre. Single or series installation.;min. 80;C;1;2;4
NOTOR36 REC D 1200 DALI HL BETA 840_16087-20036;56;1.9;4000;2684;Aluminium - Fagerhult - Beta Opti Nano;1189;2684;4000;4000;20;51;131;White;Aluminium - Fagerhult - White;7320048773807;16087-20036;21;21;Notor 36 recessed Beta Opti Nano;Recessed installation in suspended ceilings. Unventilated or ventilated ceilings. For installation in suspended ceilings with visible T-bars, VTB (24 mm) or one-piece suspended ceilings.;A recessed luminaire for installation in suspended ceilings with Beta Opti Nano louvre. Single or series installation.;min. 80;C;1;2;3
NOTOR36 REC D 2400 DALI HL BETA 840_16087-20037;56;3.4;4000;5602;Aluminium - Fagerhult - Beta Opti Nano;2389;5602;4000;4000;20;51;135;White;Aluminium - Fagerhult - White;7320048773838;16087-20037;41;41;Notor 36 recessed Beta Opti Nano;Recessed installation in suspended ceilings. Unventilated or ventilated ceilings. For installation in suspended ceilings with visible T-bars, VTB (24 mm) or one-piece suspended ceilings.;A recessed luminaire for installation in suspended ceilings with Beta Opti Nano louvre. Single or series installation.;min. 80;C;1;2;2
