;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Installation##OTHER##;Miscellaneous##OTHER##
NOTOR36 REC D 600 DALI HL OPAL 840_16087-20023;56;1;4000;1287;Acrylic - Fagerhult - Opal;589;1287;4000;4000;20;68;107;White;Aluminium - Fagerhult - White;7320048773418;16087-20023;12.5;12.5;Notor 36 recessed Opal;Recessed installation in suspended ceilings. Unventilated or ventilated ceilings. For installation in suspended ceilings with visible T-bars, VTB (24 mm) or one-piece suspended ceilings.;A recessed luminaire for installation in suspended ceilings. Single or series installation. Spot module for continuous installation.;min. 80;C;1;2;1
NOTOR36 REC D 1200 DALI HL OPAL 840_16087-20024;56;1.8;4000;2691;Acrylic - Fagerhult - Opal;1189;2691;4000;4000;20;51;120;White;Aluminium - Fagerhult - White;7320048773449;16087-20024;23.5;23.5;Notor 36 recessed Opal;Recessed installation in suspended ceilings. Unventilated or ventilated ceilings. For installation in suspended ceilings with visible T-bars, VTB (24 mm) or one-piece suspended ceilings.;A recessed luminaire for installation in suspended ceilings. Single or series installation. Spot module for continuous installation.;min. 80;C;1;2;1
NOTOR36 REC D 2400 DALI HL OPAL 840_16087-20025;56;3.3;4000;5499;Acrylic - Fagerhult - Opal;2389;5499;4000;4000;20;51;124;White;Aluminium - Fagerhult - White;7320048773470;16087-20025;47;47;Notor 36 recessed Opal;Recessed installation in suspended ceilings. Unventilated or ventilated ceilings. For installation in suspended ceilings with visible T-bars, VTB (24 mm) or one-piece suspended ceilings.;A recessed luminaire for installation in suspended ceilings. Single or series installation. Spot module for continuous installation.;min. 80;C;1;2;1
