;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Model##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Diameter##LENGTH##MILLIMETERS;Description##OTHER##;Color Rendering Index##Other##;DECOR FRAME##OTHER##
STELO FIXED D75 930 WIDE BEAM WHITE/WHITE_69005;0.3;3000;Stelo 75 Fixed;783;Aluminium - Fagerhult - White;783;3000;3000;20;100;80;White/White;Aluminium - Fagerhult - White;7320048026217;69005;10;86;A small recessed downlight with two light distributions and one colour temperature, with an IP54 rating. Provides an elegant general lighting solution for corridors or communal areas.;min. 90;1
STELO FIXED D75 930 WIDE BEAM WHITE/WHITE_69005-402;0.3;3000;Stelo 75 Fixed;783;Aluminium - Fagerhult - White;783;3000;3000;20;100;78;White/White;Aluminium - Fagerhult - White;7320048026231;69005-402;10;86;A small recessed downlight with two light distributions and one colour temperature, with an IP54 rating. Provides an elegant general lighting solution for corridors or communal areas.;min. 90;1
STELO FIXED D75 930 WIDE BEAM BLACK/WHITE_69006;0.3;3000;Stelo 75 Fixed;755;Aluminium - Fagerhult - Black;755;3000;3000;20;100;77;Black/White;Aluminium - Fagerhult - White;7320048026279;69006;10;86;A small recessed downlight with two light distributions and one colour temperature, with an IP54 rating. Provides an elegant general lighting solution for corridors or communal areas.;min. 90;1
STELO FIXED D75 930 WIDE BEAM BLACK/WHITE_69006-402;0.3;3000;Stelo 75 Fixed;755;Aluminium - Fagerhult - Black;755;3000;3000;20;100;75;Black/White;Aluminium - Fagerhult - White;7320048026293;69006-402;10;86;A small recessed downlight with two light distributions and one colour temperature, with an IP54 rating. Provides an elegant general lighting solution for corridors or communal areas.;min. 90;1
STELO FIXED D75 SQ 930 WIDE BEAM WHITE/WHITE_69007;0.3;3000;Stelo 75 Fixed;783;Aluminium - Fagerhult - White;783;3000;3000;20;100;80;White/White;Aluminium - Fagerhult - White;7320048026330;69007;10;86;A small recessed downlight with two light distributions and one colour temperature, with an IP54 rating. Provides an elegant general lighting solution for corridors or communal areas.;min. 90;2
STELO FIXED D75 SQ 930 WIDE BEAM WHITE/WHITE_69007-402;0.3;3000;Stelo 75 Fixed;783;Aluminium - Fagerhult - White;783;3000;3000;20;100;78;White/White;Aluminium - Fagerhult - White;7320048026354;69007-402;10;86;A small recessed downlight with two light distributions and one colour temperature, with an IP54 rating. Provides an elegant general lighting solution for corridors or communal areas.;min. 90;2
STELO FIXED D75 SQ 930 WIDE BEAM BLACK/WHITE_69008;0.3;3000;Stelo 75 Fixed;755;Aluminium - Fagerhult - Black;755;3000;3000;20;100;77;Black/White;Aluminium - Fagerhult - White;7320048026392;69008;10;86;A small recessed downlight with two light distributions and one colour temperature, with an IP54 rating. Provides an elegant general lighting solution for corridors or communal areas.;min. 90;2
STELO FIXED D75 SQ 930 WIDE BEAM BLACK/WHITE_69008-402;0.3;3000;Stelo 75 Fixed;755;Aluminium - Fagerhult - Black;755;3000;3000;20;100;75;Black/White;Aluminium - Fagerhult - White;7320048026415;69008-402;10;86;A small recessed downlight with two light distributions and one colour temperature, with an IP54 rating. Provides an elegant general lighting solution for corridors or communal areas.;min. 90;2
STELO FIXED D75 IP54 930 WIDE BEAM WHITE/WHITE_69009;0.3;3000;Stelo 75 Fixed;740;Aluminium - Fagerhult - White;740;3000;3000;20;100;76;White/White;Aluminium - Fagerhult - White;7320048026453;69009;10;86;A small recessed downlight with two light distributions and one colour temperature, with an IP54 rating. Provides an elegant general lighting solution for corridors or communal areas.;min. 90;1
STELO FIXED D75 IP54 930 WIDE BEAM WHITE/WHITE_69009-402;0.3;3000;Stelo 75 Fixed;740;Aluminium - Fagerhult - White;740;3000;3000;20;100;73;White/White;Aluminium - Fagerhult - White;7320048026477;69009-402;10;86;A small recessed downlight with two light distributions and one colour temperature, with an IP54 rating. Provides an elegant general lighting solution for corridors or communal areas.;min. 90;1
STELO FIXED D75 IP54 930 WIDE BEAM BLACK/WHITE_69010;0.3;3000;Stelo 75 Fixed;712;Aluminium - Fagerhult - Black;712;3000;3000;20;100;73;Black/White;Aluminium - Fagerhult - White;7320048026514;69010;10;86;A small recessed downlight with two light distributions and one colour temperature, with an IP54 rating. Provides an elegant general lighting solution for corridors or communal areas.;min. 90;1
STELO FIXED D75 IP54 930 WIDE BEAM BLACK/WHITE_69010-402;0.3;3000;Stelo 75 Fixed;712;Aluminium - Fagerhult - Black;712;3000;3000;20;100;70;Black/White;Aluminium - Fagerhult - White;7320048026538;69010-402;10;86;A small recessed downlight with two light distributions and one colour temperature, with an IP54 rating. Provides an elegant general lighting solution for corridors or communal areas.;min. 90;1
STELO FIXED D75 IP54 SQ 930 WIDE BEAM WHITE/WHITE_69011;0.3;3000;Stelo 75 Fixed;740;Aluminium - Fagerhult - White;740;3000;3000;20;100;76;White/White;Aluminium - Fagerhult - White;7320048026576;69011;10;86;A small recessed downlight with two light distributions and one colour temperature, with an IP54 rating. Provides an elegant general lighting solution for corridors or communal areas.;min. 90;2
STELO FIXED D75 IP54 SQ 930 WIDE BEAM WHITE/WHITE_69011-402;0.3;3000;Stelo 75 Fixed;740;Aluminium - Fagerhult - White;740;3000;3000;20;100;73;White/White;Aluminium - Fagerhult - White;7320048026590;69011-402;10;86;A small recessed downlight with two light distributions and one colour temperature, with an IP54 rating. Provides an elegant general lighting solution for corridors or communal areas.;min. 90;2
STELO FIXED D75 IP54 SQ 930 WIDE BEAM BLACK/WHITE_69012;0.3;3000;Stelo 75 Fixed;712;Aluminium - Fagerhult - Black;712;3000;3000;20;100;73;Black/White;Aluminium - Fagerhult - White;7320048026637;69012;10;86;A small recessed downlight with two light distributions and one colour temperature, with an IP54 rating. Provides an elegant general lighting solution for corridors or communal areas.;min. 90;2
STELO FIXED D75 IP54 SQ 930 WIDE BEAM BLACK/WHITE_69012-402;0.3;3000;Stelo 75 Fixed;712;Aluminium - Fagerhult - Black;712;3000;3000;20;100;70;Black/White;Aluminium - Fagerhult - White;7320048026651;69012-402;10;86;A small recessed downlight with two light distributions and one colour temperature, with an IP54 rating. Provides an elegant general lighting solution for corridors or communal areas.;min. 90;2
