;Diameter##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Size##OTHER##;Shape##OTHER##;ProductInformation##OTHER##;ModelReference##OTHER##;Material##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Description##OTHER##;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP_Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;CreatedOn##OTHER##;Control Gear##OTHER##;Color##OTHER##;Body##OTHER##;BarCode##OTHER##;BIMObjectName##OTHER##;ArticleNumber##OTHER##;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;ColorRenderingIndex##Other##
Robust reading luminaire LED G2_56948;163;0,5;2700;D 163 mm + H 73 mm;Half sphere;A robust wall-mounted reading/bed luminaire with high safety for exposed environments.;Robust reading luminaire LED G2;aluminium;252;Wall;Surface;Enamelled body in steel. Casing of 1 mm white enamelled (RAL9016) aluminium. Pushbutton for off/on and dimming, safe against damage.;252;2700;2700;20;73;63;Created 03/09/2018;Standard;White;Fagerhult_White_aluminium;7320046727543;Robust reading luminaire LED G2;56948;4;min. 80
Robust reading luminaire LED G2_56948-530;163;0,5;2700;D 163 mm + H 73 mm;Half sphere;A robust wall-mounted reading/bed luminaire with high safety for exposed environments.;Robust reading luminaire LED G2;aluminium;347;Wall;Surface;Enamelled body in steel. Casing of 1 mm white enamelled (RAL9016) aluminium. Pushbutton for off/on and dimming, safe against damage.;347;2700;2700;20;73;69;Created 03/09/2018;Dimming via pushbutton;White;Fagerhult_White_aluminium;7320047287947;Robust reading luminaire LED G2;56948-530;5;min. 80
