;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##
SEKTOR LED LL 3000K_17426-402;95;2.7;3000;1957;1187;1957;3000;3000;20;76;134;White;Aluminium - Fagerhult - White;7320046223472;17426-402;15.5;15.5;Sektor;For ceiling or wall mounting. Normally installed at the junction between the ceiling and wall.;A corridor luminaire installed where the ceiling and wall meet. The light is distributed on the ceiling and wall for a varied light experience and distinct sense of space.;min. 80;C;1
SEKTOR LED HL 3000K_17427-402;95;2.7;3000;3344;1187;3344;3000;3000;20;76;131;White;Aluminium - Fagerhult - White;7320046223496;17427-402;27;27;Sektor;For ceiling or wall mounting. Normally installed at the junction between the ceiling and wall.;A corridor luminaire installed where the ceiling and wall meet. The light is distributed on the ceiling and wall for a varied light experience and distinct sense of space.;min. 80;C;1
SEKTOR LED LL 4000K_17428-402;95;2.7;4000;2030;1187;2030;4000;4000;20;76;139;White;Aluminium - Fagerhult - White;7320046223519;17428-402;15.5;15.5;Sektor;For ceiling or wall mounting. Normally installed at the junction between the ceiling and wall.;A corridor luminaire installed where the ceiling and wall meet. The light is distributed on the ceiling and wall for a varied light experience and distinct sense of space.;min. 80;B;1
SEKTOR LED HL 4000K_17429-402;95;2.7;4000;3469;1187;3469;4000;4000;20;76;136;White;Aluminium - Fagerhult - White;7320046223540;17429-402;27;27;Sektor;For ceiling or wall mounting. Normally installed at the junction between the ceiling and wall.;A corridor luminaire installed where the ceiling and wall meet. The light is distributed on the ceiling and wall for a varied light experience and distinct sense of space.;min. 80;B;1
