,Type Comments##OTHER##,MaterialBody##OTHER##,MaterialLouvre##OTHER##,MaterialAccentBody##OTHER##,MaterialReflector##OTHER##,Weight_Kg##OTHER##,URL##OTHER##,Total Light Loss Factor##OTHER##,SuffixCode##OTHER##,Photometric Web File##OTHER##,Model##OTHER##,Manufacturer##OTHER##,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,LightSource##OTHER##,Light Loss Factor##OTHER##,Lamp##OTHER##,Keynote##OTHER##,Initial Intensity##OTHER##,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Initial Color##OTHER##,FagerhultPartNumber##OTHER##,Emit from Rectangle Width##LENGTH##MILLIMETERS,Emit from Rectangle Length##LENGTH##MILLIMETERS,COBieBarCode##OTHER##,Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,Description##OTHER##,Assembly Code##OTHER##,LOR##OTHER##,Wattage##ELECTRICAL_WATTAGE##WATTS,TotalLength##LENGTH##MILLIMETERS,TotalWidth##LENGTH##MILLIMETERS,Height##LENGTH##MILLIMETERS,NumberOfLamps##OTHER##,Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT
RECESSO BANDRASTER LED 150X1720 3K 1C BETA OPTI_25681,RECESSO BANDRASTER LED 150X1720 3K 1C BETA OPTI-,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.6,http://www.fagerhult.com,1,Standard,25681.IES,Recesso Beta Opti,Fagerhult,3873.0,LED,1,33,V59,3873.0,3000,3000,25681,100,1465,7320046217495,33,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,33,1720,147,88,1,117.3636364
RECESSO BANDRASTER LED 150X1720 3K 1C BETA OPTI_25681-111,RECESSO BANDRASTER LED 150X1720 3K 1C BETA OPTI-BODY W WIELAND CONNECTOR GST18I3 MALE.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.6,http://www.fagerhult.com,1,Standard,25681.IES,Recesso Beta Opti,Fagerhult,3873.0,LED,1,33,V59,3873.0,3000,3000,25681-111,100,1465,7320046217518,33,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,33,1720,147,88,1,117.3636364
RECESSO BANDRASTER LED 150X1720 3K 1C BETA OPTI_25681-3,"RECESSO BANDRASTER LED 150X1720 3K 1C BETA OPTI-BODY W CONNECTION CABLE L=2,5M FREE CABLE W PLUG.",Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.6,http://www.fagerhult.com,1,Standard,25681.IES,Recesso Beta Opti,Fagerhult,3873.0,LED,1,33,V59,3873.0,3000,3000,25681-3,100,1465,7320046217532,33,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,33,1720,147,88,1,117.3636364
RECESSO BANDRASTER LED 150X1720 3K 1C BETA OPTI_25681-402,RECESSO BANDRASTER LED 150X1720 3K 1C BETA OPTI-LED dim DALI/Phase-pulse control.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.6,http://www.fagerhult.com,1,DALI/Phase-pulse control,25681.IES,Recesso Beta Opti,Fagerhult,3873.0,LED,1,33,V59,3873.0,3000,3000,25681-402,100,1465,7320046217556,33,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,33,1720,147,88,1,117.3636364
RECESSO BANDRASTER LED 150X1720 4K 1C BETA OPTI_25682,RECESSO BANDRASTER LED 150X1720 4K 1C BETA OPTI-,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.6,http://www.fagerhult.com,1,Standard,25682.IES,Recesso Beta Opti,Fagerhult,3950.0,LED,1,33,V59,3950.0,4000,4000,25682,100,1465,7320046217570,33,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,33,1720,147,88,1,119.6969697
RECESSO BANDRASTER LED 150X1720 4K 1C BETA OPTI_25682-111,RECESSO BANDRASTER LED 150X1720 4K 1C BETA OPTI-BODY W WIELAND CONNECTOR GST18I3 MALE.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.6,http://www.fagerhult.com,1,Standard,25682.IES,Recesso Beta Opti,Fagerhult,3950.0,LED,1,33,V59,3950.0,4000,4000,25682-111,100,1465,7320046217594,33,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,33,1720,147,88,1,119.6969697
RECESSO BANDRASTER LED 150X1720 4K 1C BETA OPTI_25682-3,"RECESSO BANDRASTER LED 150X1720 4K 1C BETA OPTI-BODY W CONNECTION CABLE L=2,5M FREE CABLE W PLUG.",Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.6,http://www.fagerhult.com,1,Standard,25682.IES,Recesso Beta Opti,Fagerhult,3950.0,LED,1,33,V59,3950.0,4000,4000,25682-3,100,1465,7320046217617,33,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,33,1720,147,88,1,119.6969697
RECESSO BANDRASTER LED 150X1720 4K 1C BETA OPTI_25682-402,RECESSO BANDRASTER LED 150X1720 4K 1C BETA OPTI-LED dim DALI/Phase-pulse control.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.6,http://www.fagerhult.com,1,DALI/Phase-pulse control,25682.IES,Recesso Beta Opti,Fagerhult,3950.0,LED,1,33,V59,3950.0,4000,4000,25682-402,100,1465,7320046217631,33,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,33,1720,147,88,1,119.6969697
RECESSO BANDRASTER LED 200X1720 3K 1C BETA OPTI_25683,RECESSO BANDRASTER LED 200X1720 3K 1C BETA OPTI-,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,4.0,http://www.fagerhult.com,1,Standard,25683.IES,Recesso Beta Opti,Fagerhult,3873.0,LED,1,33,V59,3873.0,3000,3000,25683,100,1465,7320046217655,33,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,33,1720,197,88,1,117.3636364
RECESSO BANDRASTER LED 200X1720 3K 1C BETA OPTI_25683-111,RECESSO BANDRASTER LED 200X1720 3K 1C BETA OPTI-BODY W WIELAND CONNECTOR GST18I3 MALE.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,4.0,http://www.fagerhult.com,1,Standard,25683.IES,Recesso Beta Opti,Fagerhult,3873.0,LED,1,33,V59,3873.0,3000,3000,25683-111,100,1465,7320046217679,33,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,33,1720,197,88,1,117.3636364
RECESSO BANDRASTER LED 200X1720 3K 1C BETA OPTI_25683-3,"RECESSO BANDRASTER LED 200X1720 3K 1C BETA OPTI-BODY W CONNECTION CABLE L=2,5M FREE CABLE W PLUG.",Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,4.0,http://www.fagerhult.com,1,Standard,25683.IES,Recesso Beta Opti,Fagerhult,3873.0,LED,1,33,V59,3873.0,3000,3000,25683-3,100,1465,7320046217693,33,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,33,1720,197,88,1,117.3636364
RECESSO BANDRASTER LED 200X1720 3K 1C BETA OPTI_25683-402,RECESSO BANDRASTER LED 200X1720 3K 1C BETA OPTI-LED dim DALI/Phase-pulse control.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,4.0,http://www.fagerhult.com,1,DALI/Phase-pulse control,25683.IES,Recesso Beta Opti,Fagerhult,3873.0,LED,1,33,V59,3873.0,3000,3000,25683-402,100,1465,7320046217716,33,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,33,1720,197,88,1,117.3636364
RECESSO BANDRASTER LED 200X1720 4K 1C BETA OPTI_25684,RECESSO BANDRASTER LED 200X1720 4K 1C BETA OPTI-,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,4.0,http://www.fagerhult.com,1,Standard,25684.IES,Recesso Beta Opti,Fagerhult,3950.0,LED,1,33,V59,3950.0,4000,4000,25684,100,1465,7320046217730,33,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,33,1720,197,88,1,119.6969697
RECESSO BANDRASTER LED 200X1720 4K 1C BETA OPTI_25684-111,RECESSO BANDRASTER LED 200X1720 4K 1C BETA OPTI-BODY W WIELAND CONNECTOR GST18I3 MALE.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,4.0,http://www.fagerhult.com,1,Standard,25684.IES,Recesso Beta Opti,Fagerhult,3950.0,LED,1,33,V59,3950.0,4000,4000,25684-111,100,1465,7320046217754,33,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,33,1720,197,88,1,119.6969697
RECESSO BANDRASTER LED 200X1720 4K 1C BETA OPTI_25684-3,"RECESSO BANDRASTER LED 200X1720 4K 1C BETA OPTI-BODY W CONNECTION CABLE L=2,5M FREE CABLE W PLUG.",Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,4.0,http://www.fagerhult.com,1,Standard,25684.IES,Recesso Beta Opti,Fagerhult,3950.0,LED,1,33,V59,3950.0,4000,4000,25684-3,100,1465,7320046217778,33,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,33,1720,197,88,1,119.6969697
RECESSO BANDRASTER LED 200X1720 4K 1C BETA OPTI_25684-402,RECESSO BANDRASTER LED 200X1720 4K 1C BETA OPTI-LED dim DALI/Phase-pulse control.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,4.0,http://www.fagerhult.com,1,DALI/Phase-pulse control,25684.IES,Recesso Beta Opti,Fagerhult,3950.0,LED,1,33,V59,3950.0,4000,4000,25684-402,100,1465,7320046217792,33,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,33,1720,197,88,1,119.6969697
RECESSO BANDRASTER LED 300X1720 3K 1C BETA OPTI_25685,RECESSO BANDRASTER LED 300X1720 3K 1C BETA OPTI-,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,4.6,http://www.fagerhult.com,1,Standard,25685.IES,Recesso Beta Opti,Fagerhult,3873.0,LED,1,33,V59,3873.0,3000,3000,25685,100,1465,7320046217815,33,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,33,1720,297,88,1,117.3636364
RECESSO BANDRASTER LED 300X1720 3K 1C BETA OPTI_25685-111,RECESSO BANDRASTER LED 300X1720 3K 1C BETA OPTI-BODY W WIELAND CONNECTOR GST18I3 MALE.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,4.6,http://www.fagerhult.com,1,Standard,25685.IES,Recesso Beta Opti,Fagerhult,3873.0,LED,1,33,V59,3873.0,3000,3000,25685-111,100,1465,7320046217839,33,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,33,1720,297,88,1,117.3636364
RECESSO BANDRASTER LED 300X1720 3K 1C BETA OPTI_25685-3,"RECESSO BANDRASTER LED 300X1720 3K 1C BETA OPTI-BODY W CONNECTION CABLE L=2,5M FREE CABLE W PLUG.",Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,4.6,http://www.fagerhult.com,1,Standard,25685.IES,Recesso Beta Opti,Fagerhult,3873.0,LED,1,33,V59,3873.0,3000,3000,25685-3,100,1465,7320046217853,33,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,33,1720,297,88,1,117.3636364
RECESSO BANDRASTER LED 300X1720 3K 1C BETA OPTI_25685-402,RECESSO BANDRASTER LED 300X1720 3K 1C BETA OPTI-LED dim DALI/Phase-pulse control.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,4.6,http://www.fagerhult.com,1,DALI/Phase-pulse control,25685.IES,Recesso Beta Opti,Fagerhult,3873.0,LED,1,33,V59,3873.0,3000,3000,25685-402,100,1465,7320046217877,33,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,33,1720,297,88,1,117.3636364
RECESSO BANDRASTER LED 300X1720 4K 1C BETA OPTI_25686,RECESSO BANDRASTER LED 300X1720 4K 1C BETA OPTI-,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,4.6,http://www.fagerhult.com,1,Standard,25686.IES,Recesso Beta Opti,Fagerhult,3950.0,LED,1,33,V59,3950.0,4000,4000,25686,100,1465,7320046217891,33,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,33,1720,297,88,1,119.6969697
RECESSO BANDRASTER LED 300X1720 4K 1C BETA OPTI_25686-111,RECESSO BANDRASTER LED 300X1720 4K 1C BETA OPTI-BODY W WIELAND CONNECTOR GST18I3 MALE.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,4.6,http://www.fagerhult.com,1,Standard,25686.IES,Recesso Beta Opti,Fagerhult,3950.0,LED,1,33,V59,3950.0,4000,4000,25686-111,100,1465,7320046217914,33,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,33,1720,297,88,1,119.6969697
RECESSO BANDRASTER LED 300X1720 4K 1C BETA OPTI_25686-3,"RECESSO BANDRASTER LED 300X1720 4K 1C BETA OPTI-BODY W CONNECTION CABLE L=2,5M FREE CABLE W PLUG.",Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,4.6,http://www.fagerhult.com,1,Standard,25686.IES,Recesso Beta Opti,Fagerhult,3950.0,LED,1,33,V59,3950.0,4000,4000,25686-3,100,1465,7320046217938,33,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,33,1720,297,88,1,119.6969697
RECESSO BANDRASTER LED 300X1720 4K 1C BETA OPTI_25686-402,RECESSO BANDRASTER LED 300X1720 4K 1C BETA OPTI-LED dim DALI/Phase-pulse control.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,4.6,http://www.fagerhult.com,1,DALI/Phase-pulse control,25686.IES,Recesso Beta Opti,Fagerhult,3950.0,LED,1,33,V59,3950.0,4000,4000,25686-402,100,1465,7320046217952,33,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,33,1720,297,88,1,119.6969697
RECESSO 150X1200 3K 1C BETA OPTI_25712,RECESSO 150X1200 3K 1C BETA OPTI-,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,2.6,http://www.fagerhult.com,1,Standard,25712.IES,Recesso Beta Opti,Fagerhult,3850.0,LED,1,35,V59,3850.0,3000,3000,25712,100,1158,7320046216931,35,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,35,1197,147,88,1,110
RECESSO 150X1200 3K 1C BETA OPTI_25712-111,RECESSO 150X1200 3K 1C BETA OPTI-BODY W WIELAND CONNECTOR GST18I3 MALE.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,2.6,http://www.fagerhult.com,1,Standard,25712.IES,Recesso Beta Opti,Fagerhult,3850.0,LED,1,35,V59,3850.0,3000,3000,25712-111,100,1158,7320046216955,35,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,35,1197,147,88,1,110
RECESSO 150X1200 3K 1C BETA OPTI_25712-3,"RECESSO 150X1200 3K 1C BETA OPTI-BODY W CONNECTION CABLE L=2,5M FREE CABLE W PLUG.",Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,2.6,http://www.fagerhult.com,1,Standard,25712.IES,Recesso Beta Opti,Fagerhult,3850.0,LED,1,35,V59,3850.0,3000,3000,25712-3,100,1158,7320046216979,35,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,35,1197,147,88,1,110
RECESSO 150X1200 3K 1C BETA OPTI_25712-340,RECESSO 150X1200 3K 1C BETA OPTI-Body w Winsta connector 3-pole.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,2.6,http://www.fagerhult.com,1,Standard - WAGO Winsta,25712.IES,Recesso Beta Opti,Fagerhult,3850.0,LED,1,35,V59,3850.0,3000,3000,25712-340,100,1158,7320046216993,35,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,35,1197,147,88,1,110
RECESSO 150X1200 3K 1C BETA OPTI_25712-402,RECESSO 150X1200 3K 1C BETA OPTI-LED dim DALI/Phase-pulse control.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,2.6,http://www.fagerhult.com,1,DALI/Phase-pulse control,25712.IES,Recesso Beta Opti,Fagerhult,3850.0,LED,1,35,V59,3850.0,3000,3000,25712-402,100,1158,7320046217013,35,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,35,1197,147,88,1,110
RECESSO 150X1200 3K 1C BETA OPTI_25712-454,RECESSO 150X1200 3K 1C BETA OPTI-LED body w DALI driver and Winsta connector 5-pole. Blue male for dim.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,2.6,http://www.fagerhult.com,1,DALI - WAGO Winsta,25712.IES,Recesso Beta Opti,Fagerhult,3850.0,LED,1,35,V59,3850.0,3000,3000,25712-454,100,1158,7320046217037,35,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,35,1197,147,88,1,110
RECESSO 150X1200 3K 1C BETA OPTI_25712-456,RECESSO 150X1200 3K 1C BETA OPTI-LED body w DALI driver and Wieland connector 5-pole. Blue male for dim.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,2.6,http://www.fagerhult.com,1,DALI - Wieland,25712.IES,Recesso Beta Opti,Fagerhult,3850.0,LED,1,35,V59,3850.0,3000,3000,25712-456,100,1158,7320046217051,35,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,35,1197,147,88,1,110
RECESSO 150X1200 4K 1C BETA OPTI_25713,RECESSO 150X1200 4K 1C BETA OPTI-,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,2.6,http://www.fagerhult.com,1,Standard,25713.IES,Recesso Beta Opti,Fagerhult,3940.0,LED,1,35,V59,3940.0,4000,4000,25713,100,1158,7320046217075,35,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,35,1197,147,88,1,112.5714286
RECESSO 150X1200 4K 1C BETA OPTI_25713-111,RECESSO 150X1200 4K 1C BETA OPTI-BODY W WIELAND CONNECTOR GST18I3 MALE.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,2.6,http://www.fagerhult.com,1,Standard,25713.IES,Recesso Beta Opti,Fagerhult,3940.0,LED,1,35,V59,3940.0,4000,4000,25713-111,100,1158,7320046217099,35,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,35,1197,147,88,1,112.5714286
RECESSO 150X1200 4K 1C BETA OPTI_25713-3,"RECESSO 150X1200 4K 1C BETA OPTI-BODY W CONNECTION CABLE L=2,5M FREE CABLE W PLUG.",Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,2.6,http://www.fagerhult.com,1,Standard,25713.IES,Recesso Beta Opti,Fagerhult,3940.0,LED,1,35,V59,3940.0,4000,4000,25713-3,100,1158,7320046217112,35,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,35,1197,147,88,1,112.5714286
RECESSO 150X1200 4K 1C BETA OPTI_25713-340,RECESSO 150X1200 4K 1C BETA OPTI-Body w Winsta connector 3-pole.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,2.6,http://www.fagerhult.com,1,Standard - WAGO Winsta,25713.IES,Recesso Beta Opti,Fagerhult,3940.0,LED,1,35,V59,3940.0,4000,4000,25713-340,100,1158,7320046217136,35,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,35,1197,147,88,1,112.5714286
RECESSO 150X1200 4K 1C BETA OPTI_25713-402,RECESSO 150X1200 4K 1C BETA OPTI-LED dim DALI/Phase-pulse control.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,2.6,http://www.fagerhult.com,1,DALI/Phase-pulse control,25713.IES,Recesso Beta Opti,Fagerhult,3940.0,LED,1,35,V59,3940.0,4000,4000,25713-402,100,1158,7320046217150,35,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,35,1197,147,88,1,112.5714286
RECESSO 150X1200 4K 1C BETA OPTI_25713-454,RECESSO 150X1200 4K 1C BETA OPTI-LED body w DALI driver and Winsta connector 5-pole. Blue male for dim.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,2.6,http://www.fagerhult.com,1,DALI - WAGO Winsta,25713.IES,Recesso Beta Opti,Fagerhult,3940.0,LED,1,35,V59,3940.0,4000,4000,25713-454,100,1158,7320046217174,35,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,35,1197,147,88,1,112.5714286
RECESSO 150X1200 4K 1C BETA OPTI_25713-456,RECESSO 150X1200 4K 1C BETA OPTI-LED body w DALI driver and Wieland connector 5-pole. Blue male for dim.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,2.6,http://www.fagerhult.com,1,DALI - Wieland,25713.IES,Recesso Beta Opti,Fagerhult,3940.0,LED,1,35,V59,3940.0,4000,4000,25713-456,100,1158,7320046217198,35,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,35,1197,147,88,1,112.5714286
RECESSO 300X1200 3K 1C BETA OPTI_25714,RECESSO 300X1200 3K 1C BETA OPTI-,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.5,http://www.fagerhult.com,1,Standard,25714.IES,Recesso Beta Opti,Fagerhult,3850.0,LED,1,35,V59,3850.0,3000,3000,25714,100,1158,7320046217211,35,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,35,1197,297,71,1,110
RECESSO 300X1200 3K 1C BETA OPTI_25714-111,RECESSO 300X1200 3K 1C BETA OPTI-BODY W WIELAND CONNECTOR GST18I3 MALE.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.5,http://www.fagerhult.com,1,Standard,25714.IES,Recesso Beta Opti,Fagerhult,3850.0,LED,1,35,V59,3850.0,3000,3000,25714-111,100,1158,7320046217235,35,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,35,1197,297,71,1,110
RECESSO 300X1200 3K 1C BETA OPTI_25714-3,"RECESSO 300X1200 3K 1C BETA OPTI-BODY W CONNECTION CABLE L=2,5M FREE CABLE W PLUG.",Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.5,http://www.fagerhult.com,1,Standard,25714.IES,Recesso Beta Opti,Fagerhult,3850.0,LED,1,35,V59,3850.0,3000,3000,25714-3,100,1158,7320046217259,35,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,35,1197,297,71,1,110
RECESSO 300X1200 3K 1C BETA OPTI_25714-340,RECESSO 300X1200 3K 1C BETA OPTI-Body w Winsta connector 3-pole.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.5,http://www.fagerhult.com,1,Standard - WAGO Winsta,25714.IES,Recesso Beta Opti,Fagerhult,3850.0,LED,1,35,V59,3850.0,3000,3000,25714-340,100,1158,7320046217273,35,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,35,1197,297,71,1,110
RECESSO 300X1200 3K 1C BETA OPTI_25714-402,RECESSO 300X1200 3K 1C BETA OPTI-LED dim DALI/Phase-pulse control.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.5,http://www.fagerhult.com,1,DALI/Phase-pulse control,25714.IES,Recesso Beta Opti,Fagerhult,3850.0,LED,1,35,V59,3850.0,3000,3000,25714-402,100,1158,7320046217297,35,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,35,1197,297,71,1,110
RECESSO 300X1200 3K 1C BETA OPTI_25714-454,RECESSO 300X1200 3K 1C BETA OPTI-LED body w DALI driver and Winsta connector 5-pole. Blue male for dim.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.5,http://www.fagerhult.com,1,DALI - WAGO Winsta,25714.IES,Recesso Beta Opti,Fagerhult,3850.0,LED,1,35,V59,3850.0,3000,3000,25714-454,100,1158,7320046217310,35,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,35,1197,297,71,1,110
RECESSO 300X1200 3K 1C BETA OPTI_25714-456,RECESSO 300X1200 3K 1C BETA OPTI-LED body w DALI driver and Wieland connector 5-pole. Blue male for dim.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.5,http://www.fagerhult.com,1,DALI - Wieland,25714.IES,Recesso Beta Opti,Fagerhult,3850.0,LED,1,35,V59,3850.0,3000,3000,25714-456,100,1158,7320046217334,35,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,35,1197,297,71,1,110
RECESSO 300X1200 4K 1C BETA OPTI_25715,RECESSO 300X1200 4K 1C BETA OPTI-,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.5,http://www.fagerhult.com,1,Standard,25715.IES,Recesso Beta Opti,Fagerhult,3940.0,LED,1,35,V59,3940.0,4000,4000,25715,100,1158,7320046217358,35,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,35,1197,297,71,1,112.5714286
RECESSO 300X1200 4K 1C BETA OPTI_25715-111,RECESSO 300X1200 4K 1C BETA OPTI-BODY W WIELAND CONNECTOR GST18I3 MALE.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.5,http://www.fagerhult.com,1,Standard,25715.IES,Recesso Beta Opti,Fagerhult,3940.0,LED,1,35,V59,3940.0,4000,4000,25715-111,100,1158,7320046217372,35,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,35,1197,297,71,1,112.5714286
RECESSO 300X1200 4K 1C BETA OPTI_25715-3,"RECESSO 300X1200 4K 1C BETA OPTI-BODY W CONNECTION CABLE L=2,5M FREE CABLE W PLUG.",Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.5,http://www.fagerhult.com,1,Standard,25715.IES,Recesso Beta Opti,Fagerhult,3940.0,LED,1,35,V59,3940.0,4000,4000,25715-3,100,1158,7320046217396,35,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,35,1197,297,71,1,112.5714286
RECESSO 300X1200 4K 1C BETA OPTI_25715-340,RECESSO 300X1200 4K 1C BETA OPTI-Body w Winsta connector 3-pole.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.5,http://www.fagerhult.com,1,Standard - WAGO Winsta,25715.IES,Recesso Beta Opti,Fagerhult,3940.0,LED,1,35,V59,3940.0,4000,4000,25715-340,100,1158,7320046217419,35,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,35,1197,297,71,1,112.5714286
RECESSO 300X1200 4K 1C BETA OPTI_25715-402,RECESSO 300X1200 4K 1C BETA OPTI-LED dim DALI/Phase-pulse control.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.5,http://www.fagerhult.com,1,DALI/Phase-pulse control,25715.IES,Recesso Beta Opti,Fagerhult,3940.0,LED,1,35,V59,3940.0,4000,4000,25715-402,100,1158,7320046217433,35,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,35,1197,297,71,1,112.5714286
RECESSO 300X1200 4K 1C BETA OPTI_25715-454,RECESSO 300X1200 4K 1C BETA OPTI-LED body w DALI driver and Winsta connector 5-pole. Blue male for dim.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.5,http://www.fagerhult.com,1,DALI - WAGO Winsta,25715.IES,Recesso Beta Opti,Fagerhult,3940.0,LED,1,35,V59,3940.0,4000,4000,25715-454,100,1158,7320046217457,35,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,35,1197,297,71,1,112.5714286
RECESSO 300X1200 4K 1C BETA OPTI_25715-456,RECESSO 300X1200 4K 1C BETA OPTI-LED body w DALI driver and Wieland connector 5-pole. Blue male for dim.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.5,http://www.fagerhult.com,1,DALI - Wieland,25715.IES,Recesso Beta Opti,Fagerhult,3940.0,LED,1,35,V59,3940.0,4000,4000,25715-456,100,1158,7320046217471,35,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,35,1197,297,71,1,112.5714286
