;Diameter##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Size##OTHER##;Shape##OTHER##;ProductInformation##OTHER##;Photometric Web File##OTHER##;ModelReference##OTHER##;Material##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Description##OTHER##;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP_Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;CreatedOn##OTHER##;Control Gear##OTHER##;Color##OTHER##;Body##OTHER##;BarCode##OTHER##;BIMObjectName##OTHER##;ArticleNumber##OTHER##;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;ColorRenderingIndex##Other##;Class##OTHER##
DEVINA HÖSTGLÖD 830 CL1 CLO Dali_307004-461;410;16.3;3000;D 410 mm + H 876 mm;Circle;Body, heat sink and cover in cast aluminium. The cylinder in impact- and UV-resistant acrylic (PMMA). Driver is integrated in the luminaire. Driver is integrated in the luminaire. The cylinder covers a UV-resistant golden fabric and the inner core holds a honeycomb metal mesh.;307004-461.IES;Devina;aluminium;2022;Glass;Post;Post;A design for dusk where the light emphasizes the material features. As the sun sets, like fire has since the beginning of evolution, Höstglöd draws people together towards it’s warmth. ;2022;3000;3000;66;876;51;Created 09/05/2018;DaliCLO;Gold;Gold;7320047306600;Devina Höstglöd;307004-461;42;min. 80;1
DEVINA HÖSTGLÖD 830 CL1 CLONightDimming1_307004-464;410;16.3;3000;D 410 mm + H 876 mm;Circle;Body, heat sink and cover in cast aluminium. The cylinder in impact- and UV-resistant acrylic (PMMA). Driver is integrated in the luminaire. Driver is integrated in the luminaire. The cylinder covers a UV-resistant golden fabric and the inner core holds a honeycomb metal mesh.;307004-464.IES;Devina;aluminium;2022;Glass;Post;Post;A design for dusk where the light emphasizes the material features. As the sun sets, like fire has since the beginning of evolution, Höstglöd draws people together towards it’s warmth. ;2022;3000;3000;66;876;51;Created 09/05/2018;CLONightDimming1;Gold;Gold;7320047306624;Devina Höstglöd;307004-464;42;min. 80;1
DEVINA HÖSTGLÖD 830 CL1 CLONightDimming2_307004-465;410;16.3;3000;D 410 mm + H 876 mm;Circle;Body, heat sink and cover in cast aluminium. The cylinder in impact- and UV-resistant acrylic (PMMA). Driver is integrated in the luminaire. Driver is integrated in the luminaire. The cylinder covers a UV-resistant golden fabric and the inner core holds a honeycomb metal mesh.;307004-465.IES;Devina;aluminium;2022;Glass;Post;Post;A design for dusk where the light emphasizes the material features. As the sun sets, like fire has since the beginning of evolution, Höstglöd draws people together towards it’s warmth. ;2022;3000;3000;66;876;51;Created 09/05/2018;CLONightDimming2;Gold;Gold;7320047306648;Devina Höstglöd;307004-465;42;min. 80;1
DEVINA HÖSTGLÖD 840 CL1 CLO Dali_307005-461;410;16.3;4000;D 410 mm + H 876 mm;Circle;Body, heat sink and cover in cast aluminium. The cylinder in impact- and UV-resistant acrylic (PMMA). Driver is integrated in the luminaire. Driver is integrated in the luminaire. The cylinder covers a UV-resistant golden fabric and the inner core holds a honeycomb metal mesh.;307005-461.IES;Devina;aluminium;1994;Glass;Post;Post;A design for dusk where the light emphasizes the material features. As the sun sets, like fire has since the beginning of evolution, Höstglöd draws people together towards it’s warmth. ;1994;4000;4000;66;876;57;Created 09/05/2018;DaliCLO;Gold;Gold;7320047306662;Devina Höstglöd;307005-461;37;min. 80;1
DEVINA HÖSTGLÖD 840 CL1 CLONightDimming1_307005-464;410;16.3;4000;D 410 mm + H 876 mm;Circle;Body, heat sink and cover in cast aluminium. The cylinder in impact- and UV-resistant acrylic (PMMA). Driver is integrated in the luminaire. Driver is integrated in the luminaire. The cylinder covers a UV-resistant golden fabric and the inner core holds a honeycomb metal mesh.;307005-464.IES;Devina;aluminium;1994;Glass;Post;Post;A design for dusk where the light emphasizes the material features. As the sun sets, like fire has since the beginning of evolution, Höstglöd draws people together towards it’s warmth. ;1994;4000;4000;66;876;57;Created 09/05/2018;CLONightDimming1;Gold;Gold;7320047306686;Devina Höstglöd;307005-464;37;min. 80;1
DEVINA HÖSTGLÖD 840 CL1 CLONightDimming2_307005-465;410;16.3;4000;D 410 mm + H 876 mm;Circle;Body, heat sink and cover in cast aluminium. The cylinder in impact- and UV-resistant acrylic (PMMA). Driver is integrated in the luminaire. Driver is integrated in the luminaire. The cylinder covers a UV-resistant golden fabric and the inner core holds a honeycomb metal mesh.;307005-465.IES;Devina;aluminium;1994;Glass;Post;Post;A design for dusk where the light emphasizes the material features. As the sun sets, like fire has since the beginning of evolution, Höstglöd draws people together towards it’s warmth. ;1994;4000;4000;66;876;57;Created 09/05/2018;CLONightDimming2;Gold;Gold;7320047306709;Devina Höstglöd;307005-465;37;min. 80;1
DEVINA HÖSTGLÖD 830 CL2 CLO Dali_307012-461;410;16.3;3000;D 410 mm + H 876 mm;Circle;Body, heat sink and cover in cast aluminium. The cylinder in impact- and UV-resistant acrylic (PMMA). Driver is integrated in the luminaire. Driver is integrated in the luminaire. The cylinder covers a UV-resistant golden fabric and the inner core holds a honeycomb metal mesh.;307012-461.IES;Devina;aluminium;2022;Glass;Post;Post;A design for dusk where the light emphasizes the material features. As the sun sets, like fire has since the beginning of evolution, Höstglöd draws people together towards it’s warmth. ;2022;3000;3000;66;876;51;Created 09/05/2018;DaliCLO;Gold;Gold;7320047307089;Devina Höstglöd;307012-461;42;min. 80;2
DEVINA HÖSTGLÖD 830 CL2 CLONightDimming1_307012-464;410;16.3;3000;D 410 mm + H 876 mm;Circle;Body, heat sink and cover in cast aluminium. The cylinder in impact- and UV-resistant acrylic (PMMA). Driver is integrated in the luminaire. Driver is integrated in the luminaire. The cylinder covers a UV-resistant golden fabric and the inner core holds a honeycomb metal mesh.;307012-464.IES;Devina;aluminium;2022;Glass;Post;Post;A design for dusk where the light emphasizes the material features. As the sun sets, like fire has since the beginning of evolution, Höstglöd draws people together towards it’s warmth. ;2022;3000;3000;66;876;51;Created 09/05/2018;CLONightDimming1;Gold;Gold;7320047307102;Devina Höstglöd;307012-464;42;min. 80;2
DEVINA HÖSTGLÖD 830 CL2 CLONightDimming2_307012-465;410;16.3;3000;D 410 mm + H 876 mm;Circle;Body, heat sink and cover in cast aluminium. The cylinder in impact- and UV-resistant acrylic (PMMA). Driver is integrated in the luminaire. Driver is integrated in the luminaire. The cylinder covers a UV-resistant golden fabric and the inner core holds a honeycomb metal mesh.;307012-465.IES;Devina;aluminium;2022;Glass;Post;Post;A design for dusk where the light emphasizes the material features. As the sun sets, like fire has since the beginning of evolution, Höstglöd draws people together towards it’s warmth. ;2022;3000;3000;66;876;51;Created 09/05/2018;CLONightDimming2;Gold;Gold;7320047307126;Devina Höstglöd;307012-465;42;min. 80;2
DEVINA HÖSTGLÖD 840 CL2 CLO Dali_307013-461;410;16.3;4000;D 410 mm + H 876 mm;Circle;Body, heat sink and cover in cast aluminium. The cylinder in impact- and UV-resistant acrylic (PMMA). Driver is integrated in the luminaire. Driver is integrated in the luminaire. The cylinder covers a UV-resistant golden fabric and the inner core holds a honeycomb metal mesh.;307013-461.IES;Devina;aluminium;1994;Glass;Post;Post;A design for dusk where the light emphasizes the material features. As the sun sets, like fire has since the beginning of evolution, Höstglöd draws people together towards it’s warmth. ;1994;4000;4000;66;876;57;Created 09/05/2018;DaliCLO;Gold;Gold;7320047307140;Devina Höstglöd;307013-461;37;min. 80;2
DEVINA HÖSTGLÖD 840 CL2 CLONightDimming1_307013-464;410;16.3;4000;D 410 mm + H 876 mm;Circle;Body, heat sink and cover in cast aluminium. The cylinder in impact- and UV-resistant acrylic (PMMA). Driver is integrated in the luminaire. Driver is integrated in the luminaire. The cylinder covers a UV-resistant golden fabric and the inner core holds a honeycomb metal mesh.;307013-464.IES;Devina;aluminium;1994;Glass;Post;Post;A design for dusk where the light emphasizes the material features. As the sun sets, like fire has since the beginning of evolution, Höstglöd draws people together towards it’s warmth. ;1994;4000;4000;66;876;57;Created 09/05/2018;CLONightDimming1;Gold;Gold;7320047307164;Devina Höstglöd;307013-464;37;min. 80;2
DEVINA HÖSTGLÖD 840 CL2 CLONightDimming2_307013-465;410;16.3;4000;D 410 mm + H 876 mm;Circle;Body, heat sink and cover in cast aluminium. The cylinder in impact- and UV-resistant acrylic (PMMA). Driver is integrated in the luminaire. Driver is integrated in the luminaire. The cylinder covers a UV-resistant golden fabric and the inner core holds a honeycomb metal mesh.;307013-465.IES;Devina;aluminium;1994;Glass;Post;Post;A design for dusk where the light emphasizes the material features. As the sun sets, like fire has since the beginning of evolution, Höstglöd draws people together towards it’s warmth. ;1994;4000;4000;66;876;57;Created 09/05/2018;CLONightDimming2;Gold;Gold;7320047307188;Devina Höstglöd;307013-465;37;min. 80;2
