;Diameter##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Size##OTHER##;Shape##OTHER##;ProductInformation##OTHER##;Photometric Web File##OTHER##;ModelReference##OTHER##;Material##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Description##OTHER##;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP_Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;CreatedOn##OTHER##;Control Gear##OTHER##;Color##OTHER##;Body##OTHER##;BarCode##OTHER##;BIMObjectName##OTHER##;ArticleNumber##OTHER##;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;ColorRenderingIndex##Other##;Class##OTHER##
DEVINA KALLKÄLLA 830 CL1 CLO_307000-461;410;14.7;3000;D 410 mm + H 876 mm;Circle;Body, heat sink and cover in cast aluminium. The cylinder impact and UV-resistant acrylic (PMMA). Driver is integrated in the luminaire.;307000-461.IES;Devina;aluminium;1456;Glass;Post;Post;Pure minimalism creating volume without decoration, Kallkälla showcases its environment without demanding attention. The light element combines its modern aesthetics with the natural materials of the post.;1456;3000;3000;66;876;38;Created 09/05/2018;DaliCLO;Anthracite grey;Fagerhult_Alugrey_Aluminium;7320047306365;Devina Kallkälla;307000-461;40;min. 80;1
DEVINA KALLKÄLLA 830 CL1 CLO NightDimming1_307000-464;410;14.7;3000;D 410 mm + H 876 mm;Circle;Body, heat sink and cover in cast aluminium. The cylinder impact and UV-resistant acrylic (PMMA). Driver is integrated in the luminaire.;307000-464.IES;Devina;aluminium;1558;Glass;Post;Post;Pure minimalism creating volume without decoration, Kallkälla showcases its environment without demanding attention. The light element combines its modern aesthetics with the natural materials of the post.;1558;3000;3000;66;876;41;Created 09/05/2018;CLONightDimming1;Anthracite grey;Fagerhult_Alugrey_Aluminium;7320047306389;Devina Kallkälla;307000-464;40;min. 80;1
DEVINA KALLKÄLLA 830 CL1 CLO NightDimming2_307000-465;410;14.7;3000;D 410 mm + H 876 mm;Circle;Body, heat sink and cover in cast aluminium. The cylinder impact and UV-resistant acrylic (PMMA). Driver is integrated in the luminaire.;307000-465.IES;Devina;aluminium;1456;Glass;Post;Post;Pure minimalism creating volume without decoration, Kallkälla showcases its environment without demanding attention. The light element combines its modern aesthetics with the natural materials of the post.;1456;3000;3000;66;876;38;Created 09/05/2018;CLONightDimming2;Anthracite grey;Fagerhult_Alugrey_Aluminium;7320047306402;Devina Kallkälla;307000-465;40;min. 80;1
DEVINA KALLKÄLLA 840 CL1 CLO_307001-461;410;14.7;4000;D 410 mm + H 876 mm;Circle;Body, heat sink and cover in cast aluminium. The cylinder impact and UV-resistant acrylic (PMMA). Driver is integrated in the luminaire.;307001-461.IES;Devina;aluminium;1558;Glass;Post;Post;Pure minimalism creating volume without decoration, Kallkälla showcases its environment without demanding attention. The light element combines its modern aesthetics with the natural materials of the post.;1558;4000;4000;66;876;41;Created 09/05/2018;DaliCLO;Anthracite grey;Fagerhult_Alugrey_Aluminium;7320047306426;Devina Kallkälla;307001-461;40;min. 80;1
DEVINA KALLKÄLLA 840 CL1 CLO NightDimming1_307001-464;410;14.7;4000;D 410 mm + H 876 mm;Circle;Body, heat sink and cover in cast aluminium. The cylinder impact and UV-resistant acrylic (PMMA). Driver is integrated in the luminaire.;307001-464.IES;Devina;aluminium;1456;Glass;Post;Post;Pure minimalism creating volume without decoration, Kallkälla showcases its environment without demanding attention. The light element combines its modern aesthetics with the natural materials of the post.;1456;4000;4000;66;876;38;Created 09/05/2018;CLONightDimming1;Anthracite grey;Fagerhult_Alugrey_Aluminium;7320047306440;Devina Kallkälla;307001-464;40;min. 80;1
DEVINA KALLKÄLLA 840 CL1 CLO NightDimming2_307001-465;410;14.7;4000;D 410 mm + H 876 mm;Circle;Body, heat sink and cover in cast aluminium. The cylinder impact and UV-resistant acrylic (PMMA). Driver is integrated in the luminaire.;307001-465.IES;Devina;aluminium;1558;Glass;Post;Post;Pure minimalism creating volume without decoration, Kallkälla showcases its environment without demanding attention. The light element combines its modern aesthetics with the natural materials of the post.;1558;4000;4000;66;876;41;Created 09/05/2018;CLONightDimming2;Anthracite grey;Fagerhult_Alugrey_Aluminium;7320047306464;Devina Kallkälla;307001-465;40;min. 80;1
DEVINA KALLKÄLLA 830 CL2 CLO_307008-461;410;14.7;3000;D 410 mm + H 876 mm;Circle;Body, heat sink and cover in cast aluminium. The cylinder impact and UV-resistant acrylic (PMMA). Driver is integrated in the luminaire.;307008-461.IES;Devina;aluminium;1456;Glass;Post;Post;Pure minimalism creating volume without decoration, Kallkälla showcases its environment without demanding attention. The light element combines its modern aesthetics with the natural materials of the post.;1456;3000;3000;66;876;38;Created 09/05/2018;DaliCLO;Anthracite grey;Fagerhult_Alugrey_Aluminium;7320047306846;Devina Kallkälla;307008-461;40;min. 80;2
DEVINA KALLKÄLLA 830 CL2 CLO NightDimming1_307008-464;410;14.7;3000;D 410 mm + H 876 mm;Circle;Body, heat sink and cover in cast aluminium. The cylinder impact and UV-resistant acrylic (PMMA). Driver is integrated in the luminaire.;307008-464.IES;Devina;aluminium;1558;Glass;Post;Post;Pure minimalism creating volume without decoration, Kallkälla showcases its environment without demanding attention. The light element combines its modern aesthetics with the natural materials of the post.;1558;3000;3000;66;876;41;Created 09/05/2018;CLONightDimming1;Anthracite grey;Fagerhult_Alugrey_Aluminium;7320047306860;Devina Kallkälla;307008-464;40;min. 80;2
DEVINA KALLKÄLLA 830 CL2 CLO NightDimming2_307008-465;410;14.7;3000;D 410 mm + H 876 mm;Circle;Body, heat sink and cover in cast aluminium. The cylinder impact and UV-resistant acrylic (PMMA). Driver is integrated in the luminaire.;307008-465.IES;Devina;aluminium;1456;Glass;Post;Post;Pure minimalism creating volume without decoration, Kallkälla showcases its environment without demanding attention. The light element combines its modern aesthetics with the natural materials of the post.;1456;3000;3000;66;876;38;Created 09/05/2018;CLONightDimming2;Anthracite grey;Fagerhult_Alugrey_Aluminium;7320047306884;Devina Kallkälla;307008-465;40;min. 80;2
DEVINA KALLKÄLLA 840 CL2 CLO_307009-461;410;14.7;4000;D 410 mm + H 876 mm;Circle;Body, heat sink and cover in cast aluminium. The cylinder impact and UV-resistant acrylic (PMMA). Driver is integrated in the luminaire.;307009-461.IES;Devina;aluminium;1558;Glass;Post;Post;Pure minimalism creating volume without decoration, Kallkälla showcases its environment without demanding attention. The light element combines its modern aesthetics with the natural materials of the post.;1558;4000;4000;66;876;41;Created 09/05/2018;DaliCLO;Anthracite grey;Fagerhult_Alugrey_Aluminium;7320047306907;Devina Kallkälla;307009-461;40;min. 80;2
DEVINA KALLKÄLLA 840 CL2 CLO NightDimming1_307009-464;410;14.7;4000;D 410 mm + H 876 mm;Circle;Body, heat sink and cover in cast aluminium. The cylinder impact and UV-resistant acrylic (PMMA). Driver is integrated in the luminaire.;307009-464.IES;Devina;aluminium;1456;Glass;Post;Post;Pure minimalism creating volume without decoration, Kallkälla showcases its environment without demanding attention. The light element combines its modern aesthetics with the natural materials of the post.;1456;4000;4000;66;876;38;Created 09/05/2018;CLONightDimming1;Anthracite grey;Fagerhult_Alugrey_Aluminium;7320047306921;Devina Kallkälla;307009-464;40;min. 80;2
DEVINA KALLKÄLLA 840 CL2 CLO NightDimming2_307009-465;410;14.7;4000;D 410 mm + H 876 mm;Circle;Body, heat sink and cover in cast aluminium. The cylinder impact and UV-resistant acrylic (PMMA). Driver is integrated in the luminaire.;307009-465.IES;Devina;aluminium;1558;Glass;Post;Post;Pure minimalism creating volume without decoration, Kallkälla showcases its environment without demanding attention. The light element combines its modern aesthetics with the natural materials of the post.;1558;4000;4000;66;876;41;Created 09/05/2018;CLONightDimming2;Anthracite grey;Fagerhult_Alugrey_Aluminium;7320047306945;Devina Kallkälla;307009-465;40;min. 80;2
