;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Light distribution##OTHER##;Louvre type##OTHER##;Luminaire type##OTHER##
NOTOR36 PEND D 1200 DALI HL BETA 840_16085-20023;36;1.900;4000;2800;Aluminium - Fagerhult - Beta Opti Nano;1255;2800;4000;4000;20;36;135;White;Aluminium - Fagerhult - White;7320048598752;16085-20023;22.5;22.5;Notor 36;"Luminaire for pendant installation, single or in a system. Wire bracket providing flexible c/c and wire lock included in delivery. Wire suspension ordered separately; see Accessories. For various for wire suspension and mounting options, use Fagerhult Configure. To obtain an item list and calculate system length, use our configurator. Can also be mounted on wall via bracket, see Accessories. For detailed information, see the installation instructions. ";Notor 36 is a family of luminaires with minimal material use and high light comfort and performance, along with a range of louvre, length, and shape options. Made from recycled aluminium for a low carbon footprint. Pendant luminaire for single- and system-installation.;min. 80;C;3;0;1;1
NOTOR36 PEND D 1200 DALI LL BETA 840_16085-20021;36;1.900;4000;1750;Aluminium - Fagerhult - Beta Opti Nano;1255;1750;4000;4000;20;36;128;White;Aluminium - Fagerhult - White;7320048598691;16085-20021;14.5;14.5;Notor 36;"Luminaire for pendant installation, single or in a system. Wire bracket providing flexible c/c and wire lock included in delivery. Wire suspension ordered separately; see Accessories. For various for wire suspension and mounting options, use Fagerhult Configure. To obtain an item list and calculate system length, use our configurator. Can also be mounted on wall via bracket, see Accessories. For detailed information, see the installation instructions. ";Notor 36 is a family of luminaires with minimal material use and high light comfort and performance, along with a range of louvre, length, and shape options. Made from recycled aluminium for a low carbon footprint. Pendant luminaire for single- and system-installation.;min. 80;C;3;0;1;1
NOTOR36 PEND D 2400 DALI HL OPAL 840_16085-20016;36;2.900;4000;5600;Acrylic - Fagerhult - Opal;2488;5600;4000;4000;20;36;122;White;Aluminium - Fagerhult - White;7320048598547;16085-20016;47.5;47.5;Notor 36;"Luminaire for pendant installation, single or in a system. Wire bracket providing flexible c/c and wire lock included in delivery. Wire suspension ordered separately; see Accessories. For various for wire suspension and mounting options, use Fagerhult Configure. To obtain an item list and calculate system length, use our configurator. Can also be mounted on wall via bracket, see Accessories. For detailed information, see the installation instructions. ";Notor 36 is a family of luminaires with minimal material use and high light comfort and performance, along with a range of louvre, length, and shape options. Made from recycled aluminium for a low carbon footprint. Pendant luminaire for single- and system-installation.;min. 80;C;3;0;3;1
NOTOR36 PEND D 1200 DALI HL OPAL 840_16085-20015;36;1.700;4000;2800;Acrylic - Fagerhult - Opal;1249;2800;4000;4000;20;36;117;White;Aluminium - Fagerhult - White;7320048598516;16085-20015;25.5;25.5;Notor 36;"Luminaire for pendant installation, single or in a system. Wire bracket providing flexible c/c and wire lock included in delivery. Wire suspension ordered separately; see Accessories. For various for wire suspension and mounting options, use Fagerhult Configure. To obtain an item list and calculate system length, use our configurator. Can also be mounted on wall via bracket, see Accessories. For detailed information, see the installation instructions. ";Notor 36 is a family of luminaires with minimal material use and high light comfort and performance, along with a range of louvre, length, and shape options. Made from recycled aluminium for a low carbon footprint. Pendant luminaire for single- and system-installation.;min. 80;C;3;0;3;1
NOTOR36 PEND D 2400 DALI LL BETA 840_16085-20022;36;3.200;4000;3500;Aluminium - Fagerhult - Beta Opti Nano;2507;3500;4000;4000;20;36;132;White;Aluminium - Fagerhult - White;7320048598721;16085-20022;28.5;28.5;Notor 36;"Luminaire for pendant installation, single or in a system. Wire bracket providing flexible c/c and wire lock included in delivery. Wire suspension ordered separately; see Accessories. For various for wire suspension and mounting options, use Fagerhult Configure. To obtain an item list and calculate system length, use our configurator. Can also be mounted on wall via bracket, see Accessories. For detailed information, see the installation instructions. ";Notor 36 is a family of luminaires with minimal material use and high light comfort and performance, along with a range of louvre, length, and shape options. Made from recycled aluminium for a low carbon footprint. Pendant luminaire for single- and system-installation.;min. 80;C;3;0;2;1
NOTOR36 PEND D 2400 DALI LL OPAL 840_16085-20030;36;2.900;4000;3600;Acrylic - Fagerhult - Opal;2488;3600;4000;4000;20;36;119;White;Aluminium - Fagerhult - White;7320048600103;16085-20030;31.5;31.5;Notor 36;"Luminaire for pendant installation, single or in a system. Wire bracket providing flexible c/c and wire lock included in delivery. Wire suspension ordered separately; see Accessories. For various for wire suspension and mounting options, use Fagerhult Configure. To obtain an item list and calculate system length, use our configurator. Can also be mounted on wall via bracket, see Accessories. For detailed information, see the installation instructions. ";Notor 36 is a family of luminaires with minimal material use and high light comfort and performance, along with a range of louvre, length, and shape options. Made from recycled aluminium for a low carbon footprint. Pendant luminaire for single- and system-installation.;min. 80;C;3;0;3;1
NOTOR36 PEND D/I 1200 DALI  BETA 840_16085-20026;36;1.700;4000;4800;Aluminium - Fagerhult - Beta Opti Nano;1255;4800;4000;4000;20;36;133;White;Aluminium - Fagerhult - White;7320048598851;16085-20026;38;38;Notor 36;"Luminaire for pendant installation, single or in a system. Wire bracket providing flexible c/c and wire lock included in delivery. Wire suspension ordered separately; see Accessories. For various for wire suspension and mounting options, use Fagerhult Configure. To obtain an item list and calculate system length, use our configurator. Can also be mounted on wall via bracket, see Accessories. For detailed information, see the installation instructions. ";Notor 36 is a family of luminaires with minimal material use and high light comfort and performance, along with a range of louvre, length, and shape options. Made from recycled aluminium for a low carbon footprint. Pendant luminaire for single- and system-installation.;min. 80;C;3;1;1;1
NOTOR36 PEND D 2400 DALI HL BETA 840_16085-20024;36;3.200;4000;5600;Aluminium - Fagerhult - Beta Opti Nano;2507;5600;4000;4000;20;36;134;White;Aluminium - Fagerhult - White;7320048598783;16085-20024;44;44;Notor 36;"Luminaire for pendant installation, single or in a system. Wire bracket providing flexible c/c and wire lock included in delivery. Wire suspension ordered separately; see Accessories. For various for wire suspension and mounting options, use Fagerhult Configure. To obtain an item list and calculate system length, use our configurator. Can also be mounted on wall via bracket, see Accessories. For detailed information, see the installation instructions. ";Notor 36 is a family of luminaires with minimal material use and high light comfort and performance, along with a range of louvre, length, and shape options. Made from recycled aluminium for a low carbon footprint. Pendant luminaire for single- and system-installation.;min. 80;C;3;0;2;1
NOTOR36 PEND D 1200 DALI LL OPAL 840_16085-20029;36;1.700;4000;1800;Acrylic - Fagerhult - Opal;1249;1800;4000;4000;20;36;118;White;Aluminium - Fagerhult - White;7320048600073;16085-20029;16.5;16.5;Notor 36;"Luminaire for pendant installation, single or in a system. Wire bracket providing flexible c/c and wire lock included in delivery. Wire suspension ordered separately; see Accessories. For various for wire suspension and mounting options, use Fagerhult Configure. To obtain an item list and calculate system length, use our configurator. Can also be mounted on wall via bracket, see Accessories. For detailed information, see the installation instructions. ";Notor 36 is a family of luminaires with minimal material use and high light comfort and performance, along with a range of louvre, length, and shape options. Made from recycled aluminium for a low carbon footprint. Pendant luminaire for single- and system-installation.;min. 80;C;3;0;3;1
NOTOR36 PEND D 1200 DALI LL BETA 840_16085-20065;36;1.900;4000;1750;Aluminium - Fagerhult - Beta Opti Nano;1268;1750;4000;4000;20;36;128;White;Aluminium - Fagerhult - White;7320048855053;16085-20065;14.5;14.5;Notor 36;"Luminaire for pendant installation, single or in a system. Wire bracket providing flexible c/c and wire lock included in delivery. Wire suspension ordered separately; see Accessories. For various for wire suspension and mounting options, use Fagerhult Configure. To obtain an item list and calculate system length, use our configurator. Can also be mounted on wall via bracket, see Accessories. For detailed information, see the installation instructions. ";Notor 36 is a family of luminaires with minimal material use and high light comfort and performance, along with a range of louvre, length, and shape options. Made from recycled aluminium for a low carbon footprint. Pendant luminaire for single- and system-installation.;min. 80;C;3;0;1;3
NOTOR36 PEND D 1200 DALI LL OPAL 840_16085-20074;36;1.700;4000;1800;Acrylic - Fagerhult - Opal;1260;1800;4000;4000;20;36;118;White;Aluminium - Fagerhult - White;7320048855084;16085-20074;16;16;Notor 36;"Luminaire for pendant installation, single or in a system. Wire bracket providing flexible c/c and wire lock included in delivery. Wire suspension ordered separately; see Accessories. For various for wire suspension and mounting options, use Fagerhult Configure. To obtain an item list and calculate system length, use our configurator. Can also be mounted on wall via bracket, see Accessories. For detailed information, see the installation instructions. ";Notor 36 is a family of luminaires with minimal material use and high light comfort and performance, along with a range of louvre, length, and shape options. Made from recycled aluminium for a low carbon footprint. Pendant luminaire for single- and system-installation.;min. 80;C;3;0;3;3
NOTOR36 PEND D 2400 DALI LL BETA 840_16085-20075;36;3.200;4000;3500;Aluminium - Fagerhult - Beta Opti Nano;2520;3500;4000;4000;20;36;136;White;Aluminium - Fagerhult - White;7320048855114;16085-20075;27;27;Notor 36;"Luminaire for pendant installation, single or in a system. Wire bracket providing flexible c/c and wire lock included in delivery. Wire suspension ordered separately; see Accessories. For various for wire suspension and mounting options, use Fagerhult Configure. To obtain an item list and calculate system length, use our configurator. Can also be mounted on wall via bracket, see Accessories. For detailed information, see the installation instructions. ";Notor 36 is a family of luminaires with minimal material use and high light comfort and performance, along with a range of louvre, length, and shape options. Made from recycled aluminium for a low carbon footprint. Pendant luminaire for single- and system-installation.;min. 80;C;3;0;2;3
NOTOR36 PEND D 2400 DALI LL OPAL 840_16085-20076;36;2.900;4000;3600;Acrylic - Fagerhult - Opal;2499;3600;4000;4000;20;36;119;White;Aluminium - Fagerhult - White;7320048855145;16085-20076;30.5;30.5;Notor 36;"Luminaire for pendant installation, single or in a system. Wire bracket providing flexible c/c and wire lock included in delivery. Wire suspension ordered separately; see Accessories. For various for wire suspension and mounting options, use Fagerhult Configure. To obtain an item list and calculate system length, use our configurator. Can also be mounted on wall via bracket, see Accessories. For detailed information, see the installation instructions. ";Notor 36 is a family of luminaires with minimal material use and high light comfort and performance, along with a range of louvre, length, and shape options. Made from recycled aluminium for a low carbon footprint. Pendant luminaire for single- and system-installation.;min. 80;C;3;0;3;3
NOTOR36 PEND D 1200 DALI LL BETA 840_16085-20077;36;1.900;4000;1750;Aluminium - Fagerhult - Beta Opti Nano;1254;1750;4000;4000;20;36;128;White;Aluminium - Fagerhult - White;7320048855176;16085-20077;14.5;14.5;Notor 36;"Luminaire for pendant installation, single or in a system. Wire bracket providing flexible c/c and wire lock included in delivery. Wire suspension ordered separately; see Accessories. For various for wire suspension and mounting options, use Fagerhult Configure. To obtain an item list and calculate system length, use our configurator. Can also be mounted on wall via bracket, see Accessories. For detailed information, see the installation instructions. ";Notor 36 is a family of luminaires with minimal material use and high light comfort and performance, along with a range of louvre, length, and shape options. Made from recycled aluminium for a low carbon footprint. Pendant luminaire for single- and system-installation.;min. 80;C;3;0;1;2
NOTOR36 PEND D 1200 DALI LL OPAL 840_16085-20078;36;1.700;4000;1800;Acrylic - Fagerhult - Opal;1284;1800;4000;4000;20;36;118;White;Aluminium - Fagerhult - White;7320048855206;16085-20078;16;16;Notor 36;"Luminaire for pendant installation, single or in a system. Wire bracket providing flexible c/c and wire lock included in delivery. Wire suspension ordered separately; see Accessories. For various for wire suspension and mounting options, use Fagerhult Configure. To obtain an item list and calculate system length, use our configurator. Can also be mounted on wall via bracket, see Accessories. For detailed information, see the installation instructions. ";Notor 36 is a family of luminaires with minimal material use and high light comfort and performance, along with a range of louvre, length, and shape options. Made from recycled aluminium for a low carbon footprint. Pendant luminaire for single- and system-installation.;min. 80;C;3;0;3;4
NOTOR36 PEND D 2400 DALI LL OPAL 840_16085-20079;36;2.900;4000;3600;Acrylic - Fagerhult - Opal;2523;3600;4000;4000;20;36;119;White;Aluminium - Fagerhult - White;7320048855275;16085-20079;30.5;30.5;Notor 36;"Luminaire for pendant installation, single or in a system. Wire bracket providing flexible c/c and wire lock included in delivery. Wire suspension ordered separately; see Accessories. For various for wire suspension and mounting options, use Fagerhult Configure. To obtain an item list and calculate system length, use our configurator. Can also be mounted on wall via bracket, see Accessories. For detailed information, see the installation instructions. ";Notor 36 is a family of luminaires with minimal material use and high light comfort and performance, along with a range of louvre, length, and shape options. Made from recycled aluminium for a low carbon footprint. Pendant luminaire for single- and system-installation.;min. 80;C;3;0;3;4
NOTOR36 PEND D 2400 DALI LL BETA 840_16085-20064;36;3.200;4000;3500;Aluminium - Fagerhult - Beta Opti Nano;2506;3500;4000;4000;20;36;136;White;Aluminium - Fagerhult - White;7320048855244;16085-20064;27;27;Notor 36;"Luminaire for pendant installation, single or in a system. Wire bracket providing flexible c/c and wire lock included in delivery. Wire suspension ordered separately; see Accessories. For various for wire suspension and mounting options, use Fagerhult Configure. To obtain an item list and calculate system length, use our configurator. Can also be mounted on wall via bracket, see Accessories. For detailed information, see the installation instructions. ";Notor 36 is a family of luminaires with minimal material use and high light comfort and performance, along with a range of louvre, length, and shape options. Made from recycled aluminium for a low carbon footprint. Pendant luminaire for single- and system-installation.;min. 80;C;3;0;2;2
