;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Model##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Description##OTHER##;Color Rendering Index##Other##
PONDERO BETA OPTI PENDANT 1680 830 ALU_16980-402;80;4.2;3000;Pondero;4223;Aluminium - Fagerhult - BetaOpti;1678;4223;3000;3000;20;105;126;Aluminium;Aluminium - Fagerhult - White;7320048184412;16980-402;34.5;A pendant workplace luminaire that produces direct/indirect light. The Beta Opti louvre ensures high efficiency and optimal light comfort.;min. 80
PONDERO BETA OPTI PENDANT 1200 840 ALU_16983-402;80;3.4;4000;Pondero;2990;Aluminium - Fagerhult - BetaOpti;1283;2990;4000;4000;20;105;128;Aluminium;Aluminium - Fagerhult - White;7320048185754;16983-402;24;A pendant workplace luminaire that produces direct/indirect light. The Beta Opti louvre ensures high efficiency and optimal light comfort.;min. 80
PONDERO BETA OPTI PENDANT 1200 840 ALU_16983-533;80;3.4;4000;Pondero;2990;Aluminium - Fagerhult - BetaOpti;1283;2990;4000;4000;20;105;120;Aluminium;Aluminium - Fagerhult - White;7320048185761;16983-533;25;A pendant workplace luminaire that produces direct/indirect light. The Beta Opti louvre ensures high efficiency and optimal light comfort.;min. 80
PONDERO BETA OPTI PENDANT 1200 830 ALU_16982-533;80;3.4;3000;Pondero;2906;Aluminium - Fagerhult - BetaOpti;1283;2906;3000;3000;20;105;117;Aluminium;Aluminium - Fagerhult - White;7320048185747;16982-533;25;A pendant workplace luminaire that produces direct/indirect light. The Beta Opti louvre ensures high efficiency and optimal light comfort.;min. 80
PONDERO BETA OPTI PENDANT 1200 830 ALU_16982-402;80;3.4;3000;Pondero;2906;Aluminium - Fagerhult - BetaOpti;1283;2906;3000;3000;20;105;124;Aluminium;Aluminium - Fagerhult - White;7320048185730;16982-402;24;A pendant workplace luminaire that produces direct/indirect light. The Beta Opti louvre ensures high efficiency and optimal light comfort.;min. 80
PONDERO BETA OPTI PENDANT 1680 840 ALU_16981-533;80;4.2;4000;Pondero;4345;Aluminium - Fagerhult - BetaOpti;1678;4345;4000;4000;20;105;125;Aluminium;Aluminium - Fagerhult - White;7320048184467;16981-533;36;A pendant workplace luminaire that produces direct/indirect light. The Beta Opti louvre ensures high efficiency and optimal light comfort.;min. 80
PONDERO BETA OPTI PENDANT 1680 840 ALU_16981-402;80;4.2;4000;Pondero;4345;Aluminium - Fagerhult - BetaOpti;1678;4345;4000;4000;20;105;130;Aluminium;Aluminium - Fagerhult - White;7320048184443;16981-402;35;A pendant workplace luminaire that produces direct/indirect light. The Beta Opti louvre ensures high efficiency and optimal light comfort.;min. 80
PONDERO BETA OPTI PENDANT 1680 830 ALU_16980-533;80;4.2;3000;Pondero;4223;Aluminium - Fagerhult - BetaOpti;1678;4223;3000;3000;20;105;122;Aluminium;Aluminium - Fagerhult - White;7320048184429;16980-533;36;A pendant workplace luminaire that produces direct/indirect light. The Beta Opti louvre ensures high efficiency and optimal light comfort.;min. 80
