;Diameter##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Size##OTHER##;Shape##OTHER##;ProductInformation##OTHER##;Photometric Web File##OTHER##;ModelReference##OTHER##;Material##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Description##OTHER##;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP_Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;CreatedOn##OTHER##;Control Gear##OTHER##;Color##OTHER##;Body##OTHER##;BarCode##OTHER##;BIMObjectName##OTHER##;ArticleNumber##OTHER##;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;ColorRenderingIndex##Other##
TIBI  PENDANT D800 4K BRUSHED ALU_54792-402;800;9.0;4000;D 800 mm + H 270 mm;Circle;Diffuser in specular opal acrylic. Luminaire body and decorative edge ring in aluminium. Decorative edge ring enameled in glossy black (RAL 9005) or clear enamelled brushed aluminium. Colour-coordinated ceiling cup.;54791-402.IES;Tibi Pendant;aluminium;6990;Fagerhult_Opal;Ceiling;Pendant;A round beam decorative luminaire in three sizes for entrances and stairwells, for example. Also available with Tunable White for dynamic lighting. ;6990;4000;4000;20;270;119;Created 23/04/2018;DALIPhasePulseControl;Brushed aluminium;Fagerhult_Brushed_aluminium;7320046202408;Tibi Pendant;54792-402;59;min. 80
TIBI  PENDANT D800 4K BLACK_54795-402;800;9.0;4000;D 800 mm + H 270 mm;Circle;Diffuser in specular opal acrylic. Luminaire body and decorative edge ring in aluminium. Decorative edge ring enameled in glossy black (RAL 9005) or clear enamelled brushed aluminium. Colour-coordinated ceiling cup.;54794-402.IES;Tibi Pendant;aluminium;6990;Fagerhult_Opal;Ceiling;Pendant;A round beam decorative luminaire in three sizes for entrances and stairwells, for example. Also available with Tunable White for dynamic lighting. ;6990;4000;4000;20;270;119;Created 23/04/2019;DALIPhasePulseControl;Black;Fagerhult_Black_aluminium;7320046203924;Tibi Pendant;54795-402;59;min. 80
TIBI  PENDANT D800 3K BRUSHED ALU_55270-402;800;9.0;3000;D 800 mm + H 270 mm;Circle;Diffuser in specular opal acrylic. Luminaire body and decorative edge ring in aluminium. Decorative edge ring enameled in glossy black (RAL 9005) or clear enamelled brushed aluminium. Colour-coordinated ceiling cup.;55269-402.IES;Tibi Pendant;aluminium;6640;Fagerhult_Opal;Ceiling;Pendant;A round beam decorative luminaire in three sizes for entrances and stairwells, for example. Also available with Tunable White for dynamic lighting. ;6640;3000;3000;20;270;113;Created 23/04/2020;DALIPhasePulseControl;Brushed aluminium;Fagerhult_Brushed_aluminium;7320046423995;Tibi Pendant;55270-402;59;min. 80
TIBI  PENDANT D800 3K BLACK_55273-402;800;9.0;3000;D 800 mm + H 270 mm;Circle;Diffuser in specular opal acrylic. Luminaire body and decorative edge ring in aluminium. Decorative edge ring enameled in glossy black (RAL 9005) or clear enamelled brushed aluminium. Colour-coordinated ceiling cup.;55272-402.IES;Tibi Pendant;aluminium;6640;Fagerhult_Opal;Ceiling;Pendant;A round beam decorative luminaire in three sizes for entrances and stairwells, for example. Also available with Tunable White for dynamic lighting. ;6640;3000;3000;20;270;113;Created 23/04/2021;DALIPhasePulseControl;Black;Fagerhult_Black_aluminium;7320046424053;Tibi Pendant;55273-402;59;min. 80
