;Diameter##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Size##OTHER##;Shape##OTHER##;ProductInformation##OTHER##;Photometric Web File##OTHER##;ModelReference##OTHER##;Material##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Description##OTHER##;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP_Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;CreatedOn##OTHER##;Control Gear##OTHER##;Color##OTHER##;Body##OTHER##;BarCode##OTHER##;BIMObjectName##OTHER##;ArticleNumber##OTHER##;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;ColorRenderingIndex##Other##
TIBI  PENDANT D400 4K BRUSHED ALU_54790-402;400;3.3;4000;D 400 mm + H 138 mm;Circle;Diffuser in specular opal acrylic. Luminaire body and decorative edge ring in aluminium. Decorative edge ring enameled in glossy black (RAL 9005) or clear enamelled brushed aluminium. Colour-coordinated ceiling cup.;54790-402.IES;Tibi Pendant;aluminium;1790;Fagerhult_Opal;Ceiling;Pendant;A round beam decorative luminaire in three sizes for entrances and stairwells, for example. Also available with Tunable White for dynamic lighting. ;1790;4000;4000;20;138;103;Created 23/04/2018;DALIPhasePulseControl;Brushed aluminium;Fagerhult_Brushed_aluminium;7320046219079;Tibi Pendant;54790-402;17;min. 80
TIBI  PENDANT D400 4K BLACK_54793-402;400;3.3;4000;D 400 mm + H 138 mm;Circle;Diffuser in specular opal acrylic. Luminaire body and decorative edge ring in aluminium. Decorative edge ring enameled in glossy black (RAL 9005) or clear enamelled brushed aluminium. Colour-coordinated ceiling cup.;54793-402.IES;Tibi Pendant;aluminium;1790;Fagerhult_Opal;Ceiling;Pendant;A round beam decorative luminaire in three sizes for entrances and stairwells, for example. Also available with Tunable White for dynamic lighting. ;1790;4000;4000;20;138;103;Created 23/04/2019;DALIPhasePulseControl;Black;Fagerhult_Black_aluminium;7320046219086;Tibi Pendant;54793-402;17;min. 80
TIBI  PENDANT D400 3K BRUSHED ALU_55268-402;400;3.3;3000;D 400 mm + H 138 mm;Circle;Diffuser in specular opal acrylic. Luminaire body and decorative edge ring in aluminium. Decorative edge ring enameled in glossy black (RAL 9005) or clear enamelled brushed aluminium. Colour-coordinated ceiling cup.;55268-402.IES;Tibi Pendant;aluminium;1700;Fagerhult_Opal;Ceiling;Pendant;A round beam decorative luminaire in three sizes for entrances and stairwells, for example. Also available with Tunable White for dynamic lighting. ;1700;3000;3000;20;138;98;Created 23/04/2020;DALIPhasePulseControl;Brushed aluminium;Fagerhult_Brushed_aluminium;7320046423957;Tibi Pendant;55268-402;17;min. 80
TIBI  PENDANT D400 3K BLACK_55271-402;400;3.3;3000;D 400 mm + H 138 mm;Circle;Diffuser in specular opal acrylic. Luminaire body and decorative edge ring in aluminium. Decorative edge ring enameled in glossy black (RAL 9005) or clear enamelled brushed aluminium. Colour-coordinated ceiling cup.;55271-402.IES;Tibi Pendant;aluminium;1700;Fagerhult_Opal;Ceiling;Pendant;A round beam decorative luminaire in three sizes for entrances and stairwells, for example. Also available with Tunable White for dynamic lighting. ;1700;3000;3000;20;138;98;Created 23/04/2021;DALIPhasePulseControl;Black;Fagerhult_Black_aluminium;7320046424015;Tibi Pendant;55271-402;17;min. 80
