;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Diameter##LENGTH##MILLIMETERS;Model##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Type##OTHER##
ZKYE 55 G2 PENDANT D2W WHITE WIDE BEAM_65152-402;0.7;2700;963;246;963;2700;2700;20;70;White;Aluminium - Fagerhult - White;7320049852228;65152-402;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;F;1;1
ZKYE 55 G2 PENDANT D2W WHITE WIDE BEAM_65152-522;0.7;2700;963;246;963;2700;2700;20;69;White;Aluminium - Fagerhult - White;7320049852242;65152-522;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;F;1;1
ZKYE 55 G2 PENDANT D2W WHITE WIDE BEAM_65152-527;0.7;2700;963;246;963;2700;2700;20;71;White;Aluminium - Fagerhult - White;7320049852266;65152-527;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;F;1;1
ZKYE 55 G2 PENDANT D2W BLACK WIDE BEAM_65153-402;0.7;2700;963;246;963;2700;2700;20;70;Black;Aluminium - Fagerhult - Black;7320049852303;65153-402;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;F;1;1
ZKYE 55 G2 PENDANT D2W BLACK WIDE BEAM_65153-522;0.7;2700;963;246;963;2700;2700;20;69;Black;Aluminium - Fagerhult - Black;7320049852327;65153-522;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;F;1;1
ZKYE 55 G2 PENDANT D2W BLACK WIDE BEAM_65153-527;0.7;2700;963;246;963;2700;2700;20;71;Black;Aluminium - Fagerhult - Black;7320049852341;65153-527;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;F;1;1
ZKYE 55 G2 PENDANT TRACK D2W WHITE WIDE BEAM_65166-504;0.7;2700;963;246;963;2700;2700;20;70;White;Aluminium - Fagerhult - White;7320049853324;65166-504;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;F;1;3
ZKYE 55 G2 PENDANT TRACK D2W WHITE WIDE BEAM_65166-522;0.7;2700;963;246;963;2700;2700;20;70;White;Aluminium - Fagerhult - White;7320049853348;65166-522;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;F;1;2
ZKYE 55 G2 PENDANT TRACK D2W WHITE WIDE BEAM_65166-527;0.7;2700;963;246;963;2700;2700;20;70;White;Aluminium - Fagerhult - White;7320049853362;65166-527;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;F;1;2
ZKYE 55 G2 PENDANT TRACK D2W BLACK WIDE BEAM_65167-504;0.7;2700;963;246;963;2700;2700;20;70;Black;Aluminium - Fagerhult - Black;7320049853409;65167-504;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;F;1;3
ZKYE 55 G2 PENDANT TRACK D2W BLACK WIDE BEAM_65167-522;0.7;2700;963;246;963;2700;2700;20;70;Black;Aluminium - Fagerhult - Black;7320049853423;65167-522;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;F;1;2
ZKYE 55 G2 PENDANT TRACK D2W BLACK WIDE BEAM_65167-527;0.7;2700;963;246;963;2700;2700;20;70;Black;Aluminium - Fagerhult - Black;7320049853447;65167-527;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;F;1;2
ZKYE 55 G2 PENDANT 927  WHITE NARROW BEAM_65190;0.8;2700;1501;246;1501;2700;2700;20;105;White;Aluminium - Fagerhult - White;7316911255945;65190;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 927 WHITE NARROW BEAM_65190-402;0.8;2700;1501;246;1501;2700;2700;20;107;White;Aluminium - Fagerhult - White;7316911255969;65190-402;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 927 WHITE NARROW BEAM_65190-522;0.8;2700;1501;246;1501;2700;2700;20;107;White;Aluminium - Fagerhult - White;7316911255983;65190-522;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 927 WHITE NARROW BEAM_65190-527;0.8;2700;1501;246;1501;2700;2700;20;109;White;Aluminium - Fagerhult - White;7316911256003;65190-527;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 927 BLACK NARROW BEAM_65191;0.8;2700;1501;246;1501;2700;2700;20;105;Black;Aluminium - Fagerhult - Black;7316911256027;65191;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 927 BLACK NARROW BEAM_65191-402;0.8;2700;1501;246;1501;2700;2700;20;107;Black;Aluminium - Fagerhult - Black;7316911256041;65191-402;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 927 BLACK NARROW BEAM_65191-522;0.8;2700;1501;246;1501;2700;2700;20;107;Black;Aluminium - Fagerhult - Black;7316911256065;65191-522;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 927 BLACK NARROW BEAM_65191-527;0.8;2700;1501;246;1501;2700;2700;20;109;Black;Aluminium - Fagerhult - Black;7316911256089;65191-527;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 927 BLACK MEDIUM BEAM_65193;0.8;2700;1498;246;1498;2700;2700;20;105;Black;Aluminium - Fagerhult - Black;7316911256188;65193;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 927 BLACK MEDIUM BEAM_65193-402;0.8;2700;1498;246;1498;2700;2700;20;107;Black;Aluminium - Fagerhult - Black;7316911256201;65193-402;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 927 BLACK MEDIUM BEAM_65193-522;0.8;2700;1498;246;1498;2700;2700;20;107;Black;Aluminium - Fagerhult - Black;7316911256225;65193-522;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 927 BLACK MEDIUM BEAM_65193-527;0.8;2700;1498;246;1498;2700;2700;20;109;Black;Aluminium - Fagerhult - Black;7316911256249;65193-527;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 927  WHITE WIDE BEAM_65194;0.8;2700;1542;246;1542;2700;2700;20;108;White;Aluminium - Fagerhult - White;7316911256263;65194;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 927 WHITE WIDE BEAM_65194-402;0.8;2700;1542;246;1542;2700;2700;20;110;White;Aluminium - Fagerhult - White;7316911256287;65194-402;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 927 WHITE WIDE BEAM_65194-522;0.8;2700;1542;246;1542;2700;2700;20;110;White;Aluminium - Fagerhult - White;7316911256300;65194-522;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 927 WHITE WIDE BEAM_65194-527;0.8;2700;1542;246;1542;2700;2700;20;112;White;Aluminium - Fagerhult - White;7316911256324;65194-527;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 927 BLACK WIDE BEAM_65195;0.8;2700;1542;246;1542;2700;2700;20;108;Black;Aluminium - Fagerhult - Black;7316911256348;65195;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 927 BLACK WIDE BEAM_65195-402;0.8;2700;1542;246;1542;2700;2700;20;110;Black;Aluminium - Fagerhult - Black;7316911256362;65195-402;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 927 BLACK WIDE BEAM_65195-522;0.8;2700;1542;246;1542;2700;2700;20;110;Black;Aluminium - Fagerhult - Black;7316911256386;65195-522;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 927 BLACK WIDE BEAM_65195-527;0.8;2700;1542;246;1542;2700;2700;20;112;Black;Aluminium - Fagerhult - Black;7316911256409;65195-527;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 930  WHITE NARROW BEAM_65196;0.8;3000;1516;246;1516;3000;3000;20;106;White;Aluminium - Fagerhult - White;7316911256423;65196;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 930 WHITE NARROW BEAM_65196-402;0.8;3000;1516;246;1516;3000;3000;20;108;White;Aluminium - Fagerhult - White;7316911256447;65196-402;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 930 WHITE NARROW BEAM_65196-522;0.8;3000;1516;246;1516;3000;3000;20;108;White;Aluminium - Fagerhult - White;7316911256461;65196-522;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 930 WHITE NARROW BEAM_65196-527;0.8;3000;1516;246;1516;3000;3000;20;110;White;Aluminium - Fagerhult - White;7316911256485;65196-527;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 930 BLACK NARROW BEAM_65197;0.8;3000;1516;246;1516;3000;3000;20;106;Black;Aluminium - Fagerhult - Black;7316911256508;65197;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 930 BLACK NARROW BEAM_65197-402;0.8;3000;1516;246;1516;3000;3000;20;108;Black;Aluminium - Fagerhult - Black;7316911256522;65197-402;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 930 BLACK NARROW BEAM_65197-522;0.8;3000;1516;246;1516;3000;3000;20;108;Black;Aluminium - Fagerhult - Black;7316911256546;65197-522;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 930 BLACK NARROW BEAM_65197-527;0.8;3000;1516;246;1516;3000;3000;20;110;Black;Aluminium - Fagerhult - Black;7316911256560;65197-527;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 930  WHITE MEDIUM BEAM_65198;0.8;3000;1513;246;1513;3000;3000;20;106;White;Aluminium - Fagerhult - White;7316911256584;65198;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 930 WHITE MEDIUM BEAM_65198-402;0.8;3000;1513;246;1513;3000;3000;20;108;White;Aluminium - Fagerhult - White;7316911256607;65198-402;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 930 WHITE MEDIUM BEAM_65198-522;0.8;3000;1513;246;1513;3000;3000;20;108;White;Aluminium - Fagerhult - White;7316911256621;65198-522;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 930 WHITE MEDIUM BEAM_65198-527;0.8;3000;1513;246;1513;3000;3000;20;110;White;Aluminium - Fagerhult - White;7316911256645;65198-527;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 930 BLACK MEDIUM BEAM_65199;0.8;3000;1513;246;1513;3000;3000;20;106;Black;Aluminium - Fagerhult - Black;7316911256669;65199;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 930 BLACK MEDIUM BEAM_65199-402;0.8;3000;1513;246;1513;3000;3000;20;108;Black;Aluminium - Fagerhult - Black;7316911256683;65199-402;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 930 BLACK MEDIUM BEAM_65199-522;0.8;3000;1513;246;1513;3000;3000;20;108;Black;Aluminium - Fagerhult - Black;7316911256706;65199-522;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 930 BLACK MEDIUM BEAM_65199-527;0.8;3000;1513;246;1513;3000;3000;20;110;Black;Aluminium - Fagerhult - Black;7316911256720;65199-527;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 930  WHITE WIDE BEAM_65200;0.8;3000;1558;246;1558;3000;3000;20;109;White;Aluminium - Fagerhult - White;7316911256744;65200;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 930 WHITE WIDE BEAM_65200-402;0.8;3000;1558;246;1558;3000;3000;20;111;White;Aluminium - Fagerhult - White;7316911256768;65200-402;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 930 WHITE WIDE BEAM_65200-522;0.8;3000;1558;246;1558;3000;3000;20;111;White;Aluminium - Fagerhult - White;7316911256782;65200-522;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 930 WHITE WIDE BEAM_65200-527;0.8;3000;1558;246;1558;3000;3000;20;113;White;Aluminium - Fagerhult - White;7316911256805;65200-527;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 930 BLACK WIDE BEAM_65201;0.8;3000;1558;246;1558;3000;3000;20;109;Black;Aluminium - Fagerhult - Black;7316911256829;65201;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 930 BLACK WIDE BEAM_65201-402;0.8;3000;1558;246;1558;3000;3000;20;111;Black;Aluminium - Fagerhult - Black;7316911256843;65201-402;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 930 BLACK WIDE BEAM_65201-522;0.8;3000;1558;246;1558;3000;3000;20;111;Black;Aluminium - Fagerhult - Black;7316911256867;65201-522;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 930 BLACK WIDE BEAM_65201-527;0.8;3000;1558;246;1558;3000;3000;20;113;Black;Aluminium - Fagerhult - Black;7316911256881;65201-527;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT TRACK 927 WHITE NARROW BEAM_65204-504;0.8;2700;1501;246;1501;2700;2700;20;107;White;Aluminium - Fagerhult - White;7316911256928;65204-504;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;3
ZKYE 55 G2 PENDANT TRACK 927  WHITE NARROW BEAM_65204;0.8;2700;1501;246;1501;2700;2700;20;105;White;Aluminium - Fagerhult - White;7316911256904;65204;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;2
ZKYE 55 G2 PENDANT TRACK 927 WHITE NARROW BEAM_65204-522;0.8;2700;1501;246;1501;2700;2700;20;107;White;Aluminium - Fagerhult - White;7316911256942;65204-522;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;2
ZKYE 55 G2 PENDANT TRACK 927 WHITE NARROW BEAM_65204-527;0.8;2700;1501;246;1501;2700;2700;20;109;White;Aluminium - Fagerhult - White;7316911256966;65204-527;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;2
ZKYE 55 G2 PENDANT TRACK 927 BLACK NARROW BEAM_65205;0.8;2700;1501;246;1501;2700;2700;20;105;Black;Aluminium - Fagerhult - Black;7316911256980;65205;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;2
ZKYE 55 G2 PENDANT TRACK 927 BLACK NARROW BEAM_65205-504;0.8;2700;1501;246;1501;2700;2700;20;107;Black;Aluminium - Fagerhult - Black;7316911257000;65205-504;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;3
ZKYE 55 G2 PENDANT TRACK 927 BLACK NARROW BEAM_65205-522;0.8;2700;1501;246;1501;2700;2700;20;107;Black;Aluminium - Fagerhult - Black;7316911257024;65205-522;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;2
ZKYE 55 G2 PENDANT TRACK 927 BLACK NARROW BEAM_65205-527;0.8;2700;1501;246;1501;2700;2700;20;109;Black;Aluminium - Fagerhult - Black;7316911257048;65205-527;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;2
ZKYE 55 G2 PENDANT TRACK 927  WHITE MEDIUM BEAM_65206;0.8;2700;1498;246;1498;2700;2700;20;105;White;Aluminium - Fagerhult - White;7316911257062;65206;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;2
ZKYE 55 G2 PENDANT TRACK 927 WHITE MEDIUM BEAM_65206-504;0.8;2700;1498;246;1498;2700;2700;20;107;White;Aluminium - Fagerhult - White;7316911257086;65206-504;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;3
ZKYE 55 G2 PENDANT TRACK 927 WHITE MEDIUM BEAM_65206-522;0.8;2700;1498;246;1498;2700;2700;20;107;White;Aluminium - Fagerhult - White;7316911257109;65206-522;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;2
ZKYE 55 G2 PENDANT TRACK 927 WHITE MEDIUM BEAM_65206-527;0.8;2700;1498;246;1498;2700;2700;20;109;White;Aluminium - Fagerhult - White;7316911257123;65206-527;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;2
ZKYE 55 G2 PENDANT TRACK 927 BLACK MEDIUM BEAM_65207;0.8;2700;1498;246;1498;2700;2700;20;105;Black;Aluminium - Fagerhult - Black;7316911257147;65207;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;2
ZKYE 55 G2 PENDANT TRACK 927 BLACK MEDIUM BEAM_65207-504;0.8;2700;1498;246;1498;2700;2700;20;107;Black;Aluminium - Fagerhult - Black;7316911257161;65207-504;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;3
ZKYE 55 G2 PENDANT TRACK 927 BLACK MEDIUM BEAM_65207-522;0.8;2700;1498;246;1498;2700;2700;20;107;Black;Aluminium - Fagerhult - Black;7316911257185;65207-522;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;2
ZKYE 55 G2 PENDANT TRACK 927 BLACK MEDIUM BEAM_65207-527;0.8;2700;1498;246;1498;2700;2700;20;109;Black;Aluminium - Fagerhult - Black;7316911257208;65207-527;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;2
ZKYE 55 G2 PENDANT TRACK 927  WHITE WIDE BEAM_65208;0.8;2700;1542;246;1542;2700;2700;20;108;White;Aluminium - Fagerhult - White;7316911257222;65208;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;2
ZKYE 55 G2 PENDANT TRACK 927 WHITE WIDE BEAM_65208-504;0.8;2700;1542;246;1542;2700;2700;20;110;White;Aluminium - Fagerhult - White;7316911257246;65208-504;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;3
ZKYE 55 G2 PENDANT TRACK 927 WHITE WIDE BEAM_65208-522;0.8;2700;1542;246;1542;2700;2700;20;110;White;Aluminium - Fagerhult - White;7316911257260;65208-522;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;2
ZKYE 55 G2 PENDANT TRACK 927 WHITE WIDE BEAM_65208-527;0.8;2700;1542;246;1542;2700;2700;20;112;White;Aluminium - Fagerhult - White;7316911257284;65208-527;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;2
ZKYE 55 G2 PENDANT TRACK 927 BLACK WIDE BEAM_65209;0.8;2700;1542;246;1542;2700;2700;20;108;Black;Aluminium - Fagerhult - Black;7316911257307;65209;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;2
ZKYE 55 G2 PENDANT TRACK 927 BLACK WIDE BEAM_65209-522;0.8;2700;1542;246;1542;2700;2700;20;110;Black;Aluminium - Fagerhult - Black;7316911257345;65209-522;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;2
ZKYE 55 G2 PENDANT TRACK 927 BLACK WIDE BEAM_65209-504;0.8;2700;1542;246;1542;2700;2700;20;110;Black;Aluminium - Fagerhult - Black;7316911257321;65209-504;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;3
ZKYE 55 G2 PENDANT TRACK 927 BLACK WIDE BEAM_65209-527;0.8;2700;1542;246;1542;2700;2700;20;112;Black;Aluminium - Fagerhult - Black;7316911257369;65209-527;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;2
ZKYE 55 G2 PENDANT TRACK 930  WHITE NARROW BEAM_65210;0.8;3000;1516;246;1516;3000;3000;20;106;White;Aluminium - Fagerhult - White;7316911257383;65210;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;2
ZKYE 55 G2 PENDANT TRACK 930 WHITE NARROW BEAM_65210-504;0.8;3000;1516;246;1516;3000;3000;20;108;White;Aluminium - Fagerhult - White;7316911257406;65210-504;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;3
ZKYE 55 G2 PENDANT TRACK 930 WHITE NARROW BEAM_65210-522;0.8;3000;1516;246;1516;3000;3000;20;108;White;Aluminium - Fagerhult - White;7316911257420;65210-522;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;2
ZKYE 55 G2 PENDANT TRACK 930 WHITE NARROW BEAM_65210-527;0.8;3000;1516;246;1516;3000;3000;20;110;White;Aluminium - Fagerhult - White;7316911257444;65210-527;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;2
ZKYE 55 G2 PENDANT TRACK 930 BLACK NARROW BEAM_65211;0.8;3000;1516;246;1516;3000;3000;20;106;Black;Aluminium - Fagerhult - Black;7316911257468;65211;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;2
ZKYE 55 G2 PENDANT TRACK 930 BLACK NARROW BEAM_65211-504;0.8;3000;1516;246;1516;3000;3000;20;108;Black;Aluminium - Fagerhult - Black;7316911257482;65211-504;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;3
ZKYE 55 G2 PENDANT TRACK 930 BLACK NARROW BEAM_65211-522;0.8;3000;1516;246;1516;3000;3000;20;108;Black;Aluminium - Fagerhult - Black;7316911257505;65211-522;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;2
ZKYE 55 G2 PENDANT TRACK 930 BLACK NARROW BEAM_65211-527;0.8;3000;1516;246;1516;3000;3000;20;110;Black;Aluminium - Fagerhult - Black;7316911257529;65211-527;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;2
ZKYE 55 G2 PENDANT TRACK 930  WHITE MEDIUM BEAM_65212;0.8;3000;1513;246;1513;3000;3000;20;106;White;Aluminium - Fagerhult - White;7316911257543;65212;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;2
ZKYE 55 G2 PENDANT TRACK 930 WHITE MEDIUM BEAM_65212-504;0.8;3000;1513;246;1513;3000;3000;20;108;White;Aluminium - Fagerhult - White;7316911257567;65212-504;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;3
ZKYE 55 G2 PENDANT TRACK 930 WHITE MEDIUM BEAM_65212-522;0.8;3000;1513;246;1513;3000;3000;20;108;White;Aluminium - Fagerhult - White;7316911257581;65212-522;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;2
ZKYE 55 G2 PENDANT TRACK 930 WHITE MEDIUM BEAM_65212-527;0.8;3000;1513;246;1513;3000;3000;20;110;White;Aluminium - Fagerhult - White;7316911257604;65212-527;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;2
ZKYE 55 G2 PENDANT TRACK 930 BLACK MEDIUM BEAM_65213;0.8;3000;1513;246;1513;3000;3000;20;106;Black;Aluminium - Fagerhult - Black;7316911257628;65213;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;2
ZKYE 55 G2 PENDANT TRACK 930 BLACK MEDIUM BEAM_65213-504;0.8;3000;1513;246;1513;3000;3000;20;108;Black;Aluminium - Fagerhult - Black;7316911257642;65213-504;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;3
ZKYE 55 G2 PENDANT TRACK 930 BLACK MEDIUM BEAM_65213-522;0.8;3000;1513;246;1513;3000;3000;20;108;Black;Aluminium - Fagerhult - Black;7316911257666;65213-522;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;2
ZKYE 55 G2 PENDANT TRACK 930 BLACK MEDIUM BEAM_65213-527;0.8;3000;1513;246;1513;3000;3000;20;110;Black;Aluminium - Fagerhult - Black;7316911257680;65213-527;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;2
ZKYE 55 G2 PENDANT TRACK 930  WHITE WIDE BEAM_65214;0.8;3000;1558;246;1558;3000;3000;20;109;White;Aluminium - Fagerhult - White;7316911257703;65214;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;2
ZKYE 55 G2 PENDANT TRACK 930 WHITE WIDE BEAM_65214-504;0.8;3000;1558;246;1558;3000;3000;20;111;White;Aluminium - Fagerhult - White;7316911257727;65214-504;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;3
ZKYE 55 G2 PENDANT TRACK 930 WHITE WIDE BEAM_65214-522;0.8;3000;1558;246;1558;3000;3000;20;111;White;Aluminium - Fagerhult - White;7316911257741;65214-522;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;2
ZKYE 55 G2 PENDANT TRACK 930 WHITE WIDE BEAM_65214-527;0.8;3000;1558;246;1558;3000;3000;20;113;White;Aluminium - Fagerhult - White;7316911257765;65214-527;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;2
ZKYE 55 G2 PENDANT TRACK 930 BLACK WIDE BEAM_65215;0.8;3000;1558;246;1558;3000;3000;20;109;Black;Aluminium - Fagerhult - Black;7316911257789;65215;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;2
ZKYE 55 G2 PENDANT TRACK 930 BLACK WIDE BEAM_65215-504;0.8;3000;1558;246;1558;3000;3000;20;111;Black;Aluminium - Fagerhult - Black;7316911257802;65215-504;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;3
ZKYE 55 G2 PENDANT TRACK 930 BLACK WIDE BEAM_65215-522;0.8;3000;1558;246;1558;3000;3000;20;111;Black;Aluminium - Fagerhult - Black;7316911257826;65215-522;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;2
ZKYE 55 G2 PENDANT TRACK 930 BLACK WIDE BEAM_65215-527;0.8;3000;1558;246;1558;3000;3000;20;113;Black;Aluminium - Fagerhult - Black;7316911257840;65215-527;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;2
ZKYE 55 G2 PENDANT 927  WHITE MEDIUM BEAM_65192;0.8;2700;1498;246;1498;2700;2700;20;105;White;Aluminium - Fagerhult - White;7316911256102;65192;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 927 WHITE MEDIUM BEAM_65192-402;0.8;2700;1498;246;1498;2700;2700;20;107;White;Aluminium - Fagerhult - White;7316911256126;65192-402;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 927 WHITE MEDIUM BEAM_65192-522;0.8;2700;1498;246;1498;2700;2700;20;107;White;Aluminium - Fagerhult - White;7316911256140;65192-522;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
ZKYE 55 G2 PENDANT 927 WHITE MEDIUM BEAM_65192-527;0.8;2700;1498;246;1498;2700;2700;20;109;White;Aluminium - Fagerhult - White;7316911256164;65192-527;14;14;55;Zkye 55 G2 Pendant;A Ø 55 mm pendant luminaire. Deep reflector for optimal light comfort and and good light distribution. For mounting to fixed ceilings with ceiling cups, or on contact rails with adapter.;min. 90;E;1;1
