;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Organic Response##OTHER##
MULTILUME FLAT DELTA VTB 300X1200 4K 4KLM_23914-402;296;6;4000;3309;Acrylic - Fagerhult - Delta Microprism;1196;3309;4000;4000;44;52;134;White;Steel - Fagerhult - White;7320043467978;23914-402;26;26;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X600 3K CRI 90_23164;296;3.5;3000;2083;Acrylic - Fagerhult - Delta Microprism;596;2083;3000;3000;44;52;103;White;Steel - Fagerhult - White;7320046618827;23164;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 300X600 3K CRI 90_23164-3;296;3.5;3000;2083;Acrylic - Fagerhult - Delta Microprism;596;2083;3000;3000;44;52;103;White;Steel - Fagerhult - White;7320046634858;23164-3;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 300X600 4K CRI 90_23164-111;296;3.5;3000;2083;Acrylic - Fagerhult - Delta Microprism;596;2083;3000;3000;44;52;103;White;Steel - Fagerhult - White;7320047269288;23164-111;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 300X600 4K CRI 90_23164-340;296;3.5;3000;2083;Acrylic - Fagerhult - Delta Microprism;596;2083;3000;3000;44;52;103;White;Steel - Fagerhult - White;7320047269325;23164-340;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 300X600 3K CRI 90_23164-402;296;3.5;3000;1905;Acrylic - Fagerhult - Delta Microprism;596;1905;3000;3000;44;52;103;White;Steel - Fagerhult - White;7320046634865;23164-402;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 300X600 4K CRI 90_23164-519;296;3.5;3000;2083;Acrylic - Fagerhult - Delta Microprism;596;2083;3000;3000;44;52;103;White;Steel - Fagerhult - White;7320047269363;23164-519;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 300X600 4K CRI 90_23164-520;296;3.5;3000;1905;Acrylic - Fagerhult - Delta Microprism;596;1905;3000;3000;44;52;103;White;Steel - Fagerhult - White;7320047269387;23164-520;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 300X600 4K CRI 90_23164-528;296;3.5;3000;1905;Acrylic - Fagerhult - Delta Microprism;596;1905;3000;3000;44;52;103;White;Steel - Fagerhult - White;7320047269301;23164-528;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 300X600 4K CRI 90_23164-529;296;3.5;3000;1905;Acrylic - Fagerhult - Delta Microprism;596;1905;3000;3000;44;52;103;White;Steel - Fagerhult - White;7320047269349;23164-529;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 300X600 4K CRI 90_23165;296;3.5;4000;2218;Acrylic - Fagerhult - Delta Microprism;596;2218;4000;4000;44;52;109;White;Steel - Fagerhult - White;7320046618834;23165;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 300X600 4K CRI 90_23165-3;296;3.5;4000;2218;Acrylic - Fagerhult - Delta Microprism;596;2218;4000;4000;44;52;109;White;Steel - Fagerhult - White;7320046634872;23165-3;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 300X600 4K CRI 90_23165-111;296;3.5;4000;2218;Acrylic - Fagerhult - Delta Microprism;596;2218;4000;4000;44;52;109;White;Steel - Fagerhult - White;7320047269400;23165-111;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 300X600 4K CRI 90_23165-340;296;3.5;4000;2218;Acrylic - Fagerhult - Delta Microprism;596;2218;4000;4000;44;52;109;White;Steel - Fagerhult - White;7320047269448;23165-340;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 300X600 4K CRI 90_23165-402;296;3.5;4000;2029;Acrylic - Fagerhult - Delta Microprism;596;2029;4000;4000;44;52;110;White;Steel - Fagerhult - White;7320046634889;23165-402;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 300X600 4K CRI 90_23165-519;296;3.5;4000;2218;Acrylic - Fagerhult - Delta Microprism;596;2218;4000;4000;44;52;109;White;Steel - Fagerhult - White;7320047269486;23165-519;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 300X600 4K CRI 90_23165-520;296;3.5;4000;2029;Acrylic - Fagerhult - Delta Microprism;596;2029;4000;4000;44;52;110;White;Steel - Fagerhult - White;7320047269509;23165-520;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 300X600 4K CRI 90_23165-528;296;3.5;4000;2029;Acrylic - Fagerhult - Delta Microprism;596;2029;4000;4000;44;52;110;White;Steel - Fagerhult - White;7320047269424;23165-528;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 300X600 4K CRI 90_23165-529;296;3.5;4000;2029;Acrylic - Fagerhult - Delta Microprism;596;2029;4000;4000;44;52;110;White;Steel - Fagerhult - White;7320047269462;23165-529;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 300X1200 3K 3,5KLM CRI 90_23720;296;6;3000;4025;Acrylic - Fagerhult - Delta Microprism;1196;4025;3000;3000;44;52;108;White;Steel - Fagerhult - White;7320046651190;23720;37;37;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 300X1200 3K 3,5KLM CRI 90_23720-3;296;6;3000;4025;Acrylic - Fagerhult - Delta Microprism;1196;4025;3000;3000;44;52;108;White;Steel - Fagerhult - White;7320046651213;23720-3;37;37;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 300X1200 3K CRI 90_23720-111;296;6;3000;4025;Acrylic - Fagerhult - Delta Microprism;1196;4025;3000;3000;44;52;108;White;Steel - Fagerhult - White;7320047269523;23720-111;37;37;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 300X1200 3K CRI 90_23720-340;296;6;3000;4025;Acrylic - Fagerhult - Delta Microprism;1196;4025;3000;3000;44;52;108;White;Steel - Fagerhult - White;7320047269561;23720-340;37;37;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 300X1200 3K 3,5KLM CRI 90_23720-402;296;6;3000;3757;Acrylic - Fagerhult - Delta Microprism;1196;3757;3000;3000;44;52;110;White;Steel - Fagerhult - White;7320046651237;23720-402;37;37;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 300X1200 3K CRI 90_23720-519;296;6;3000;4025;Acrylic - Fagerhult - Delta Microprism;1196;4025;3000;3000;44;52;108;White;Steel - Fagerhult - White;7320047269608;23720-519;37;37;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 300X1200 3K CRI 90_23720-520;296;6;3000;3757;Acrylic - Fagerhult - Delta Microprism;1196;3757;3000;3000;44;52;110;White;Steel - Fagerhult - White;7320047269622;23720-520;37;37;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 300X1200 3K CRI 90_23720-528;296;6;3000;3757;Acrylic - Fagerhult - Delta Microprism;1196;3757;3000;3000;44;52;110;White;Steel - Fagerhult - White;7320047269547;23720-528;37;37;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 300X1200 3K CRI 90_23720-529;296;6;3000;3757;Acrylic - Fagerhult - Delta Microprism;1196;3757;3000;3000;44;52;110;White;Steel - Fagerhult - White;7320047269585;23720-529;37;37;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 300X1200 4K 3,5KLM CRI 90_23721;296;6;4000;4286;Acrylic - Fagerhult - Delta Microprism;1196;4286;4000;4000;44;52;115;White;Steel - Fagerhult - White;7320046651244;23721;37;37;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 300X1200 4K 3,5KLM CRI 90_23721-3;296;6;4000;4286;Acrylic - Fagerhult - Delta Microprism;1196;4286;4000;4000;44;52;115;White;Steel - Fagerhult - White;7320046651251;23721-3;37;37;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 300X1200 4K CRI 90_23721-111;296;6;4000;4286;Acrylic - Fagerhult - Delta Microprism;1196;4286;4000;4000;44;52;115;White;Steel - Fagerhult - White;7320047269646;23721-111;37;37;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 300X1200 4K CRI 90_23721-340;296;6;4000;4286;Acrylic - Fagerhult - Delta Microprism;1196;4286;4000;4000;44;52;115;White;Steel - Fagerhult - White;7320047269684;23721-340;37;37;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 300X1200 4K 3,5KLM CRI 90_23721-402;296;6;4000;4001;Acrylic - Fagerhult - Delta Microprism;1196;4001;4000;4000;44;52;117;White;Steel - Fagerhult - White;7320046651275;23721-402;37;37;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 300X1200 4K CRI 90_23721-519;296;6;4000;4286;Acrylic - Fagerhult - Delta Microprism;1196;4286;4000;4000;44;52;115;White;Steel - Fagerhult - White;7320047269721;23721-519;37;37;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 300X1200 4K CRI 90_23721-520;296;6;4000;4001;Acrylic - Fagerhult - Delta Microprism;1196;4001;4000;4000;44;52;117;White;Steel - Fagerhult - White;7320047269745;23721-520;37;37;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 300X1200 4K CRI 90_23721-528;296;6;4000;4001;Acrylic - Fagerhult - Delta Microprism;1196;4001;4000;4000;44;52;117;White;Steel - Fagerhult - White;7320047269660;23721-528;37;37;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 300X1200 4K CRI 90_23721-529;296;6;4000;4001;Acrylic - Fagerhult - Delta Microprism;1196;4001;4000;4000;44;52;117;White;Steel - Fagerhult - White;7320047269707;23721-529;37;37;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 600X600 3K 3,5KLM CRI90_23783;596;4.5;3000;4256;Acrylic - Fagerhult - Delta Microprism;596;4256;3000;3000;44;52;114;White;Steel - Fagerhult - White;7320043448342;23783;37;37;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 600X600 3K 3,5KLM CRI90_23783-3;596;4.5;3000;4256;Acrylic - Fagerhult - Delta Microprism;596;4256;3000;3000;44;52;114;White;Steel - Fagerhult - White;7320043448403;23783-3;37;37;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 600X600 3K CRI 90_23783-111;596;4.5;3000;4256;Acrylic - Fagerhult - Delta Microprism;596;4256;3000;3000;44;52;114;White;Steel - Fagerhult - White;7320047269769;23783-111;37;37;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 600X600 3K CRI 90_23783-340;596;4.5;3000;4256;Acrylic - Fagerhult - Delta Microprism;596;4256;3000;3000;44;52;114;White;Steel - Fagerhult - White;7320047269806;23783-340;37;37;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 600X600 3K 3,5KLM CRI90_23783-402;596;4.5;3000;3973;Acrylic - Fagerhult - Delta Microprism;596;3973;3000;3000;44;52;116;White;Steel - Fagerhult - White;7320043448410;23783-402;37;37;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 600X600 3K CRI 90_23783-519;596;4.5;3000;4256;Acrylic - Fagerhult - Delta Microprism;596;4256;3000;3000;44;52;114;White;Steel - Fagerhult - White;7320047269844;23783-519;37;37;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 600X600 3K CRI 90_23783-520;596;4.5;3000;3973;Acrylic - Fagerhult - Delta Microprism;596;3973;3000;3000;44;52;116;White;Steel - Fagerhult - White;7320047269868;23783-520;37;37;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 600X600 3K CRI 90_23783-528;596;4.5;3000;3973;Acrylic - Fagerhult - Delta Microprism;596;3973;3000;3000;44;52;116;White;Steel - Fagerhult - White;7320047269783;23783-528;37;37;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 600X600 3K CRI 90_23783-529;596;4.5;3000;3973;Acrylic - Fagerhult - Delta Microprism;596;3973;3000;3000;44;52;116;White;Steel - Fagerhult - White;7320047269820;23783-529;37;37;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 600X600 4K 3,5KLM CRI90_23784;596;4.5;4000;4532;Acrylic - Fagerhult - Delta Microprism;596;4532;4000;4000;44;52;121;White;Steel - Fagerhult - White;7320043448427;23784;37;37;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 600X600 4K 3,5KLM CRI90_23784-3;596;4.5;4000;4532;Acrylic - Fagerhult - Delta Microprism;596;4532;4000;4000;44;52;121;White;Steel - Fagerhult - White;7320043448434;23784-3;37;37;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT HB DELTA 600X600 4K 4KLM_23784-111;596;4.5;4000;3804;Acrylic - Fagerhult - Delta Microprism;596;3804;4000;4000;44;52;106;White;Steel - Fagerhult - White;7320047381140;23784-111;36;36;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 600X600 4K CRI 90_23784-340;596;4.5;4000;4532;Acrylic - Fagerhult - Delta Microprism;596;4532;4000;4000;44;52;121;White;Steel - Fagerhult - White;7320047269929;23784-340;37;37;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 600X600 4K 3,5KLM CRI90_23784-402;596;4.5;4000;4231;Acrylic - Fagerhult - Delta Microprism;596;4231;4000;4000;44;52;123;White;Steel - Fagerhult - White;7320043448441;23784-402;37;37;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 600X600 4K CRI 90_23784-519;596;4.5;4000;4532;Acrylic - Fagerhult - Delta Microprism;596;4532;4000;4000;44;52;121;White;Steel - Fagerhult - White;7320047269967;23784-519;37;37;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 600X600 4K CRI 90_23784-520;596;4.5;4000;4231;Acrylic - Fagerhult - Delta Microprism;596;4231;4000;4000;44;52;123;White;Steel - Fagerhult - White;7320047269981;23784-520;37;37;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 600X600 4K CRI 90_23784-528;596;4.5;4000;4231;Acrylic - Fagerhult - Delta Microprism;596;4231;4000;4000;44;52;123;White;Steel - Fagerhult - White;7320047269905;23784-528;37;37;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 600X600 4K CRI 90_23784-529;596;4.5;4000;4231;Acrylic - Fagerhult - Delta Microprism;596;4231;4000;4000;44;52;123;White;Steel - Fagerhult - White;7320047269943;23784-529;37;37;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 600X600 3K 3KLM_23786;596;4.5;3000;2733;Acrylic - Fagerhult - Delta Microprism;596;2733;3000;3000;44;52;135;White;Steel - Fagerhult - White;7320043343456;23786;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 3K 3KLM_23786-3;596;4.5;3000;2733;Acrylic - Fagerhult - Delta Microprism;596;2733;3000;3000;44;52;135;White;Steel - Fagerhult - White;7320043343463;23786-3;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 3K_23786-111;596;4.5;3000;2733;Acrylic - Fagerhult - Delta Microprism;596;2733;3000;3000;44;52;135;White;Steel - Fagerhult - White;7320047270000;23786-111;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 3K_23786-340;596;4.5;3000;2733;Acrylic - Fagerhult - Delta Microprism;596;2733;3000;3000;44;52;135;White;Steel - Fagerhult - White;7320047270048;23786-340;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 3K 3KLM_23786-402;596;4.5;3000;2460;Acrylic - Fagerhult - Delta Microprism;596;2460;3000;3000;44;52;138;White;Steel - Fagerhult - White;7320043343470;23786-402;19;19;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 3K_23786-519;596;4.5;3000;2733;Acrylic - Fagerhult - Delta Microprism;596;2733;3000;3000;44;52;135;White;Steel - Fagerhult - White;7320047270086;23786-519;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 3K_23786-520;596;4.5;3000;2460;Acrylic - Fagerhult - Delta Microprism;596;2460;3000;3000;44;52;138;White;Steel - Fagerhult - White;7320047270109;23786-520;19;19;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 3K_23786-528;596;4.5;3000;2460;Acrylic - Fagerhult - Delta Microprism;596;2460;3000;3000;44;52;138;White;Steel - Fagerhult - White;7320047270024;23786-528;19;19;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 3K_23786-529;596;4.5;3000;2460;Acrylic - Fagerhult - Delta Microprism;596;2460;3000;3000;44;52;138;White;Steel - Fagerhult - White;7320047270062;23786-529;19;19;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT HB DELTA 600X600 3K 3KLM_23788;599;4.5;3000;2733;Acrylic - Fagerhult - Delta Microprism;599;2733;3000;3000;44;52;135;White;Steel - Fagerhult - White;7320043343562;23788;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT HB DELTA 600X600 3K 3KLM_23788-3;599;4.5;3000;2733;Acrylic - Fagerhult - Delta Microprism;599;2733;3000;3000;44;52;135;White;Steel - Fagerhult - White;7320043343579;23788-3;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA 600X600 HB 3K_23788-111;599;4.5;3000;2733;Acrylic - Fagerhult - Delta Microprism;599;2733;3000;3000;44;52;135;White;Steel - Fagerhult - White;7320047270123;23788-111;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA 600X600 HB 3K_23788-340;599;4.5;3000;2733;Acrylic - Fagerhult - Delta Microprism;599;2733;3000;3000;44;52;135;White;Steel - Fagerhult - White;7320047270161;23788-340;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT HB DELTA 600X600 3K 3KLM_23788-402;599;4.5;3000;2460;Acrylic - Fagerhult - Delta Microprism;599;2460;3000;3000;44;52;138;White;Steel - Fagerhult - White;7320043343586;23788-402;19;19;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA 600X600 HB 3K_23788-519;599;4.5;3000;2733;Acrylic - Fagerhult - Delta Microprism;599;2733;3000;3000;44;52;135;White;Steel - Fagerhult - White;7320047270208;23788-519;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA 600X600 HB 3K_23788-520;599;4.5;3000;2460;Acrylic - Fagerhult - Delta Microprism;599;2460;3000;3000;44;52;138;White;Steel - Fagerhult - White;7320047270222;23788-520;19;19;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA 600X600 HB 3K_23788-528;599;4.5;3000;2460;Acrylic - Fagerhult - Delta Microprism;599;2460;3000;3000;44;52;138;White;Steel - Fagerhult - White;7320047270147;23788-528;19;19;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA 600X600 HB 3K_23788-529;599;4.5;3000;2460;Acrylic - Fagerhult - Delta Microprism;599;2460;3000;3000;44;52;138;White;Steel - Fagerhult - White;7320047270185;23788-529;19;19;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 4K 3KLM_23790;596;4.5;4000;2812;Acrylic - Fagerhult - Delta Microprism;596;2812;4000;4000;44;52;139;White;Steel - Fagerhult - White;7320043343784;23790;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 4K 3KLM_23790-3;596;4.5;4000;2812;Acrylic - Fagerhult - Delta Microprism;596;2812;4000;4000;44;52;139;White;Steel - Fagerhult - White;7320043343791;23790-3;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 4K_23790-111;596;4.5;4000;2812;Acrylic - Fagerhult - Delta Microprism;596;2812;4000;4000;44;52;139;White;Steel - Fagerhult - White;7320047270246;23790-111;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 4K_23790-340;596;4.5;4000;2812;Acrylic - Fagerhult - Delta Microprism;596;2812;4000;4000;44;52;139;White;Steel - Fagerhult - White;7320047270284;23790-340;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X6004K 3KLM_23790-402;596;4.5;4000;2531;Acrylic - Fagerhult - Delta Microprism;596;2531;4000;4000;44;52;142;White;Steel - Fagerhult - White;7320043343807;23790-402;19;19;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 4K_23790-519;596;4.5;4000;2812;Acrylic - Fagerhult - Delta Microprism;596;2812;4000;4000;44;52;139;White;Steel - Fagerhult - White;7320047270321;23790-519;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 4K_23790-520;596;4.5;4000;2531;Acrylic - Fagerhult - Delta Microprism;596;2531;4000;4000;44;52;142;White;Steel - Fagerhult - White;7320047270345;23790-520;19;19;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 4K_23790-528;596;4.5;4000;2531;Acrylic - Fagerhult - Delta Microprism;596;2531;4000;4000;44;52;142;White;Steel - Fagerhult - White;7320047270260;23790-528;19;19;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 4K_23790-529;596;4.5;4000;2531;Acrylic - Fagerhult - Delta Microprism;596;2531;4000;4000;44;52;142;White;Steel - Fagerhult - White;7320047270307;23790-529;19;19;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT HB DELTA 600X600 4K 3KLM_23792;599;4.5;4000;2812;Acrylic - Fagerhult - Delta Microprism;599;2812;4000;4000;44;52;139;White;Steel - Fagerhult - White;7320043343852;23792;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT HB DELTA 600X600 4K 3KLM_23792-3;599;4.5;4000;2812;Acrylic - Fagerhult - Delta Microprism;599;2812;4000;4000;44;52;139;White;Steel - Fagerhult - White;7320043343869;23792-3;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA 600X600 HB 4K_23792-111;599;4.5;4000;2812;Acrylic - Fagerhult - Delta Microprism;599;2812;4000;4000;44;52;139;White;Steel - Fagerhult - White;7320047270369;23792-111;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA 600X600 HB 4K_23792-340;599;4.5;4000;2812;Acrylic - Fagerhult - Delta Microprism;599;2812;4000;4000;44;52;139;White;Steel - Fagerhult - White;7320047270406;23792-340;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT HB DELTA 600X600 4K 3KLM_23792-402;599;4.5;4000;2531;Acrylic - Fagerhult - Delta Microprism;599;2531;4000;4000;44;52;142;White;Steel - Fagerhult - White;7320043343883;23792-402;19;19;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA 600X600 HB 4K_23792-519;599;4.5;4000;2812;Acrylic - Fagerhult - Delta Microprism;599;2812;4000;4000;44;52;139;White;Steel - Fagerhult - White;7320047270444;23792-519;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA 600X600 HB 4K_23792-520;599;4.5;4000;2531;Acrylic - Fagerhult - Delta Microprism;599;2531;4000;4000;44;52;142;White;Steel - Fagerhult - White;7320047270468;23792-520;19;19;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA 600X600 HB 4K_23792-528;599;4.5;4000;2531;Acrylic - Fagerhult - Delta Microprism;599;2531;4000;4000;44;52;142;White;Steel - Fagerhult - White;7320047270383;23792-528;19;19;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA 600X600 HB 4K_23792-529;599;4.5;4000;2531;Acrylic - Fagerhult - Delta Microprism;599;2531;4000;4000;44;52;142;White;Steel - Fagerhult - White;7320047270420;23792-529;19;19;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB TW 300X600_23801;296;2.5;4000;2304;Acrylic - Fagerhult - Delta Microprism;596;2304;4000;4000;44;52;98;White;Steel - Fagerhult - White;7320047592928;23801;24;24;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA VTB 600X600 3K 4,5KLM_23806;596;4.5;3000;4394;Acrylic - Fagerhult - Delta Microprism;596;4394;3000;3000;44;52;136;White;Steel - Fagerhult - White;7320043326206;23806;32;32;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 3K 4,5KLM_23806-3;596;4.5;3000;4394;Acrylic - Fagerhult - Delta Microprism;596;4394;3000;3000;44;52;136;White;Steel - Fagerhult - White;7320043326213;23806-3;32;32;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 3K_23806-111;596;4.5;3000;4394;Acrylic - Fagerhult - Delta Microprism;596;4394;3000;3000;44;52;136;White;Steel - Fagerhult - White;7320047270482;23806-111;32;32;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 3K_23806-340;596;4.5;3000;4394;Acrylic - Fagerhult - Delta Microprism;596;4394;3000;3000;44;52;136;White;Steel - Fagerhult - White;7320047270529;23806-340;32;32;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 3K 4,5KLM_23806-402;596;4.5;3000;3961;Acrylic - Fagerhult - Delta Microprism;596;3961;3000;3000;44;52;138;White;Steel - Fagerhult - White;7320043326237;23806-402;30.5;30.5;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 3K_23806-519;596;4.5;3000;4394;Acrylic - Fagerhult - Delta Microprism;596;4394;3000;3000;44;52;136;White;Steel - Fagerhult - White;7320047270567;23806-519;32;32;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 3K_23806-520;596;4.5;3000;3961;Acrylic - Fagerhult - Delta Microprism;596;3961;3000;3000;44;52;138;White;Steel - Fagerhult - White;7320047270581;23806-520;30.5;30.5;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 3K_23806-528;596;4.5;3000;3961;Acrylic - Fagerhult - Delta Microprism;596;3961;3000;3000;44;52;138;White;Steel - Fagerhult - White;7320047270505;23806-528;30.5;30.5;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 3K_23806-529;596;4.5;3000;3961;Acrylic - Fagerhult - Delta Microprism;596;3961;3000;3000;44;52;138;White;Steel - Fagerhult - White;7320047270543;23806-529;30.5;30.5;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT HB DELTA 600X600 3K 4,5KLM_23808;599;4.5;3000;4394;Acrylic - Fagerhult - Delta Microprism;599;4394;3000;3000;44;52;136;White;Steel - Fagerhult - White;7320043326275;23808;32;32;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT HB DELTA 600X600 3K 4,5KLM_23808-3;599;4.5;3000;4394;Acrylic - Fagerhult - Delta Microprism;599;4394;3000;3000;44;52;136;White;Steel - Fagerhult - White;7320043326282;23808-3;32;32;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA 600X600 HB 3K_23808-111;599;4.5;3000;4394;Acrylic - Fagerhult - Delta Microprism;599;4394;3000;3000;44;52;136;White;Steel - Fagerhult - White;7320047270604;23808-111;32;32;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA 600X600 HB 3K_23808-340;599;4.5;3000;4394;Acrylic - Fagerhult - Delta Microprism;599;4394;3000;3000;44;52;136;White;Steel - Fagerhult - White;7320047270642;23808-340;32;32;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT HB DELTA 600X600 3K 4,5KLM_23808-402;599;4.5;3000;3961;Acrylic - Fagerhult - Delta Microprism;599;3961;3000;3000;44;52;138;White;Steel - Fagerhult - White;7320043326299;23808-402;30.5;30.5;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA 600X600 HB 3K_23808-519;599;4.5;3000;4394;Acrylic - Fagerhult - Delta Microprism;599;4394;3000;3000;44;52;136;White;Steel - Fagerhult - White;7320047270680;23808-519;32;32;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA 600X600 HB 3K_23808-520;599;4.5;3000;3961;Acrylic - Fagerhult - Delta Microprism;599;3961;3000;3000;44;52;138;White;Steel - Fagerhult - White;7320047270703;23808-520;30.5;30.5;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA 600X600 HB 3K_23808-528;599;4.5;3000;3961;Acrylic - Fagerhult - Delta Microprism;599;3961;3000;3000;44;52;138;White;Steel - Fagerhult - White;7320047270628;23808-528;30.5;30.5;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA 600X600 HB 3K_23808-529;599;4.5;3000;3961;Acrylic - Fagerhult - Delta Microprism;599;3961;3000;3000;44;52;138;White;Steel - Fagerhult - White;7320047270666;23808-529;30.5;30.5;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 4K 4,5KLM_23810;596;4.5;4000;4521;Acrylic - Fagerhult - Delta Microprism;596;4521;4000;4000;44;52;140;White;Steel - Fagerhult - White;7320043326350;23810;32;32;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 4K 4,5KLM_23810-3;596;4.5;4000;4521;Acrylic - Fagerhult - Delta Microprism;596;4521;4000;4000;44;52;140;White;Steel - Fagerhult - White;7320043326367;23810-3;32;32;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 4K_23810-111;596;4.5;4000;4521;Acrylic - Fagerhult - Delta Microprism;596;4521;4000;4000;44;52;140;White;Steel - Fagerhult - White;7320047270727;23810-111;32;32;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 4K_23810-340;596;4.5;4000;4521;Acrylic - Fagerhult - Delta Microprism;596;4521;4000;4000;44;52;140;White;Steel - Fagerhult - White;7320047270765;23810-340;32;32;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 4K 4,5KLM_23810-402;596;4.5;4000;4075;Acrylic - Fagerhult - Delta Microprism;596;4075;4000;4000;44;52;142;White;Steel - Fagerhult - White;7320043326374;23810-402;30.5;30.5;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 4K_23810-519;596;4.5;4000;4521;Acrylic - Fagerhult - Delta Microprism;596;4521;4000;4000;44;52;140;White;Steel - Fagerhult - White;7320047270802;23810-519;32;32;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 4K_23810-520;596;4.5;4000;4075;Acrylic - Fagerhult - Delta Microprism;596;4075;4000;4000;44;52;142;White;Steel - Fagerhult - White;7320047270826;23810-520;30.5;30.5;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 4K_23810-528;596;4.5;4000;4075;Acrylic - Fagerhult - Delta Microprism;596;4075;4000;4000;44;52;142;White;Steel - Fagerhult - White;7320047270741;23810-528;30.5;30.5;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 4K_23810-529;596;4.5;4000;4075;Acrylic - Fagerhult - Delta Microprism;596;4075;4000;4000;44;52;142;White;Steel - Fagerhult - White;7320047270789;23810-529;30.5;30.5;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT HB DELTA 600X600 4K 4,5KLM_23812;599;4.5;4000;4521;Acrylic - Fagerhult - Delta Microprism;599;4521;4000;4000;44;52;140;White;Steel - Fagerhult - White;7320043326411;23812;32;32;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT HB DELTA 600X600 4K 4,5KLM_23812-3;599;4.5;4000;4521;Acrylic - Fagerhult - Delta Microprism;599;4521;4000;4000;44;52;140;White;Steel - Fagerhult - White;7320043326428;23812-3;32;32;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA 600X600 HB 4K_23812-111;599;4.5;4000;4521;Acrylic - Fagerhult - Delta Microprism;599;4521;4000;4000;44;52;140;White;Steel - Fagerhult - White;7320047270840;23812-111;32;32;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA 600X600 HB 4K_23812-340;599;4.5;4000;4521;Acrylic - Fagerhult - Delta Microprism;599;4521;4000;4000;44;52;140;White;Steel - Fagerhult - White;7320047270888;23812-340;32;32;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT HB DELTA 600X600 4K 4,5KLM_23812-402;599;4.5;4000;4075;Acrylic - Fagerhult - Delta Microprism;599;4075;4000;4000;44;52;142;White;Steel - Fagerhult - White;7320043326435;23812-402;30.5;30.5;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA 600X600 HB 4K_23812-519;599;4.5;4000;4521;Acrylic - Fagerhult - Delta Microprism;599;4521;4000;4000;44;52;140;White;Steel - Fagerhult - White;7320047270925;23812-519;32;32;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA 600X600 HB 4K_23812-520;599;4.5;4000;4075;Acrylic - Fagerhult - Delta Microprism;599;4075;4000;4000;44;52;142;White;Steel - Fagerhult - White;7320047270949;23812-520;30.5;30.5;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA 600X600 HB 4K_23812-528;599;4.5;4000;4075;Acrylic - Fagerhult - Delta Microprism;599;4075;4000;4000;44;52;142;White;Steel - Fagerhult - White;7320047270864;23812-528;30.5;30.5;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA 600X600 HB 4K_23812-529;599;4.5;4000;4075;Acrylic - Fagerhult - Delta Microprism;599;4075;4000;4000;44;52;142;White;Steel - Fagerhult - White;7320047270901;23812-529;30.5;30.5;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X300 3K_23837;296;2.3;3000;989;Acrylic - Fagerhult - Delta Microprism;296;989;3000;3000;44;52;114;White;Steel - Fagerhult - White;7320046367824;23837;9;9;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X300 3K_23837-3;296;2.3;3000;989;Acrylic - Fagerhult - Delta Microprism;296;989;3000;3000;44;52;114;White;Steel - Fagerhult - White;7320046367831;23837-3;9;9;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X300 3K_23837-402;296;2.3;3000;892;Acrylic - Fagerhult - Delta Microprism;296;892;3000;3000;44;52;114;White;Steel - Fagerhult - White;7320046367848;23837-402;8.5;8.5;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X300 4K_23839;296;2.3;4000;1018;Acrylic - Fagerhult - Delta Microprism;296;1018;4000;4000;44;52;117;White;Steel - Fagerhult - White;7320046367886;23839;9;9;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X300 4K_23839-3;296;2.3;4000;1018;Acrylic - Fagerhult - Delta Microprism;296;1018;4000;4000;44;52;117;White;Steel - Fagerhult - White;7320046367893;23839-3;9;9;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X300 4K_23839-402;296;2.3;4000;918;Acrylic - Fagerhult - Delta Microprism;296;918;4000;4000;44;52;118;White;Steel - Fagerhult - White;7320046367909;23839-402;8.5;8.5;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 3K 4KLM_23868;596;4.5;3000;3774;Acrylic - Fagerhult - Delta Microprism;596;3774;3000;3000;44;52;136;White;Steel - Fagerhult - White;7320043382769;23868;28;28;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 3K 4KLM_23868-3;596;4.5;3000;3774;Acrylic - Fagerhult - Delta Microprism;596;3774;3000;3000;44;52;136;White;Steel - Fagerhult - White;7320043382776;23868-3;28;28;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 3K 4KLM_23868-111;596;4.5;3000;3774;Acrylic - Fagerhult - Delta Microprism;596;3774;3000;3000;44;52;136;White;Steel - Fagerhult - White;7320047270963;23868-111;28;28;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 3K 4KLM_23868-340;596;4.5;3000;3774;Acrylic - Fagerhult - Delta Microprism;596;3774;3000;3000;44;52;136;White;Steel - Fagerhult - White;7320047271007;23868-340;28;28;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 3K 4KLM_23868-402;596;4.5;3000;3401;Acrylic - Fagerhult - Delta Microprism;596;3401;3000;3000;44;52;138;White;Steel - Fagerhult - White;7320043382783;23868-402;26;26;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 3K 4KLM_23868-519;596;4.5;3000;3774;Acrylic - Fagerhult - Delta Microprism;596;3774;3000;3000;44;52;136;White;Steel - Fagerhult - White;7320047271045;23868-519;28;28;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 3K 4KLM_23868-520;596;4.5;3000;3401;Acrylic - Fagerhult - Delta Microprism;596;3401;3000;3000;44;52;138;White;Steel - Fagerhult - White;7320047271069;23868-520;26;26;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 3K 4KLM_23868-528;596;4.5;3000;3401;Acrylic - Fagerhult - Delta Microprism;596;3401;3000;3000;44;52;138;White;Steel - Fagerhult - White;7320047270987;23868-528;26;26;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 3K 4KLM_23868-529;596;4.5;3000;3401;Acrylic - Fagerhult - Delta Microprism;596;3401;3000;3000;44;52;138;White;Steel - Fagerhult - White;7320047271021;23868-529;26;26;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT HB DELTA 600X600 3K 4KLM_23870;599;4.5;3000;3774;Acrylic - Fagerhult - Delta Microprism;599;3774;3000;3000;44;52;136;White;Steel - Fagerhult - White;7320043382820;23870;28;28;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT HB DELTA 600X600 3K 4KLM_23870-3;599;4.5;3000;3774;Acrylic - Fagerhult - Delta Microprism;599;3774;3000;3000;44;52;136;White;Steel - Fagerhult - White;7320043382837;23870-3;28;28;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA 600X600 HB 3K_23870-111;599;4.5;3000;3774;Acrylic - Fagerhult - Delta Microprism;599;3774;3000;3000;44;52;136;White;Steel - Fagerhult - White;7320047271083;23870-111;28;28;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA 600X600 HB 3K_23870-340;599;4.5;3000;3774;Acrylic - Fagerhult - Delta Microprism;599;3774;3000;3000;44;52;136;White;Steel - Fagerhult - White;7320047271120;23870-340;28;28;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT HB DELTA 600X600 3K 4KLM_23870-402;599;4.5;3000;3401;Acrylic - Fagerhult - Delta Microprism;599;3401;3000;3000;44;52;138;White;Steel - Fagerhult - White;7320043382844;23870-402;26;26;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA 600X600 HB 3K_23870-519;599;4.5;3000;3774;Acrylic - Fagerhult - Delta Microprism;599;3774;3000;3000;44;52;136;White;Steel - Fagerhult - White;7320047271168;23870-519;28;28;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA 600X600 HB 3K_23870-520;599;4.5;3000;3401;Acrylic - Fagerhult - Delta Microprism;599;3401;3000;3000;44;52;138;White;Steel - Fagerhult - White;7320047271182;23870-520;26;26;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA 600X600 HB 3K_23870-528;599;4.5;3000;3401;Acrylic - Fagerhult - Delta Microprism;599;3401;3000;3000;44;52;138;White;Steel - Fagerhult - White;7320047271106;23870-528;26;26;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA 600X600 HB 3K_23870-529;599;4.5;3000;3401;Acrylic - Fagerhult - Delta Microprism;599;3401;3000;3000;44;52;138;White;Steel - Fagerhult - White;7320047271144;23870-529;26;26;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 4K 4KLM_23872;596;4.5;4000;3883;Acrylic - Fagerhult - Delta Microprism;596;3883;4000;4000;44;52;140;White;Steel - Fagerhult - White;7320043383124;23872;28;28;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 4K 4KLM_23872-3;596;4.5;4000;3883;Acrylic - Fagerhult - Delta Microprism;596;3883;4000;4000;44;52;140;White;Steel - Fagerhult - White;7320043383131;23872-3;28;28;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 4K_23872-111;596;4.5;4000;3883;Acrylic - Fagerhult - Delta Microprism;596;3883;4000;4000;44;52;140;White;Steel - Fagerhult - White;7320047271205;23872-111;28;28;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 4K_23872-340;596;4.5;4000;3883;Acrylic - Fagerhult - Delta Microprism;596;3883;4000;4000;44;52;140;White;Steel - Fagerhult - White;7320047271243;23872-340;28;28;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 4K 4KLM_23872-402;596;4.5;4000;3499;Acrylic - Fagerhult - Delta Microprism;596;3499;4000;4000;44;52;142;White;Steel - Fagerhult - White;7320043383148;23872-402;26;26;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 4K_23872-519;596;4.5;4000;3883;Acrylic - Fagerhult - Delta Microprism;596;3883;4000;4000;44;52;140;White;Steel - Fagerhult - White;7320047271281;23872-519;28;28;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 4K_23872-520;596;4.5;4000;3499;Acrylic - Fagerhult - Delta Microprism;596;3499;4000;4000;44;52;142;White;Steel - Fagerhult - White;7320047271304;23872-520;26;26;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 4K_23872-528;596;4.5;4000;3499;Acrylic - Fagerhult - Delta Microprism;596;3499;4000;4000;44;52;142;White;Steel - Fagerhult - White;7320047271229;23872-528;26;26;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 600X600 4K_23872-529;596;4.5;4000;3499;Acrylic - Fagerhult - Delta Microprism;596;3499;4000;4000;44;52;142;White;Steel - Fagerhult - White;7320047271267;23872-529;26;26;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT HB DELTA 600X600 4K 4KLM_23874;599;4.5;4000;3883;Acrylic - Fagerhult - Delta Microprism;599;3883;4000;4000;44;52;140;White;Steel - Fagerhult - White;7320043383247;23874;28;28;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT HB DELTA 600X600 4K 4KLM_23874-3;599;4.5;4000;4054;Acrylic - Fagerhult - Delta Microprism;599;4054;4000;4000;44;52;131;White;Steel - Fagerhult - White;7320043383254;23874-3;31;31;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA 600X600 HB 4K_23874-111;599;4.5;4000;3883;Acrylic - Fagerhult - Delta Microprism;599;3883;4000;4000;44;52;140;White;Steel - Fagerhult - White;7320047271328;23874-111;28;28;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA 600X600 HB 4K_23874-340;599;4.5;4000;3883;Acrylic - Fagerhult - Delta Microprism;599;3883;4000;4000;44;52;140;White;Steel - Fagerhult - White;7320047271366;23874-340;28;28;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT HB DELTA 600X600 4K 4KLM_23874-402;599;4.5;4000;3499;Acrylic - Fagerhult - Delta Microprism;599;3499;4000;4000;44;52;142;White;Steel - Fagerhult - White;7320043383261;23874-402;26;26;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA 600X600 HB 4K_23874-519;599;4.5;4000;3883;Acrylic - Fagerhult - Delta Microprism;599;3883;4000;4000;44;52;140;White;Steel - Fagerhult - White;7320047271403;23874-519;28;28;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA 600X600 HB 4K_23874-520;599;4.5;4000;3499;Acrylic - Fagerhult - Delta Microprism;599;3499;4000;4000;44;52;142;White;Steel - Fagerhult - White;7320047271427;23874-520;26;26;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA 600X600 HB 4K_23874-528;599;4.5;4000;3499;Acrylic - Fagerhult - Delta Microprism;599;3499;4000;4000;44;52;142;White;Steel - Fagerhult - White;7320047271342;23874-528;26;26;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA 600X600 HB 4K_23874-529;599;4.5;4000;3499;Acrylic - Fagerhult - Delta Microprism;599;3499;4000;4000;44;52;142;White;Steel - Fagerhult - White;7320047271380;23874-529;26;26;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 3K 3KLM_23911;296;6;3000;2584;Acrylic - Fagerhult - Delta Microprism;1196;2584;3000;3000;44;52;127;White;Steel - Fagerhult - White;7320043467862;23911;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 3K 3KLM_23911-3;296;6;3000;2584;Acrylic - Fagerhult - Delta Microprism;1196;2584;3000;3000;44;52;127;White;Steel - Fagerhult - White;7320043467879;23911-3;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 3K_23911-111;296;6;3000;2584;Acrylic - Fagerhult - Delta Microprism;1196;2584;3000;3000;44;52;127;White;Steel - Fagerhult - White;7320047271441;23911-111;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 3K_23911-340;296;6;3000;2584;Acrylic - Fagerhult - Delta Microprism;1196;2584;3000;3000;44;52;127;White;Steel - Fagerhult - White;7320047271489;23911-340;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 3K 3KLM_23911-402;296;6;3000;2326;Acrylic - Fagerhult - Delta Microprism;1196;2326;3000;3000;44;52;131;White;Steel - Fagerhult - White;7320043467886;23911-402;19;19;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 3K_23911-519;296;6;3000;2584;Acrylic - Fagerhult - Delta Microprism;1196;2584;3000;3000;44;52;127;White;Steel - Fagerhult - White;7320047271526;23911-519;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 3K_23911-520;296;6;3000;2326;Acrylic - Fagerhult - Delta Microprism;1196;2326;3000;3000;44;52;131;White;Steel - Fagerhult - White;7320047271540;23911-520;19;19;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 3K_23911-528;296;6;3000;2326;Acrylic - Fagerhult - Delta Microprism;1196;2326;3000;3000;44;52;131;White;Steel - Fagerhult - White;7320047271465;23911-528;19;19;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 3K_23911-529;296;6;3000;2326;Acrylic - Fagerhult - Delta Microprism;1196;2326;3000;3000;44;52;131;White;Steel - Fagerhult - White;7320047271502;23911-529;19;19;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 4K 3KLM_23912;296;6;4000;2659;Acrylic - Fagerhult - Delta Microprism;1196;2659;4000;4000;44;52;131;White;Steel - Fagerhult - White;7320043467893;23912;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 4K 3KLM_23912-3;296;6;4000;2659;Acrylic - Fagerhult - Delta Microprism;1196;2659;4000;4000;44;52;131;White;Steel - Fagerhult - White;7320043467909;23912-3;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 4K_23912-111;296;6;4000;2659;Acrylic - Fagerhult - Delta Microprism;1196;2659;4000;4000;44;52;131;White;Steel - Fagerhult - White;7320047271564;23912-111;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 4K_23912-340;296;6;4000;2659;Acrylic - Fagerhult - Delta Microprism;1196;2659;4000;4000;44;52;131;White;Steel - Fagerhult - White;7320047271601;23912-340;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 4K 3KLM_23912-402;296;6;4000;2393;Acrylic - Fagerhult - Delta Microprism;1196;2393;4000;4000;44;52;134;White;Steel - Fagerhult - White;7320043467916;23912-402;19;19;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 4K_23912-519;296;6;4000;2659;Acrylic - Fagerhult - Delta Microprism;1196;2659;4000;4000;44;52;131;White;Steel - Fagerhult - White;7320047271649;23912-519;20;20;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 4K_23912-520;296;6;4000;2393;Acrylic - Fagerhult - Delta Microprism;1196;2393;4000;4000;44;52;134;White;Steel - Fagerhult - White;7320047271663;23912-520;19;19;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 4K_23912-528;296;6;4000;2393;Acrylic - Fagerhult - Delta Microprism;1196;2393;4000;4000;44;52;134;White;Steel - Fagerhult - White;7320047271588;23912-528;19;19;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 4K_23912-529;296;6;4000;2393;Acrylic - Fagerhult - Delta Microprism;1196;2393;4000;4000;44;52;134;White;Steel - Fagerhult - White;7320047271625;23912-529;19;19;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 3K 4KLM_23913;296;6;3000;3569;Acrylic - Fagerhult - Delta Microprism;1196;3569;3000;3000;44;52;129;White;Steel - Fagerhult - White;7320043467923;23913;28;28;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 3K 4KLM_23913-3;296;6;3000;3569;Acrylic - Fagerhult - Delta Microprism;1196;3569;3000;3000;44;52;129;White;Steel - Fagerhult - White;7320043467930;23913-3;28;28;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 3K_23913-111;296;6;3000;3569;Acrylic - Fagerhult - Delta Microprism;1196;3569;3000;3000;44;52;129;White;Steel - Fagerhult - White;7320047271687;23913-111;28;28;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 3K_23913-340;296;6;3000;3569;Acrylic - Fagerhult - Delta Microprism;1196;3569;3000;3000;44;52;129;White;Steel - Fagerhult - White;7320047271724;23913-340;28;28;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 3K 4KLM_23913-402;296;6;3000;3216;Acrylic - Fagerhult - Delta Microprism;1196;3216;3000;3000;44;52;130;White;Steel - Fagerhult - White;7320043467947;23913-402;26;26;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 3K_23913-519;296;6;3000;3569;Acrylic - Fagerhult - Delta Microprism;1196;3569;3000;3000;44;52;129;White;Steel - Fagerhult - White;7320047271762;23913-519;28;28;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 3K_23913-520;296;6;3000;3216;Acrylic - Fagerhult - Delta Microprism;1196;3216;3000;3000;44;52;130;White;Steel - Fagerhult - White;7320047271786;23913-520;26;26;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 3K_23913-528;296;6;3000;3216;Acrylic - Fagerhult - Delta Microprism;1196;3216;3000;3000;44;52;130;White;Steel - Fagerhult - White;7320047271700;23913-528;26;26;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 3K_23913-529;296;6;3000;3216;Acrylic - Fagerhult - Delta Microprism;1196;3216;3000;3000;44;52;130;White;Steel - Fagerhult - White;7320047271748;23913-529;26;26;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 4K 4KLM_23914;296;6;4000;3672;Acrylic - Fagerhult - Delta Microprism;1196;3672;4000;4000;44;52;133;White;Steel - Fagerhult - White;7320043467954;23914;28;28;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 4K 4KLM_23914-3;296;6;4000;3672;Acrylic - Fagerhult - Delta Microprism;1196;3672;4000;4000;44;52;133;White;Steel - Fagerhult - White;7320043467961;23914-3;28;28;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 4K_23914-111;296;6;4000;3672;Acrylic - Fagerhult - Delta Microprism;1196;3672;4000;4000;44;52;133;White;Steel - Fagerhult - White;7320047271809;23914-111;28;28;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 4K_23914-340;296;6;4000;3672;Acrylic - Fagerhult - Delta Microprism;1196;3672;4000;4000;44;52;133;White;Steel - Fagerhult - White;7320047271847;23914-340;28;28;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 4K_23914-519;296;6;4000;3672;Acrylic - Fagerhult - Delta Microprism;1196;3672;4000;4000;44;52;133;White;Steel - Fagerhult - White;7320047271885;23914-519;28;28;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 4K_23914-520;296;6;4000;3309;Acrylic - Fagerhult - Delta Microprism;1196;3309;4000;4000;44;52;134;White;Steel - Fagerhult - White;7320047271908;23914-520;26;26;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 4K_23914-528;296;6;4000;3309;Acrylic - Fagerhult - Delta Microprism;1196;3309;4000;4000;44;52;134;White;Steel - Fagerhult - White;7320047271823;23914-528;26;26;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 4K_23914-529;296;6;4000;3309;Acrylic - Fagerhult - Delta Microprism;1196;3309;4000;4000;44;52;134;White;Steel - Fagerhult - White;7320047271861;23914-529;26;26;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 3K 4,5KLM_23915;296;6;3000;4155;Acrylic - Fagerhult - Delta Microprism;1196;4155;3000;3000;44;52;128;White;Steel - Fagerhult - White;7320043468111;23915;32;32;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 3K 4,5KLM_23915-3;296;6;3000;4155;Acrylic - Fagerhult - Delta Microprism;1196;4155;3000;3000;44;52;128;White;Steel - Fagerhult - White;7320043468135;23915-3;32;32;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 3K_23915-111;296;6;3000;4155;Acrylic - Fagerhult - Delta Microprism;1196;4155;3000;3000;44;52;128;White;Steel - Fagerhult - White;7320047271922;23915-111;32;32;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 3K_23915-340;296;6;3000;4155;Acrylic - Fagerhult - Delta Microprism;1196;4155;3000;3000;44;52;128;White;Steel - Fagerhult - White;7320047271960;23915-340;32;32;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 3K 4,5KLM_23915-402;296;6;3000;3746;Acrylic - Fagerhult - Delta Microprism;1196;3746;3000;3000;44;52;131;White;Steel - Fagerhult - White;7320043468166;23915-402;30.5;30.5;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 3K_23915-519;296;6;3000;4155;Acrylic - Fagerhult - Delta Microprism;1196;4155;3000;3000;44;52;128;White;Steel - Fagerhult - White;7320047272004;23915-519;32;32;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 3K_23915-520;296;6;3000;3746;Acrylic - Fagerhult - Delta Microprism;1196;3746;3000;3000;44;52;131;White;Steel - Fagerhult - White;7320047272028;23915-520;30.5;30.5;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 3K_23915-528;296;6;3000;3746;Acrylic - Fagerhult - Delta Microprism;1196;3746;3000;3000;44;52;131;White;Steel - Fagerhult - White;7320047271946;23915-528;30.5;30.5;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 3K_23915-529;296;6;3000;3746;Acrylic - Fagerhult - Delta Microprism;1196;3746;3000;3000;44;52;131;White;Steel - Fagerhult - White;7320047271984;23915-529;30.5;30.5;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 4K 4,5KLM_23916;296;6;4000;4275;Acrylic - Fagerhult - Delta Microprism;1196;4275;4000;4000;44;52;132;White;Steel - Fagerhult - White;7320043468180;23916;32;32;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 4K 4,5KLM_23916-3;296;6;4000;4275;Acrylic - Fagerhult - Delta Microprism;1196;4275;4000;4000;44;52;132;White;Steel - Fagerhult - White;7320043468203;23916-3;32;32;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 4K_23916-111;296;6;4000;4275;Acrylic - Fagerhult - Delta Microprism;1196;4275;4000;4000;44;52;132;White;Steel - Fagerhult - White;7320047272042;23916-111;32;32;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 4K_23916-340;296;6;4000;4275;Acrylic - Fagerhult - Delta Microprism;1196;4275;4000;4000;44;52;132;White;Steel - Fagerhult - White;7320047272080;23916-340;32;32;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 4K 4,5KLM_23916-402;296;6;4000;3853;Acrylic - Fagerhult - Delta Microprism;1196;3853;4000;4000;44;52;134;White;Steel - Fagerhult - White;7320043468210;23916-402;30.5;30.5;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 4K_23916-519;296;6;4000;4275;Acrylic - Fagerhult - Delta Microprism;1196;4275;4000;4000;44;52;132;White;Steel - Fagerhult - White;7320047272127;23916-519;32;32;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 4K_23916-520;296;6;4000;3853;Acrylic - Fagerhult - Delta Microprism;1196;3853;4000;4000;44;52;134;White;Steel - Fagerhult - White;7320047272141;23916-520;30.5;30.5;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 4K_23916-528;296;6;4000;3853;Acrylic - Fagerhult - Delta Microprism;1196;3853;4000;4000;44;52;134;White;Steel - Fagerhult - White;7320047272066;23916-528;30.5;30.5;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X1200 4K_23916-529;296;6;4000;3853;Acrylic - Fagerhult - Delta Microprism;1196;3853;4000;4000;44;52;134;White;Steel - Fagerhult - White;7320047272103;23916-529;30.5;30.5;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X600 STD 3K_23919;296;3.5;3000;2144;Acrylic - Fagerhult - Delta Microprism;596;2144;3000;3000;44;52;119;White;Steel - Fagerhult - White;7320043530436;23919;18;18;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X600 STD 3K_23919-3;296;3.5;3000;2144;Acrylic - Fagerhult - Delta Microprism;596;2144;3000;3000;44;52;119;White;Steel - Fagerhult - White;7320043530443;23919-3;18;18;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X600 3K_23919-111;296;3.5;3000;2144;Acrylic - Fagerhult - Delta Microprism;596;2144;3000;3000;44;52;119;White;Steel - Fagerhult - White;7320047272165;23919-111;18;18;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X600 3K_23919-340;296;3.5;3000;2144;Acrylic - Fagerhult - Delta Microprism;596;2144;3000;3000;44;52;119;White;Steel - Fagerhult - White;7320047272202;23919-340;18;18;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X600 STD 3K_23919-402;296;3.5;3000;1929;Acrylic - Fagerhult - Delta Microprism;596;1929;3000;3000;44;52;121;White;Steel - Fagerhult - White;7320043530450;23919-402;17;17;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X600 3K_23919-519;296;3.5;3000;2144;Acrylic - Fagerhult - Delta Microprism;596;2144;3000;3000;44;52;119;White;Steel - Fagerhult - White;7320047266249;23919-519;18;18;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X600 3K_23919-520;296;3.5;3000;1929;Acrylic - Fagerhult - Delta Microprism;596;1929;3000;3000;44;52;121;White;Steel - Fagerhult - White;7320047266263;23919-520;17;17;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X600 3K_23919-528;296;3.5;3000;1929;Acrylic - Fagerhult - Delta Microprism;596;1929;3000;3000;44;52;121;White;Steel - Fagerhult - White;7320047272189;23919-528;17;17;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X600 3K_23919-529;296;3.5;3000;1929;Acrylic - Fagerhult - Delta Microprism;596;1929;3000;3000;44;52;121;White;Steel - Fagerhult - White;7320047272226;23919-529;17;17;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X600 STD 4K_23921;296;3.5;4000;2206;Acrylic - Fagerhult - Delta Microprism;596;2206;4000;4000;44;52;123;White;Steel - Fagerhult - White;7320043530368;23921;18;18;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X600 STD 4K_23921-3;296;3.5;4000;2206;Acrylic - Fagerhult - Delta Microprism;596;2206;4000;4000;44;52;123;White;Steel - Fagerhult - White;7320043530405;23921-3;18;18;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X600 4K_23921-111;296;3.5;4000;2206;Acrylic - Fagerhult - Delta Microprism;596;2206;4000;4000;44;52;123;White;Steel - Fagerhult - White;7320047266287;23921-111;18;18;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X600 4K_23921-340;296;3.5;4000;2206;Acrylic - Fagerhult - Delta Microprism;596;2206;4000;4000;44;52;123;White;Steel - Fagerhult - White;7320047266324;23921-340;18;18;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X600 STD 4K_23921-402;296;3.5;4000;1985;Acrylic - Fagerhult - Delta Microprism;596;1985;4000;4000;44;52;124;White;Steel - Fagerhult - White;7320043530412;23921-402;17;17;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X600 4K_23921-519;296;3.5;4000;2206;Acrylic - Fagerhult - Delta Microprism;596;2206;4000;4000;44;52;123;White;Steel - Fagerhult - White;7320047266362;23921-519;18;18;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X600 4K_23921-520;296;3.5;4000;1985;Acrylic - Fagerhult - Delta Microprism;596;1985;4000;4000;44;52;124;White;Steel - Fagerhult - White;7320047266386;23921-520;17;17;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X600 4K_23921-528;296;3.5;4000;1985;Acrylic - Fagerhult - Delta Microprism;596;1985;4000;4000;44;52;124;White;Steel - Fagerhult - White;7320047266300;23921-528;17;17;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB 300X600 4K_23921-529;296;3.5;4000;1985;Acrylic - Fagerhult - Delta Microprism;596;1985;4000;4000;44;52;124;White;Steel - Fagerhult - White;7320047266348;23921-529;17;17;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;0
MULTILUME FLAT DELTA VTB TW 300X1200_23994;296;5.8;4000;4566;Acrylic - Fagerhult - Delta Microprism;1196;4566;4000;4000;44;62;103;White;Steel - Fagerhult - White;7320047582417;23994;46;46;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA 600X600 TW VTB_23993;596;4.3;4000;4739;Acrylic - Fagerhult - Delta Microprism;596;4739;4000;4000;44;52;107;White;Steel - Fagerhult - White;7316911439000;23993;46;46;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA 600X600 TW VTB_23993-528;596;4.3;4000;4739;Acrylic - Fagerhult - Delta Microprism;596;4739;4000;4000;44;52;107;White;Steel - Fagerhult - White;7316911439024;23993-528;46;46;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA 600X600 TW VTB_23993-529;596;4.3;4000;4739;Acrylic - Fagerhult - Delta Microprism;596;4739;4000;4000;44;52;107;White;Steel - Fagerhult - White;7316911439048;23993-529;46;46;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA 600X600 TW VTB_23993-520;596;4.3;4000;4739;Acrylic - Fagerhult - Delta Microprism;596;4739;4000;4000;44;52;107;White;Steel - Fagerhult - White;7316911439062;23993-520;46;46;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 90;D;1;0
MULTILUME FLAT DELTA 600X600 840 OR VTB_23998-519;596;4.3;4000;4075;Acrylic - Fagerhult - Delta Microprism;596;4075;4000;4000;20;52;136;White;Steel - Fagerhult - White;7316911441980;23998-519;31.5;31.5;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;1
MULTILUME FLAT DELTA 600X600 840 OR VTB_23998-340;596;4.3;4000;4075;Acrylic - Fagerhult - Delta Microprism;596;4075;4000;4000;20;52;136;White;Steel - Fagerhult - White;7316911441973;23998-340;31.5;31.5;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;1
MULTILUME FLAT DELTA 600X600 840 OR VTB_23998-3;596;4.3;4000;4075;Acrylic - Fagerhult - Delta Microprism;596;4075;4000;4000;20;52;139;White;Steel - Fagerhult - White;7316911441966;23998-3;31;31;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;1
MULTILUME FLAT DELTA 600X600 840 OR VTB_23998-111;596;4.3;4000;4075;Acrylic - Fagerhult - Delta Microprism;596;4075;4000;4000;20;52;136;White;Steel - Fagerhult - White;7316911441959;23998-111;31.5;31.5;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;1
MULTILUME FLAT DELTA 600X600 830 OR VTB_23997-519;596;4.3;3000;3961;Acrylic - Fagerhult - Delta Microprism;596;3961;3000;3000;20;52;132;White;Steel - Fagerhult - White;7316911441942;23997-519;31.5;31.5;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;1
MULTILUME FLAT DELTA 600X600 830 OR VTB_23997-340;596;4.3;3000;3961;Acrylic - Fagerhult - Delta Microprism;596;3961;3000;3000;20;52;132;White;Steel - Fagerhult - White;7316911441881;23997-340;31.5;31.5;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;1
MULTILUME FLAT DELTA 600X600 830 OR VTB_23997-3;596;4.3;3000;3961;Acrylic - Fagerhult - Delta Microprism;596;3961;3000;3000;20;52;135;White;Steel - Fagerhult - White;7316911441874;23997-3;31;31;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;1
MULTILUME FLAT DELTA 600X600 830 OR VTB_23997-111;596;4.3;3000;3961;Acrylic - Fagerhult - Delta Microprism;596;3961;3000;3000;20;52;132;White;Steel - Fagerhult - White;7316911441867;23997-111;31.5;31.5;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;1
MULTILUME FLAT DELTA 600X600 830 OR VTB_23997;596;4.3;3000;3961;Acrylic - Fagerhult - Delta Microprism;596;3961;3000;3000;20;52;135;White;Steel - Fagerhult - White;7316911438805;23997;31;31;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;1
MULTILUME FLAT DELTA 600X600 840 OR VTB_23998;596;4.3;4000;4075;Acrylic - Fagerhult - Delta Microprism;596;4075;4000;4000;20;52;139;White;Steel - Fagerhult - White;7316911438904;23998;31;31;Multilume Flat Delta;Recessed mounting in ventilated or unventilated suspended ceilings.Two optional designs.<br><i>VTB</i> – for suspended ceilings with visible T-bars 15 or 24 mm. 300x300 also for fixed  suspended ceilings.</br><br><i>HB</i> – for suspended ceiling with concealed T-bars/D-edge, symmetrical attachment of ceiling boards (20–22 mm thick). Supplement with fixing brackets for fixed suspended ceiling, see Accessories.</br>;A recessed workplace luminaire in various sizes for most types of suspended ceilings. Delta louvres provide efficiency and optimal lighting comfort.;min. 80;C;1;1
