;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Tilt Angle##ANGLE##DEGREES;Temperature Color##OTHER##;Size##OTHER##;Shape##OTHER##;ServiceLifeDuration##OTHER##;ProductInformation##OTHER##;Photometric Web File##OTHER##;Optic##OTHER##;ModelReference##OTHER##;Material##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;LightFixturePlacingType##OTHER##;LightFixtureMountingType##OTHER##;Length##LENGTH##MILLIMETERS;Description##OTHER##;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP_Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;DiffuserMaterial##OTHER##;Control Gear##OTHER##;Color##OTHER##;Body##OTHER##;BarCode##OTHER##;BIMObjectName##OTHER##;ArticleNumber##OTHER##;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;ColorRenderingIndex##Other##
MULTILUME FLAT OPAL VTB 300X1200 3K CRI 90 4000LM_23718;300;5.0;90;3000;L 1200 mm + W 300 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23718.IES;<By Category>;Multilume Flat Opal;aluminium;3587;Fagerhult_Opal;Ceiling;Recessed ;1200;Luminaire body in white enamelled sheet steel (RAL 9016).;3587;3000;3000;44;116;100;<By Category>;Standard;White;Fagerhult_White_aluminium;7320046614898;Multilume Flat Opal;23718;36;930
MULTILUME FLAT OPAL VTB 300X1200 3K CRI 90 4000LM_23718-3;300;5.0;90;3000;L 1200 mm + W 300 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23718-3.IES;<By Category>;Multilume Flat Opal;aluminium;3587;Fagerhult_Opal;Ceiling;Recessed ;1200;Luminaire body in white enamelled sheet steel (RAL 9016).;3587;3000;3000;44;116;100;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7320046614904;Multilume Flat Opal;23718-3;36;930
MULTILUME FLAT OPAL VTB 300X1200 3K CRI 90 4000LM_23718-402;300;5.0;90;3000;L 1200 mm + W 300 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23718-402.IES;<By Category>;Multilume Flat Opal;aluminium;3587;Fagerhult_Opal;Ceiling;Recessed ;1200;Luminaire body in white enamelled sheet steel (RAL 9016).;3587;3000;3000;44;116;100;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046614911;Multilume Flat Opal;23718-402;36;930
MULTILUME FLAT OPAL VTB 300X1200 4K CRI 90 4200LM_23719;300;5.0;90;4000;L 1200 mm + W 300 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23719.IES;<By Category>;Multilume Flat Opal;aluminium;3857;Fagerhult_Opal;Ceiling;Recessed ;1200;Luminaire body in white enamelled sheet steel (RAL 9016).;3857;4000;4000;44;116;107;<By Category>;Standard;White;Fagerhult_White_aluminium;7320046592806;Multilume Flat Opal;23719;36;940
MULTILUME FLAT OPAL VTB 300X1200 4K CRI 90 4200LM_23719-3;300;5.0;90;4000;L 1200 mm + W 300 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23719-3.IES;<By Category>;Multilume Flat Opal;aluminium;3857;Fagerhult_Opal;Ceiling;Recessed ;1200;Luminaire body in white enamelled sheet steel (RAL 9016).;3857;4000;4000;44;116;107;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7320046592820;Multilume Flat Opal;23719-3;36;940
MULTILUME FLAT OPAL VTB 300X1200 4K CRI 90 4200LM_23719-402;300;5.0;90;4000;L 1200 mm + W 300 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23719-402.IES;<By Category>;Multilume Flat Opal;aluminium;3857;Fagerhult_Opal;Ceiling;Recessed ;1200;Luminaire body in white enamelled sheet steel (RAL 9016).;3857;4000;4000;44;116;107;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046592844;Multilume Flat Opal;23719-402;36;940
MULTILUME FLAT OPAL VTB 600X600 3K 4KLM CRI90_23781;600;4.5;90;3000;L 600 mm + W 600 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23781.IES;<By Category>;Multilume Flat Opal;aluminium;3707;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;3707;3000;3000;44;116;103;<By Category>;Standard;White;Fagerhult_White_aluminium;7320043448281;Multilume Flat Opal;23781;36;930
MULTILUME FLAT OPAL VTB 600X600 3K 4KLM CRI90_23781-3;600;4.5;90;3000;L 600 mm + W 600 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23781-3.IES;<By Category>;Multilume Flat Opal;aluminium;3707;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;3707;3000;3000;44;116;103;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7320043448298;Multilume Flat Opal;23781-3;36;930
MULTILUME FLAT OPAL VTB 600X600 3K 4KLM CRI90_23781-402;600;4.5;90;3000;L 600 mm + W 600 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23781-402.IES;<By Category>;Multilume Flat Opal;aluminium;3707;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;3707;3000;3000;44;116;103;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320043448304;Multilume Flat Opal;23781-402;36;930
MULTILUME FLAT OPAL VTB 600X600 4K 4,5KLM CRI90_23782;600;4.5;90;4000;L 600 mm + W 600 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23782.IES;<By Category>;Multilume Flat Opal;aluminium;3906;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;3906;4000;4000;44;116;111;<By Category>;Standard;White;Fagerhult_White_aluminium;7320043448311;Multilume Flat Opal;23782;36;940
MULTILUME FLAT OPAL VTB 600X600 4K 4,5KLM CRI90_23782-3;600;4.5;90;4000;L 600 mm + W 600 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23782-3.IES;<By Category>;Multilume Flat Opal;aluminium;3906;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;3906;4000;4000;44;116;111;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7320043448328;Multilume Flat Opal;23782-3;36;940
MULTILUME FLAT OPAL VTB 600X600 4K 4,5KLM CRI90_23782-402;600;4.5;90;4000;L 600 mm + W 600 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23782-402.IES;<By Category>;Multilume Flat Opal;aluminium;3906;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;3906;4000;4000;44;116;111;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320043448335;Multilume Flat Opal;23782-402;36;940
MULTILUME FLAT OPAL VTB 600X600 3K 3KLM_23785;600;4.5;90;3000;L 600 mm + W 600 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23785.IES;<By Category>;Multilume Flat Opal;aluminium;3054;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;3054;3000;3000;44;116;127;<By Category>;Standard;White;Fagerhult_White_aluminium;7320043343418;Multilume Flat Opal;23785;24;830
MULTILUME FLAT OPAL VTB 600X600 3K 3KLM_23785-3;600;4.5;90;3000;L 600 mm + W 600 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23785-3.IES;<By Category>;Multilume Flat Opal;aluminium;3054;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;3054;3000;3000;44;116;127;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7320043343425;Multilume Flat Opal;23785-3;24;830
MULTILUME FLAT OPAL VTB 600X600 3K 3KLM_23785-402;600;4.5;90;3000;L 600 mm + W 600 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23785-402.IES;<By Category>;Multilume Flat Opal;aluminium;3054;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;3054;3000;3000;44;116;127;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320043343449;Multilume Flat Opal;23785-402;24;830
MULTILUME FLAT HB OPAL 600X600 3K 3KLM_23787;600;4.5;90;3000;L 600 mm + W 600 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23787.IES;<By Category>;Multilume Flat Opal;aluminium;3054;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;3054;3000;3000;44;116;127;<By Category>;Standard;White;Fagerhult_White_aluminium;7320043343494;Multilume Flat Opal;23787;24;830
MULTILUME FLAT HB OPAL 600X600 3K 3KLM_23787-3;600;4.5;90;3000;L 600 mm + W 600 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23787-3.IES;<By Category>;Multilume Flat Opal;aluminium;3054;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;3054;3000;3000;44;116;127;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7320043343500;Multilume Flat Opal;23787-3;24;830
MULTILUME FLAT HB OPAL 600X600 3K 3KLM_23787-402;600;4.5;90;3000;L 600 mm + W 600 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23787-402.IES;<By Category>;Multilume Flat Opal;aluminium;3054;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;3054;3000;3000;44;116;127;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320043343555;Multilume Flat Opal;23787-402;24;830
MULTILUME FLAT OPAL VTB 600X600 4K 3KLM_23789;600;4.5;90;4000;L 600 mm + W 600 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23789.IES;<By Category>;Multilume Flat Opal;aluminium;3215;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;3215;4000;4000;44;116;134;<By Category>;Standard;White;Fagerhult_White_aluminium;7320043343593;Multilume Flat Opal;23789;24;840
MULTILUME FLAT OPAL VTB 600X600 4K 3KLM_23789-3;600;4.5;90;4000;L 600 mm + W 600 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23789-3.IES;<By Category>;Multilume Flat Opal;aluminium;3215;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;3215;4000;4000;44;116;134;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7320043343616;Multilume Flat Opal;23789-3;24;840
MULTILUME FLAT OPAL VTB 600X600 4K 3KLM_23789-402;600;4.5;90;4000;L 600 mm + W 600 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23789-402.IES;<By Category>;Multilume Flat Opal;aluminium;3215;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;3215;4000;4000;44;116;134;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320043343623;Multilume Flat Opal;23789-402;24;840
MULTILUME FLAT HB OPAL 600X600 4K 3KLM_23791;600;4.5;90;4000;L 600 mm + W 600 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23791.IES;<By Category>;Multilume Flat Opal;aluminium;3215;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;3215;4000;4000;44;116;134;<By Category>;Standard;White;Fagerhult_White_aluminium;7320043343814;Multilume Flat Opal;23791;24;840
MULTILUME FLAT HB OPAL 600X600 4K 3KLM_23791-3;600;4.5;90;4000;L 600 mm + W 600 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23791-3.IES;<By Category>;Multilume Flat Opal;aluminium;3215;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;3215;4000;4000;44;116;134;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7320043343838;Multilume Flat Opal;23791-3;24;840
MULTILUME FLAT OPAL 600X600 HB 4K LM_23791-402;600;4.5;90;4000;L 600 mm + W 600 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23791-402.IES;<By Category>;Multilume Flat Opal;aluminium;3215;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;3215;4000;4000;44;116;134;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320043343845;Multilume Flat Opal;23791-402;24;840
MULTILUME FLAT OPAL VTB 600X600 3K 4KLM_23805;600;4.5;90;3000;L 600 mm + W 600 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23805.IES;<By Category>;Multilume Flat Opal;aluminium;4618;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;4618;3000;3000;44;116;128;<By Category>;Standard;White;Fagerhult_White_aluminium;7320043326169;Multilume Flat Opal;23805;36;830
MULTILUME FLAT OPAL VTB 600X600 3K 4KLM_23805-3;600;4.5;90;3000;L 600 mm + W 600 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23805-3.IES;<By Category>;Multilume Flat Opal;aluminium;4618;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;4618;3000;3000;44;116;128;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7320043326176;Multilume Flat Opal;23805-3;36;830
MULTILUME FLAT OPAL VTB 600X600 3K 4KLM_23805-402;600;4.5;90;3000;L 600 mm + W 600 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23805-402.IES;<By Category>;Multilume Flat Opal;aluminium;4618;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;4618;3000;3000;44;116;128;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320043326190;Multilume Flat Opal;23805-402;36;830
MULTILUME FLAT HB OPAL 600X600 3K 4,5KLM_23807;600;4.5;90;3000;L 600 mm + W 600 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23807.IES;<By Category>;Multilume Flat Opal;aluminium;4658;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;4658;3000;3000;44;116;129;<By Category>;Standard;White;Fagerhult_White_aluminium;7320043326244;Multilume Flat Opal;23807;36;830
MULTILUME FLAT HB OPAL 600X600 3K 4,5KLM_23807-3;600;4.5;90;3000;L 600 mm + W 600 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23807-3.IES;<By Category>;Multilume Flat Opal;aluminium;4658;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;4658;3000;3000;44;116;129;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7320043326251;Multilume Flat Opal;23807-3;36;830
MULTILUME FLAT HB OPAL 600X600 3K 4,5KLM_23807-402;600;4.5;90;3000;L 600 mm + W 600 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23807-402.IES;<By Category>;Multilume Flat Opal;aluminium;4658;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;4658;3000;3000;44;116;129;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320043326268;Multilume Flat Opal;23807-402;36;830
MULTILUME FLAT OPAL VTB 600X600 4K 4,5KLM_23809;600;4.5;90;4000;L 600 mm + W 600 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23809.IES;<By Category>;Multilume Flat Opal;aluminium;4861;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;4861;4000;4000;44;116;135;<By Category>;Standard;White;Fagerhult_White_aluminium;7320043326329;Multilume Flat Opal;23809;36;840
MULTILUME FLAT OPAL VTB 600X600 4K 4,5KLM_23809-3;600;4.5;90;4000;L 600 mm + W 600 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23809-3.IES;<By Category>;Multilume Flat Opal;aluminium;4861;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;4861;4000;4000;44;116;135;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7320043326336;Multilume Flat Opal;23809-3;36;840
MULTILUME FLAT OPAL VTB 600X600 4K 4,5KLM_23809-402;600;4.5;90;4000;L 600 mm + W 600 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23809-402.IES;<By Category>;Multilume Flat Opal;aluminium;4861;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;4861;4000;4000;44;116;135;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320043326343;Multilume Flat Opal;23809-402;36;840
MULTILUME FLAT HB OPAL 600X600 4K 4,5KLM_23811;600;4.5;90;4000;L 600 mm + W 600 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23811.IES;<By Category>;Multilume Flat Opal;aluminium;4861;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;4861;4000;4000;44;116;135;<By Category>;Standard;White;Fagerhult_White_aluminium;7320043326381;Multilume Flat Opal;23811;36;840
MULTILUME FLAT HB OPAL 600X600 4K 4,5KLM_23811-3;600;4.5;90;4000;L 600 mm + W 600 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23811-3.IES;<By Category>;Multilume Flat Opal;aluminium;4861;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;4861;4000;4000;44;116;135;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7320043326398;Multilume Flat Opal;23811-3;36;840
MULTILUME FLAT HB OPAL 600X600 4K 4,5KLM_23811-402;600;4.5;90;4000;L 600 mm + W 600 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23811-402.IES;<By Category>;Multilume Flat Opal;aluminium;4861;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;4861;4000;4000;44;116;135;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320043326404;Multilume Flat Opal;23811-402;36;840
MULTILUME FLAT OPAL VTB 300X300 3K_23836;300;2.0;90;3000;L 300 mm + W 300 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23836.IES;<By Category>;Multilume Flat Opal;aluminium;1058;Fagerhult_Opal;Ceiling;Recessed ;300;Luminaire body in white enamelled sheet steel (RAL 9016).;1058;3000;3000;44;116;118;<By Category>;Standard;White;Fagerhult_White_aluminium;7320046367770;Multilume Flat Opal;23836;9;830
MULTILUME FLAT OPAL VTB 300X300 3K_23836-3;300;2.0;90;3000;L 300 mm + W 300 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23836-3.IES;<By Category>;Multilume Flat Opal;aluminium;1058;Fagerhult_Opal;Ceiling;Recessed ;300;Luminaire body in white enamelled sheet steel (RAL 9016).;1058;3000;3000;44;116;118;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7320046367800;Multilume Flat Opal;23836-3;9;830
MULTILUME FLAT OPAL VTB 300X300 3K_23836-402;300;2.0;90;3000;L 300 mm + W 300 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23836-402.IES;<By Category>;Multilume Flat Opal;aluminium;1058;Fagerhult_Opal;Ceiling;Recessed ;300;Luminaire body in white enamelled sheet steel (RAL 9016).;1058;3000;3000;44;116;118;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046367817;Multilume Flat Opal;23836-402;9;830
MULTILUME FLAT OPAL VTB 300X300 4K_23838;300;2.0;90;4000;L 300 mm + W 300 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23838.IES;<By Category>;Multilume Flat Opal;aluminium;1111;Fagerhult_Opal;Ceiling;Recessed ;300;Luminaire body in white enamelled sheet steel (RAL 9016).;1111;4000;4000;44;116;123;<By Category>;Standard;White;Fagerhult_White_aluminium;7320046367855;Multilume Flat Opal;23838;9;840
MULTILUME FLAT OPAL VTB 300X300 4K_23838-3;300;2.0;90;4000;L 300 mm + W 300 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23838-3.IES;<By Category>;Multilume Flat Opal;aluminium;1111;Fagerhult_Opal;Ceiling;Recessed ;300;Luminaire body in white enamelled sheet steel (RAL 9016).;1111;4000;4000;44;116;123;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7320046367862;Multilume Flat Opal;23838-3;9;840
MULTILUME FLAT OPAL VTB 300X300 4K_23838-402;300;2.0;90;4000;L 300 mm + W 300 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23838-402.IES;<By Category>;Multilume Flat Opal;aluminium;1111;Fagerhult_Opal;Ceiling;Recessed ;300;Luminaire body in white enamelled sheet steel (RAL 9016).;1111;4000;4000;44;116;123;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320046367879;Multilume Flat Opal;23838-402;9;840
MULTILUME FLAT OPAL VTB 600X600 3K 4KLM_23867;600;4.5;90;3000;L 600 mm + W 600 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23867.IES;<By Category>;Multilume Flat Opal;aluminium;4032;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;4032;3000;3000;44;116;130;<By Category>;Standard;White;Fagerhult_White_aluminium;7320043382363;Multilume Flat Opal;23867;31;830
MULTILUME FLAT OPAL VTB 600X600 3K 4KLM_23867-3;600;4.5;90;3000;L 600 mm + W 600 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23867-3.IES;<By Category>;Multilume Flat Opal;aluminium;4032;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;4032;3000;3000;44;116;130;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7320043382370;Multilume Flat Opal;23867-3;31;830
MULTILUME FLAT OPAL VTB 600X600 3K 4KLM_23867-402;600;4.5;90;3000;L 600 mm + W 600 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23867-402.IES;<By Category>;Multilume Flat Opal;aluminium;4032;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;4032;3000;3000;44;116;130;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320043382561;Multilume Flat Opal;23867-402;31;830
MULTILUME FLAT HB OPAL 600X600 3K 4KLM_23869;600;4.5;90;3000;L 600 mm + W 600 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23869.IES;<By Category>;Multilume Flat Opal;aluminium;4042;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;4042;3000;3000;44;116;130;<By Category>;Standard;White;Fagerhult_White_aluminium;7320043382790;Multilume Flat Opal;23869;31;830
MULTILUME FLAT HB OPAL 600X600 3K 4KLM_23869-3;600;4.5;90;3000;L 600 mm + W 600 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23869-3.IES;<By Category>;Multilume Flat Opal;aluminium;4042;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;4042;3000;3000;44;116;130;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7320043382806;Multilume Flat Opal;23869-3;31;830
MULTILUME FLAT HB OPAL 600X600 3K 4KLM_23869-402;600;4.5;90;3000;L 600 mm + W 600 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23869-402.IES;<By Category>;Multilume Flat Opal;aluminium;4042;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;4042;3000;3000;44;116;130;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320043382813;Multilume Flat Opal;23869-402;31;830
MULTILUME FLAT OPAL VTB 600X600 4K 4KLM_23871;600;4.5;90;4000;L 600 mm + W 600 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23871.IES;<By Category>;Multilume Flat Opal;aluminium;4244;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;4244;4000;4000;44;116;137;<By Category>;Standard;White;Fagerhult_White_aluminium;7320043382882;Multilume Flat Opal;23871;31;840
MULTILUME FLAT OPAL VTB 600X600 4K 4KLM_23871-3;600;4.5;90;4000;L 600 mm + W 600 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23871-3.IES;<By Category>;Multilume Flat Opal;aluminium;4244;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;4244;4000;4000;44;116;137;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7320043382899;Multilume Flat Opal;23871-3;31;840
MULTILUME FLAT OPAL VTB 600X600 4K 4KLM_23871-402;600;4.5;90;4000;L 600 mm + W 600 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23871-402.IES;<By Category>;Multilume Flat Opal;aluminium;4244;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;4244;4000;4000;44;116;137;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320043382905;Multilume Flat Opal;23871-402;31;840
MULTILUME FLAT HB OPAL 600X600 4K 4KLM_23873;600;4.5;90;4000;L 600 mm + W 600 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23873.IES;<By Category>;Multilume Flat Opal;aluminium;4244;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;4244;4000;4000;44;116;137;<By Category>;Standard;White;Fagerhult_White_aluminium;7320043383155;Multilume Flat Opal;23873;31;840
MULTILUME FLAT HB OPAL 600X600 4K 4KLM_23873-3;600;4.5;90;4000;L 600 mm + W 600 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23873-3.IES;<By Category>;Multilume Flat Opal;aluminium;4244;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;4244;4000;4000;44;116;137;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7320043383162;Multilume Flat Opal;23873-3;31;840
MULTILUME FLAT HB OPAL 600X600 4K 4KLM_23873-402;600;4.5;90;4000;L 600 mm + W 600 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23873-402.IES;<By Category>;Multilume Flat Opal;aluminium;4244;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;4244;4000;4000;44;116;137;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320043383179;Multilume Flat Opal;23873-402;31;840
MULTILUME FLAT OPAL VTB 300X1200 3K 3KLM_23905;300;5.0;90;3000;L 1200 mm + W 300 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23905.IES;<By Category>;Multilume Flat Opal;aluminium;2914;Fagerhult_Opal;Ceiling;Recessed ;1200;Luminaire body in white enamelled sheet steel (RAL 9016).;2914;3000;3000;44;116;121;<By Category>;Standard;White;Fagerhult_White_aluminium;7320043467626;Multilume Flat Opal;23905;24;830
MULTILUME FLAT OPAL VTB 300X1200 3K 3KLM_23905-3;300;5.0;90;3000;L 1200 mm + W 300 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23905-3.IES;<By Category>;Multilume Flat Opal;aluminium;2914;Fagerhult_Opal;Ceiling;Recessed ;1200;Luminaire body in white enamelled sheet steel (RAL 9016).;2914;3000;3000;44;116;121;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7320043467633;Multilume Flat Opal;23905-3;24;830
MULTILUME FLAT OPAL VTB 300X1200 3K 3KLM_23905-402;300;5.0;90;3000;L 1200 mm + W 300 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23905-402.IES;<By Category>;Multilume Flat Opal;aluminium;2914;Fagerhult_Opal;Ceiling;Recessed ;1200;Luminaire body in white enamelled sheet steel (RAL 9016).;2914;3000;3000;44;116;121;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320043467640;Multilume Flat Opal;23905-402;24;830
MULTILUME FLAT OPAL VTB 300X1200 4K 3KLM_23906;300;5.0;90;4000;L 1200 mm + W 300 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23906.IES;<By Category>;Multilume Flat Opal;aluminium;3068;Fagerhult_Opal;Ceiling;Recessed ;1200;Luminaire body in white enamelled sheet steel (RAL 9016).;3068;4000;4000;44;116;128;<By Category>;Standard;White;Fagerhult_White_aluminium;7320043467664;Multilume Flat Opal;23906;24;840
MULTILUME FLAT OPAL VTB 300X1200 4K 3KLM_23906-3;300;5.0;90;4000;L 1200 mm + W 300 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23906-3.IES;<By Category>;Multilume Flat Opal;aluminium;3068;Fagerhult_Opal;Ceiling;Recessed ;1200;Luminaire body in white enamelled sheet steel (RAL 9016).;3068;4000;4000;44;116;128;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7320043467671;Multilume Flat Opal;23906-3;24;840
MULTILUME FLAT OPAL VTB 300X1200 4K 3KLM_23906-402;300;5.0;90;4000;L 1200 mm + W 300 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23906-402.IES;<By Category>;Multilume Flat Opal;aluminium;3068;Fagerhult_Opal;Ceiling;Recessed ;1200;Luminaire body in white enamelled sheet steel (RAL 9016).;3068;4000;4000;44;116;128;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320043467688;Multilume Flat Opal;23906-402;24;840
MULTILUME FLAT OPAL VTB 300X1200 3K 4KLM_23907;300;5.0;90;3000;L 1200 mm + W 300 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23907.IES;<By Category>;Multilume Flat Opal;aluminium;3885;Fagerhult_Opal;Ceiling;Recessed ;1200;Luminaire body in white enamelled sheet steel (RAL 9016).;3885;3000;3000;44;116;125;<By Category>;Standard;White;Fagerhult_White_aluminium;7320043467695;Multilume Flat Opal;23907;31;830
MULTILUME FLAT OPAL VTB 300X1200 3K 4KLM_23907-3;300;5.0;90;3000;L 1200 mm + W 300 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23907-3.IES;<By Category>;Multilume Flat Opal;aluminium;3885;Fagerhult_Opal;Ceiling;Recessed ;1200;Luminaire body in white enamelled sheet steel (RAL 9016).;3885;3000;3000;44;116;125;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7320043467718;Multilume Flat Opal;23907-3;31;830
MULTILUME FLAT OPAL VTB 300X1200 3K 4KLM_23907-402;300;5.0;90;3000;L 1200 mm + W 300 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23907-402.IES;<By Category>;Multilume Flat Opal;aluminium;3885;Fagerhult_Opal;Ceiling;Recessed ;1200;Luminaire body in white enamelled sheet steel (RAL 9016).;3885;3000;3000;44;116;125;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320043467725;Multilume Flat Opal;23907-402;31;830
MULTILUME FLAT OPAL VTB 300X1200 4K 4KLM_23908;300;5.0;90;4000;L 1200 mm + W 300 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23908.IES;<By Category>;Multilume Flat Opal;aluminium;4090;Fagerhult_Opal;Ceiling;Recessed ;1200;Luminaire body in white enamelled sheet steel (RAL 9016).;4090;4000;4000;44;116;132;<By Category>;Standard;White;Fagerhult_White_aluminium;7320043467732;Multilume Flat Opal;23908;31;840
MULTILUME FLAT OPAL VTB 300X1200 4K 4KLM_23908-3;300;5.0;90;4000;L 1200 mm + W 300 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23908-3.IES;<By Category>;Multilume Flat Opal;aluminium;4090;Fagerhult_Opal;Ceiling;Recessed ;1200;Luminaire body in white enamelled sheet steel (RAL 9016).;4090;4000;4000;44;116;132;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7320043467749;Multilume Flat Opal;23908-3;31;840
MULTILUME FLAT OPAL VTB 300X1200 4K 4KLM_23908-402;300;5.0;90;4000;L 1200 mm + W 300 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23908-402.IES;<By Category>;Multilume Flat Opal;aluminium;4090;Fagerhult_Opal;Ceiling;Recessed ;1200;Luminaire body in white enamelled sheet steel (RAL 9016).;4090;4000;4000;44;116;132;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320043467756;Multilume Flat Opal;23908-402;31;840
MULTILUME FLAT OPAL VTB 300X1200 3K 4,5KLM_23909;300;5.0;90;3000;L 1200 mm + W 300 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23909.IES;<By Category>;Multilume Flat Opal;aluminium;4468;Fagerhult_Opal;Ceiling;Recessed ;1200;Luminaire body in white enamelled sheet steel (RAL 9016).;4468;3000;3000;44;116;124;<By Category>;Standard;White;Fagerhult_White_aluminium;7320043467763;Multilume Flat Opal;23909;36;830
MULTILUME FLAT OPAL VTB 300X1200 3K 4,5KLM_23909-3;300;5.0;90;3000;L 1200 mm + W 300 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23909-3.IES;<By Category>;Multilume Flat Opal;aluminium;4468;Fagerhult_Opal;Ceiling;Recessed ;1200;Luminaire body in white enamelled sheet steel (RAL 9016).;4468;3000;3000;44;116;124;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7320043467770;Multilume Flat Opal;23909-3;36;830
MULTILUME FLAT OPAL VTB 300X1200 3K 4,5KLM_23909-402;300;5.0;90;3000;L 1200 mm + W 300 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23909-402.IES;<By Category>;Multilume Flat Opal;aluminium;4468;Fagerhult_Opal;Ceiling;Recessed ;1200;Luminaire body in white enamelled sheet steel (RAL 9016).;4468;3000;3000;44;116;124;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320043467787;Multilume Flat Opal;23909-402;36;830
MULTILUME FLAT OPAL VTB 300X1200 4K 4,5KLM_23910;300;5.0;90;4000;L 1200 mm + W 300 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23910.IES;<By Category>;Multilume Flat Opal;aluminium;4704;Fagerhult_Opal;Ceiling;Recessed ;1200;Luminaire body in white enamelled sheet steel (RAL 9016).;4704;4000;4000;44;116;131;<By Category>;Standard;White;Fagerhult_White_aluminium;7320043467800;Multilume Flat Opal;23910;36;840
MULTILUME FLAT OPAL VTB 300X1200 4K 4,5KLM_23910-3;300;5.0;90;4000;L 1200 mm + W 300 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23910-3.IES;<By Category>;Multilume Flat Opal;aluminium;4704;Fagerhult_Opal;Ceiling;Recessed ;1200;Luminaire body in white enamelled sheet steel (RAL 9016).;4704;4000;4000;44;116;131;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7320043467817;Multilume Flat Opal;23910-3;36;840
MULTILUME FLAT OPAL VTB 300X1200 4K 4,5KLM_23910-402;300;5.0;90;4000;L 1200 mm + W 300 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23910-402.IES;<By Category>;Multilume Flat Opal;aluminium;4704;Fagerhult_Opal;Ceiling;Recessed ;1200;Luminaire body in white enamelled sheet steel (RAL 9016).;4704;4000;4000;44;116;131;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320043467848;Multilume Flat Opal;23910-402;36;840
MULTILUME FLAT OPAL VTB 300X600 STD 3K_23918;300;2.5;90;3000;L 600 mm + W 300 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23918.IES;<By Category>;Multilume Flat Opal;aluminium;2176;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;2176;3000;3000;44;116;114;<By Category>;Standard;White;Fagerhult_White_aluminium;7320043530467;Multilume Flat Opal;23918;19;830
MULTILUME FLAT OPAL VTB 300X600 STD 3K_23918-3;300;2.5;90;3000;L 600 mm + W 300 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23918-3.IES;<By Category>;Multilume Flat Opal;aluminium;2176;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;2176;3000;3000;44;116;114;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7320043530474;Multilume Flat Opal;23918-3;19;830
MULTILUME FLAT OPAL VTB 300X600 STD 3K_23918-402;300;2.5;90;3000;L 600 mm + W 300 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23918-402.IES;<By Category>;Multilume Flat Opal;aluminium;2176;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;2176;3000;3000;44;116;114;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320043530481;Multilume Flat Opal;23918-402;19;830
MULTILUME FLAT OPAL VTB 300X600 STD 4K_23920;300;2.5;90;4000;L 600 mm + W 300 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23920.IES;<By Category>;Multilume Flat Opal;aluminium;2285;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;2285;4000;4000;44;116;120;<By Category>;Standard;White;Fagerhult_White_aluminium;7320043530498;Multilume Flat Opal;23920;19;840
MULTILUME FLAT OPAL VTB 300X600 STD 4K_23920-3;300;2.5;90;4000;L 600 mm + W 300 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23920-3.IES;<By Category>;Multilume Flat Opal;aluminium;2285;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;2285;4000;4000;44;116;120;<By Category>;ConnectionCableWithPlug;White;Fagerhult_White_aluminium;7320043530504;Multilume Flat Opal;23920-3;19;840
MULTILUME FLAT OPAL VTB 300X600 STD 4K_23920-402;300;2.5;90;4000;L 600 mm + W 300 mm + H 83 mm;Rectangle;100 000/10 %;A recessed general luminaire in various sizes for most types of suspended ceilings. Opal louvres that follow the ceiling surface provide a stylish and discrete feel.;23920-402.IES;<By Category>;Multilume Flat Opal;aluminium;2285;Fagerhult_Opal;Ceiling;Recessed ;600;Luminaire body in white enamelled sheet steel (RAL 9016).;2285;4000;4000;44;116;120;<By Category>;DALIPhasePulseControl;White;Fagerhult_White_aluminium;7320043530511;Multilume Flat Opal;23920-402;19;840
