;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Type##OTHER##
NOTOR 36 L LEFT CEIL D DALI HL OPAL 840_16086-20359;563;1.4;4000;2566;Acrylic - Fagerhult - Opal;563;2566;4000;4000;20;36;118;White;Aluminium - Fagerhult - White;7320049576582;16086-20359;23;23;Notor 36 ceiling Opal;Keyhole slots permit individual or system surface-mounted installation.;"Luminaire with Opal louvre for surface-mounted installation, individually or in a system. 
Choose between linear modules and shapes X, T, L, ceiling-to-wall and spotlight modules to freely create the system that best suits your project.";min. 80;C;1;1
NOTOR 36 L RIGHT CEIL D DALI HL OPAL 840_16086-20360;563;1.4;4000;2566;Acrylic - Fagerhult - Opal;563;2566;4000;4000;20;36;118;White;Aluminium - Fagerhult - White;7320049576612;16086-20360;23;23;Notor 36 ceiling Opal;Keyhole slots permit individual or system surface-mounted installation.;"Luminaire with Opal louvre for surface-mounted installation, individually or in a system. 
Choose between linear modules and shapes X, T, L, ceiling-to-wall and spotlight modules to freely create the system that best suits your project.";min. 80;C;1;2
