,Type Comments##OTHER##,MaterialBody##OTHER##,MaterialLouvre##OTHER##,MaterialAccentBody##OTHER##,MaterialReflector##OTHER##,Weight_Kg##OTHER##,URL##OTHER##,Total Light Loss Factor##OTHER##,SuffixCode##OTHER##,Photometric Web File##OTHER##,Model##OTHER##,Manufacturer##OTHER##,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,LightSource##OTHER##,Light Loss Factor##OTHER##,Lamp##OTHER##,Keynote##OTHER##,Initial Intensity##OTHER##,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Initial Color##OTHER##,FagerhultPartNumber##OTHER##,Emit from Rectangle Width##LENGTH##MILLIMETERS,Emit from Rectangle Length##LENGTH##MILLIMETERS,COBieBarCode##OTHER##,Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,Description##OTHER##,Assembly Code##OTHER##,LOR##OTHER##,Wattage##ELECTRICAL_WATTAGE##WATTS,TotalLength##LENGTH##MILLIMETERS,TotalWidth##LENGTH##MILLIMETERS,Height##LENGTH##MILLIMETERS,NumberOfLamps##OTHER##,Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT
RECESSO 600X600 3K 2C BETA OPTI LUMEN SWITCH_25786,RECESSO 600X600 3K 2C BETA OPTI LUMEN SWITCH-,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.0,http://www.fagerhult.com,1,Standard,25786.IES,Recesso Beta Opti,Fagerhult,2940.0,LED,1,26,V59,2940.0,3000,3000,25786,200,558,7320046217976,26,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,26,597,597,71,1,113.0769231
RECESSO 600X600 3K 2C BETA OPTI LUMEN SWITCH_25786-111,RECESSO 600X600 3K 2C BETA OPTI LUMEN SWITCH-BODY W WIELAND CONNECTOR GST18I3 MALE.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.0,http://www.fagerhult.com,1,Standard,25786.IES,Recesso Beta Opti,Fagerhult,2940.0,LED,1,26,V59,2940.0,3000,3000,25786-111,200,558,7320046217990,26,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,26,597,597,71,1,113.0769231
RECESSO 600X600 3K 2C BETA OPTI LUMEN SWITCH_25786-3,"RECESSO 600X600 3K 2C BETA OPTI LUMEN SWITCH-BODY W CONNECTION CABLE L=2,5M FREE CABLE W PLUG.",Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.0,http://www.fagerhult.com,1,Standard,25786.IES,Recesso Beta Opti,Fagerhult,2940.0,LED,1,26,V59,2940.0,3000,3000,25786-3,200,558,7320046218010,26,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,26,597,597,71,1,113.0769231
RECESSO 600X600 3K 2C BETA OPTI LUMEN SWITCH_25786-340,RECESSO 600X600 3K 2C BETA OPTI LUMEN SWITCH-Body w Winsta connector 3-pole.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.0,http://www.fagerhult.com,1,Standard - WAGO Winsta,25786.IES,Recesso Beta Opti,Fagerhult,2940.0,LED,1,26,V59,2940.0,3000,3000,25786-340,200,558,7320046218034,26,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,26,597,597,71,1,113.0769231
RECESSO 600X600 3K 2C BETA OPTI LUMEN SWITCH_25786-402,RECESSO 600X600 3K 2C BETA OPTI LUMEN SWITCH-LED dim DALI/Phase-pulse control.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.0,http://www.fagerhult.com,1,DALI/Phase-pulse control,25786.IES,Recesso Beta Opti,Fagerhult,2940.0,LED,1,26,V59,2940.0,3000,3000,25786-402,200,558,7320046218058,26,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,26,597,597,71,1,113.0769231
RECESSO 600X600 3K 2C BETA OPTI LUMEN SWITCH_25786-454,RECESSO 600X600 3K 2C BETA OPTI LUMEN SWITCH-LED body w DALI driver and Winsta connector 5-pole. Blue male for dim.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.0,http://www.fagerhult.com,1,DALI - WAGO Winsta,25786.IES,Recesso Beta Opti,Fagerhult,2940.0,LED,1,26,V59,2940.0,3000,3000,25786-454,200,558,7320046218072,26,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,26,597,597,71,1,113.0769231
RECESSO 600X600 3K 2C BETA OPTI LUMEN SWITCH_25786-456,RECESSO 600X600 3K 2C BETA OPTI LUMEN SWITCH-LED body w DALI driver and Wieland connector 5-pole. Blue male for dim.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.0,http://www.fagerhult.com,1,DALI - Wieland,25786.IES,Recesso Beta Opti,Fagerhult,2940.0,LED,1,26,V59,2940.0,3000,3000,25786-456,200,558,7320046218096,26,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,26,597,597,71,1,113.0769231
RECESSO 600X600 4K 2C BETA OPTI LUMEN SWITCH_25788,RECESSO 600X600 4K 2C BETA OPTI LUMEN SWITCH-,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.0,http://www.fagerhult.com,1,Standard,25788.IES,Recesso Beta Opti,Fagerhult,3001.0,LED,1,26,V59,3001.0,4000,4000,25788,200,558,7320046218119,26,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,26,597,597,71,1,115.4230769
RECESSO 600X600 4K 2C BETA OPTI LUMEN SWITCH_25788-111,RECESSO 600X600 4K 2C BETA OPTI LUMEN SWITCH-BODY W WIELAND CONNECTOR GST18I3 MALE.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.0,http://www.fagerhult.com,1,Standard,25788.IES,Recesso Beta Opti,Fagerhult,3001.0,LED,1,26,V59,3001.0,4000,4000,25788-111,200,558,7320046218133,26,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,26,597,597,71,1,115.4230769
RECESSO 600X600 4K 2C BETA OPTI LUMEN SWITCH_25788-3,"RECESSO 600X600 4K 2C BETA OPTI LUMEN SWITCH-BODY W CONNECTION CABLE L=2,5M FREE CABLE W PLUG.",Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.0,http://www.fagerhult.com,1,Standard,25788.IES,Recesso Beta Opti,Fagerhult,3001.0,LED,1,26,V59,3001.0,4000,4000,25788-3,200,558,7320046218157,26,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,26,597,597,71,1,115.4230769
RECESSO 600X600 4K 2C BETA OPTI LUMEN SWITCH_25788-340,RECESSO 600X600 4K 2C BETA OPTI LUMEN SWITCH-Body w Winsta connector 3-pole.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.0,http://www.fagerhult.com,1,Standard - WAGO Winsta,25788.IES,Recesso Beta Opti,Fagerhult,3001.0,LED,1,26,V59,3001.0,4000,4000,25788-340,200,558,7320046218171,26,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,26,597,597,71,1,115.4230769
RECESSO 600X600 4K 2C BETA OPTI LUMEN SWITCH_25788-402,RECESSO 600X600 4K 2C BETA OPTI LUMEN SWITCH-LED dim DALI/Phase-pulse control.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.0,http://www.fagerhult.com,1,DALI/Phase-pulse control,25788.IES,Recesso Beta Opti,Fagerhult,3001.0,LED,1,26,V59,3001.0,4000,4000,25788-402,200,558,7320046218195,26,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,26,597,597,71,1,115.4230769
RECESSO 600X600 4K 2C BETA OPTI LUMEN SWITCH_25788-454,RECESSO 600X600 4K 2C BETA OPTI LUMEN SWITCH-LED body w DALI driver and Winsta connector 5-pole. Blue male for dim.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.0,http://www.fagerhult.com,1,DALI - WAGO Winsta,25788.IES,Recesso Beta Opti,Fagerhult,3001.0,LED,1,26,V59,3001.0,4000,4000,25788-454,200,558,7320046218218,26,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,26,597,597,71,1,115.4230769
RECESSO 600X600 4K 2C BETA OPTI LUMEN SWITCH_25788-456,RECESSO 600X600 4K 2C BETA OPTI LUMEN SWITCH-LED body w DALI driver and Wieland connector 5-pole. Blue male for dim.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.0,http://www.fagerhult.com,1,DALI - Wieland,25788.IES,Recesso Beta Opti,Fagerhult,3001.0,LED,1,26,V59,3001.0,4000,4000,25788-456,200,558,7320046218232,26,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,26,597,597,71,1,115.4230769
RECESSO 600X600 3K 2C BETA OPTI LUMEN SWITCH_25815,RECESSO 600X600 3K 2C BETA OPTI LUMEN SWITCH-,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.0,http://www.fagerhult.com,1,Standard,25815.IES,Recesso Beta Opti,Fagerhult,3851.0,LED,1,36,V59,3851.0,3000,3000,25815,200,558,7320046216375,36,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,36,597,597,71,1,106.9722222
RECESSO 600X600 3K 2C BETA OPTI LUMEN SWITCH_25815-111,RECESSO 600X600 3K 2C BETA OPTI LUMEN SWITCH-BODY W WIELAND CONNECTOR GST18I3 MALE.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.0,http://www.fagerhult.com,1,Standard,25815.IES,Recesso Beta Opti,Fagerhult,3851.0,LED,1,36,V59,3851.0,3000,3000,25815-111,200,558,7320046216399,36,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,36,597,597,71,1,106.9722222
RECESSO 600X600 3K 2C BETA OPTI LUMEN SWITCH_25815-3,"RECESSO 600X600 3K 2C BETA OPTI LUMEN SWITCH-BODY W CONNECTION CABLE L=2,5M FREE CABLE W PLUG.",Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.0,http://www.fagerhult.com,1,Standard,25815.IES,Recesso Beta Opti,Fagerhult,3851.0,LED,1,36,V59,3851.0,3000,3000,25815-3,200,558,7320046216412,36,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,36,597,597,71,1,106.9722222
RECESSO 600X600 3K 2C BETA OPTI LUMEN SWITCH_25815-340,RECESSO 600X600 3K 2C BETA OPTI LUMEN SWITCH-Body w Winsta connector 3-pole.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.0,http://www.fagerhult.com,1,Standard - WAGO Winsta,25815.IES,Recesso Beta Opti,Fagerhult,3851.0,LED,1,36,V59,3851.0,3000,3000,25815-340,200,558,7320046216436,36,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,36,597,597,71,1,106.9722222
RECESSO 600X600 3K 2C BETA OPTI LUMEN SWITCH_25815-402,RECESSO 600X600 3K 2C BETA OPTI LUMEN SWITCH-LED dim DALI/Phase-pulse control.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.0,http://www.fagerhult.com,1,DALI/Phase-pulse control,25815.IES,Recesso Beta Opti,Fagerhult,3851.0,LED,1,36,V59,3851.0,3000,3000,25815-402,200,558,7320046216450,36,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,36,597,597,71,1,106.9722222
RECESSO 600X600 3K 2C BETA OPTI LUMEN SWITCH_25815-454,RECESSO 600X600 3K 2C BETA OPTI LUMEN SWITCH-LED body w DALI driver and Winsta connector 5-pole. Blue male for dim.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.0,http://www.fagerhult.com,1,DALI - WAGO Winsta,25815.IES,Recesso Beta Opti,Fagerhult,3851.0,LED,1,36,V59,3851.0,3000,3000,25815-454,200,558,7320046216474,36,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,36,597,597,71,1,106.9722222
RECESSO 600X600 3K 2C BETA OPTI LUMEN SWITCH_25815-456,RECESSO 600X600 3K 2C BETA OPTI LUMEN SWITCH-LED body w DALI driver and Wieland connector 5-pole. Blue male for dim.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.0,http://www.fagerhult.com,1,DALI - Wieland,25815.IES,Recesso Beta Opti,Fagerhult,3851.0,LED,1,36,V59,3851.0,3000,3000,25815-456,200,558,7320046216498,36,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,36,597,597,71,1,106.9722222
RECESSO 600X600 4K 2C BETA OPTI LUMEN SWITCH_25816,RECESSO 600X600 4K 2C BETA OPTI LUMEN SWITCH-,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.0,http://www.fagerhult.com,1,Standard,25816.IES,Recesso Beta Opti,Fagerhult,3931.0,LED,1,36,V59,3931.0,4000,4000,25816,200,558,7320046216511,36,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,36,597,597,71,1,109.1944444
RECESSO 600X600 4K 2C BETA OPTI LUMEN SWITCH_25816-111,RECESSO 600X600 4K 2C BETA OPTI LUMEN SWITCH-BODY W WIELAND CONNECTOR GST18I3 MALE.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.0,http://www.fagerhult.com,1,Standard,25816.IES,Recesso Beta Opti,Fagerhult,3931.0,LED,1,36,V59,3931.0,4000,4000,25816-111,200,558,7320046216535,36,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,36,597,597,71,1,109.1944444
RECESSO 600X600 4K 2C BETA OPTI LUMEN SWITCH_25816-3,"RECESSO 600X600 4K 2C BETA OPTI LUMEN SWITCH-BODY W CONNECTION CABLE L=2,5M FREE CABLE W PLUG.",Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.0,http://www.fagerhult.com,1,Standard,25816.IES,Recesso Beta Opti,Fagerhult,3931.0,LED,1,36,V59,3931.0,4000,4000,25816-3,200,558,7320046216559,36,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,36,597,597,71,1,109.1944444
RECESSO 600X600 4K 2C BETA OPTI LUMEN SWITCH_25816-340,RECESSO 600X600 4K 2C BETA OPTI LUMEN SWITCH-Body w Winsta connector 3-pole.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.0,http://www.fagerhult.com,1,Standard - WAGO Winsta,25816.IES,Recesso Beta Opti,Fagerhult,3931.0,LED,1,36,V59,3931.0,4000,4000,25816-340,200,558,7320046216573,36,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,36,597,597,71,1,109.1944444
RECESSO 600X600 4K 2C BETA OPTI LUMEN SWITCH_25816-402,RECESSO 600X600 4K 2C BETA OPTI LUMEN SWITCH-LED dim DALI/Phase-pulse control.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.0,http://www.fagerhult.com,1,DALI/Phase-pulse control,25816.IES,Recesso Beta Opti,Fagerhult,3931.0,LED,1,36,V59,3931.0,4000,4000,25816-402,200,558,7320046216597,36,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,36,597,597,71,1,109.1944444
RECESSO 600X600 4K 2C BETA OPTI LUMEN SWITCH_25816-454,RECESSO 600X600 4K 2C BETA OPTI LUMEN SWITCH-LED body w DALI driver and Winsta connector 5-pole. Blue male for dim.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.0,http://www.fagerhult.com,1,DALI - WAGO Winsta,25816.IES,Recesso Beta Opti,Fagerhult,3931.0,LED,1,36,V59,3931.0,4000,4000,25816-454,200,558,7320046216610,36,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,36,597,597,71,1,109.1944444
RECESSO 600X600 4K 2C BETA OPTI LUMEN SWITCH_25816-456,RECESSO 600X600 4K 2C BETA OPTI LUMEN SWITCH-LED body w DALI driver and Wieland connector 5-pole. Blue male for dim.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.0,http://www.fagerhult.com,1,DALI - Wieland,25816.IES,Recesso Beta Opti,Fagerhult,3931.0,LED,1,36,V59,3931.0,4000,4000,25816-456,200,558,7320046216634,36,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,36,597,597,71,1,109.1944444