,Type Comments##OTHER##,MaterialBody##OTHER##,MaterialLouvre##OTHER##,MaterialAccentBody##OTHER##,MaterialReflector##OTHER##,Weight_Kg##OTHER##,URL##OTHER##,Total Light Loss Factor##OTHER##,SuffixCode##OTHER##,Photometric Web File##OTHER##,Model##OTHER##,Manufacturer##OTHER##,Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS,LightSource##OTHER##,Light Loss Factor##OTHER##,Lamp##OTHER##,Keynote##OTHER##,Initial Intensity##OTHER##,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Initial Color##OTHER##,FagerhultPartNumber##OTHER##,Emit from Rectangle Width##LENGTH##MILLIMETERS,Emit from Rectangle Length##LENGTH##MILLIMETERS,COBieBarCode##OTHER##,Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,Description##OTHER##,Assembly Code##OTHER##,LOR##OTHER##,Wattage##ELECTRICAL_WATTAGE##WATTS,TotalLength##LENGTH##MILLIMETERS,TotalWidth##LENGTH##MILLIMETERS,Height##LENGTH##MILLIMETERS,NumberOfLamps##OTHER##,Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT
RECESSO 600X600 3K 4C BETA OPTI LUMEN SWITCH_25789-111,RECESSO 600X600 3K 4C BETA OPTI LUMEN SWITCH-BODY W WIELAND CONNECTOR GST18I3 MALE.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.7,http://www.fagerhult.com,1,Standard,25789.IES,Recesso Beta Opti,Fagerhult,3900.0,LED,1,30,V59,3900.0,3000,3000,25789-111,400,557,7320046218270,30,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,30,597,597,71,1,130
RECESSO 600X600 3K 4C BETA OPTI LUMEN SWITCH_25789-3,"RECESSO 600X600 3K 4C BETA OPTI LUMEN SWITCH-BODY W CONNECTION CABLE L=2,5M FREE CABLE W PLUG.",Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.7,http://www.fagerhult.com,1,Standard,25789.IES,Recesso Beta Opti,Fagerhult,3900.0,LED,1,30,V59,3900.0,3000,3000,25789-3,400,557,7320046218294,30,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,30,597,597,72,1,130
RECESSO 600X600 3K 4C BETA OPTI LUMEN SWITCH_25789-340,RECESSO 600X600 3K 4C BETA OPTI LUMEN SWITCH-Body w Winsta connector 3-pole.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.7,http://www.fagerhult.com,1,Standard - WAGO Winsta,25789.IES,Recesso Beta Opti,Fagerhult,3900.0,LED,1,30,V59,3900.0,3000,3000,25789-340,400,557,7320046218317,30,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,30,597,597,73,1,130
RECESSO 600X600 3K 4C BETA OPTI LUMEN SWITCH_25789-402,RECESSO 600X600 3K 4C BETA OPTI LUMEN SWITCH-LED dim DALI/Phase-pulse control.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.7,http://www.fagerhult.com,1,DALI/Phase-pulse control,25789.IES,Recesso Beta Opti,Fagerhult,3900.0,LED,1,30,V59,3900.0,3000,3000,25789-402,400,557,7320046218331,30,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,30,597,597,74,1,130
RECESSO 600X600 3K 4C BETA OPTI LUMEN SWITCH_25789-454,RECESSO 600X600 3K 4C BETA OPTI LUMEN SWITCH-LED body w DALI driver and Winsta connector 5-pole. Blue male for dim.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.7,http://www.fagerhult.com,1,DALI - WAGO Winsta,25789.IES,Recesso Beta Opti,Fagerhult,3900.0,LED,1,30,V59,3900.0,3000,3000,25789-454,400,557,7320046218355,30,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,30,597,597,75,1,130
RECESSO 600X600 3K 4C BETA OPTI LUMEN SWITCH_25789-456,RECESSO 600X600 3K 4C BETA OPTI LUMEN SWITCH-LED body w DALI driver and Wieland connector 5-pole. Blue male for dim.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.7,http://www.fagerhult.com,1,DALI - Wieland,25789.IES,Recesso Beta Opti,Fagerhult,3900.0,LED,1,30,V59,3900.0,3000,3000,25789-456,400,557,7320046218379,30,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,30,597,597,76,1,130
RECESSO 600X600 4K 4C BETA OPTI LUMEN SWITCH_25791,RECESSO 600X600 4K 4C BETA OPTI LUMEN SWITCH-,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.7,http://www.fagerhult.com,1,Standard,25791.IES,Recesso Beta Opti,Fagerhult,3950.0,LED,1,30,V59,3950.0,4000,4000,25791,400,557,7320046218393,30,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,30,597,597,71,1,131.6666667
RECESSO 600X600 4K 4C BETA OPTI LUMEN SWITCH_25791-111,RECESSO 600X600 4K 4C BETA OPTI LUMEN SWITCH-BODY W WIELAND CONNECTOR GST18I3 MALE.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.7,http://www.fagerhult.com,1,Standard,25791.IES,Recesso Beta Opti,Fagerhult,3950.0,LED,1,30,V59,3950.0,4000,4000,25791-111,400,557,7320046218416,30,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,30,597,597,71,1,131.6666667
RECESSO 600X600 4K 4C BETA OPTI LUMEN SWITCH_25791-3,"RECESSO 600X600 4K 4C BETA OPTI LUMEN SWITCH-BODY W CONNECTION CABLE L=2,5M FREE CABLE W PLUG.",Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.7,http://www.fagerhult.com,1,Standard,25791.IES,Recesso Beta Opti,Fagerhult,3950.0,LED,1,30,V59,3950.0,4000,4000,25791-3,400,557,7320046218430,30,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,30,597,597,71,1,131.6666667
RECESSO 600X600 4K 4C BETA OPTI LUMEN SWITCH_25791-340,RECESSO 600X600 4K 4C BETA OPTI LUMEN SWITCH-Body w Winsta connector 3-pole.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.7,http://www.fagerhult.com,1,Standard - WAGO Winsta,25791.IES,Recesso Beta Opti,Fagerhult,3950.0,LED,1,30,V59,3950.0,4000,4000,25791-340,400,557,7320046218454,30,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,30,597,597,71,1,131.6666667
RECESSO 600X600 4K 4C BETA OPTI LUMEN SWITCH_25791-402,RECESSO 600X600 4K 4C BETA OPTI LUMEN SWITCH-LED dim DALI/Phase-pulse control.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.7,http://www.fagerhult.com,1,DALI/Phase-pulse control,25791.IES,Recesso Beta Opti,Fagerhult,3950.0,LED,1,30,V59,3950.0,4000,4000,25791-402,400,557,7320046218478,30,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,30,597,597,71,1,131.6666667
RECESSO 600X600 4K 4C BETA OPTI LUMEN SWITCH_25791-454,RECESSO 600X600 4K 4C BETA OPTI LUMEN SWITCH-LED body w DALI driver and Winsta connector 5-pole. Blue male for dim.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.7,http://www.fagerhult.com,1,DALI - WAGO Winsta,25791.IES,Recesso Beta Opti,Fagerhult,3950.0,LED,1,30,V59,3950.0,4000,4000,25791-454,400,557,7320046218492,30,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,30,597,597,71,1,131.6666667
RECESSO 600X600 4K 4C BETA OPTI LUMEN SWITCH_25791-456,RECESSO 600X600 4K 4C BETA OPTI LUMEN SWITCH-LED body w DALI driver and Wieland connector 5-pole. Blue male for dim.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.7,http://www.fagerhult.com,1,DALI - Wieland,25791.IES,Recesso Beta Opti,Fagerhult,3950.0,LED,1,30,V59,3950.0,4000,4000,25791-456,400,557,7320046218515,30,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,30,597,597,71,1,131.6666667
RECESSO 600X600 3K 4C BETA OPTI LUMEN SWITCH_25817,RECESSO 600X600 3K 4C BETA OPTI LUMEN SWITCH-,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.7,http://www.fagerhult.com,1,Standard,25817.IES,Recesso Beta Opti,Fagerhult,5442.0,LED,1,43,V59,5442.0,3000,3000,25817,400,557,7320046216658,43,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,43,597,597,71,1,126.5581395
RECESSO 600X600 3K 4C BETA OPTI LUMEN SWITCH_25817-111,RECESSO 600X600 3K 4C BETA OPTI LUMEN SWITCH-BODY W WIELAND CONNECTOR GST18I3 MALE.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.7,http://www.fagerhult.com,1,Standard,25817.IES,Recesso Beta Opti,Fagerhult,5442.0,LED,1,43,V59,5442.0,3000,3000,25817-111,400,557,7320046216672,43,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,43,597,597,71,1,126.5581395
RECESSO 600X600 3K 4C BETA OPTI LUMEN SWITCH_25817-3,"RECESSO 600X600 3K 4C BETA OPTI LUMEN SWITCH-BODY W CONNECTION CABLE L=2,5M FREE CABLE W PLUG.",Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.7,http://www.fagerhult.com,1,Standard,25817.IES,Recesso Beta Opti,Fagerhult,5442.0,LED,1,43,V59,5442.0,3000,3000,25817-3,400,557,7320046216696,43,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,43,597,597,71,1,126.5581395
RECESSO 600X600 3K 4C BETA OPTI LUMEN SWITCH_25817-340,RECESSO 600X600 3K 4C BETA OPTI LUMEN SWITCH-Body w Winsta connector 3-pole.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.7,http://www.fagerhult.com,1,Standard - WAGO Winsta,25817.IES,Recesso Beta Opti,Fagerhult,5442.0,LED,1,43,V59,5442.0,3000,3000,25817-340,400,557,7320046216719,43,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,43,597,597,71,1,126.5581395
RECESSO 600X600 3K 4C BETA OPTI LUMEN SWITCH_25817-402,RECESSO 600X600 3K 4C BETA OPTI LUMEN SWITCH-LED dim DALI/Phase-pulse control.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.7,http://www.fagerhult.com,1,DALI/Phase-pulse control,25817.IES,Recesso Beta Opti,Fagerhult,5442.0,LED,1,43,V59,5442.0,3000,3000,25817-402,400,557,7320046216733,43,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,43,597,597,71,1,126.5581395
RECESSO 600X600 3K 4C BETA OPTI LUMEN SWITCH_25817-454,RECESSO 600X600 3K 4C BETA OPTI LUMEN SWITCH-LED body w DALI driver and Winsta connector 5-pole. Blue male for dim.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.7,http://www.fagerhult.com,1,DALI - WAGO Winsta,25817.IES,Recesso Beta Opti,Fagerhult,5442.0,LED,1,43,V59,5442.0,3000,3000,25817-454,400,557,7.32005E+12,43,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,43,597,597,71,1,126.5581395
RECESSO 600X600 3K 4C BETA OPTI LUMEN SWITCH_25817-456,RECESSO 600X600 3K 4C BETA OPTI LUMEN SWITCH-LED body w DALI driver and Wieland connector 5-pole. Blue male for dim.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.7,http://www.fagerhult.com,1,DALI - Wieland,25817.IES,Recesso Beta Opti,Fagerhult,5442.0,LED,1,43,V59,5442.0,3000,3000,25817-456,400,557,7.32005E+12,43,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,43,597,597,71,1,126.5581395
RECESSO 600X600 4K 4C BETA OPTI LUMEN SWITCH_25818,RECESSO 600X600 4K 4C BETA OPTI LUMEN SWITCH-,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.7,http://www.fagerhult.com,1,Standard,25818.IES,Recesso Beta Opti,Fagerhult,5512.0,LED,1,43,V59,5512.0,4000,4000,25818,400,557,7.32005E+12,43,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,43,597,597,71,1,128.1860465
RECESSO 600X600 4K 4C BETA OPTI LUMEN SWITCH_25818-111,RECESSO 600X600 4K 4C BETA OPTI LUMEN SWITCH-BODY W WIELAND CONNECTOR GST18I3 MALE.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.7,http://www.fagerhult.com,1,Standard,25818.IES,Recesso Beta Opti,Fagerhult,5512.0,LED,1,43,V59,5512.0,4000,4000,25818-111,400,557,7.32005E+12,43,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,43,597,597,71,1,128.1860465
RECESSO 600X600 4K 4C BETA OPTI LUMEN SWITCH_25818-3,"RECESSO 600X600 4K 4C BETA OPTI LUMEN SWITCH-BODY W CONNECTION CABLE L=2,5M FREE CABLE W PLUG.",Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.7,http://www.fagerhult.com,1,Standard,25818.IES,Recesso Beta Opti,Fagerhult,5512.0,LED,1,43,V59,5512.0,4000,4000,25818-3,400,557,7.32005E+12,43,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,43,597,597,71,1,128.1860465
RECESSO 600X600 4K 4C BETA OPTI LUMEN SWITCH_25818-340,RECESSO 600X600 4K 4C BETA OPTI LUMEN SWITCH-Body w Winsta connector 3-pole.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.7,http://www.fagerhult.com,1,Standard - WAGO Winsta,25818.IES,Recesso Beta Opti,Fagerhult,5512.0,LED,1,43,V59,5512.0,4000,4000,25818-340,400,557,7.32005E+12,43,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,43,597,597,71,1,128.1860465
RECESSO 600X600 4K 4C BETA OPTI LUMEN SWITCH_25818-402,RECESSO 600X600 4K 4C BETA OPTI LUMEN SWITCH-LED dim DALI/Phase-pulse control.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.7,http://www.fagerhult.com,1,DALI/Phase-pulse control,25818.IES,Recesso Beta Opti,Fagerhult,5512.0,LED,1,43,V59,5512.0,4000,4000,25818-402,400,557,7.32005E+12,43,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,43,597,597,71,1,128.1860465
RECESSO 600X600 4K 4C BETA OPTI LUMEN SWITCH_25818-454,RECESSO 600X600 4K 4C BETA OPTI LUMEN SWITCH-LED body w DALI driver and Winsta connector 5-pole. Blue male for dim.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.7,http://www.fagerhult.com,1,DALI - WAGO Winsta,25818.IES,Recesso Beta Opti,Fagerhult,5512.0,LED,1,43,V59,5512.0,4000,4000,25818-454,400,557,7.32005E+12,43,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,43,597,597,71,1,128.1860465
RECESSO 600X600 4K 4C BETA OPTI LUMEN SWITCH_25818-456,RECESSO 600X600 4K 4C BETA OPTI LUMEN SWITCH-LED body w DALI driver and Wieland connector 5-pole. Blue male for dim.,Fagerhult_White_steel,Fagerhult_Beta_matt_aluminium,,Fagerhult_Aluminium,3.7,http://www.fagerhult.com,1,DALI - Wieland,25818.IES,Recesso Beta Opti,Fagerhult,5512.0,LED,1,43,V59,5512.0,4000,4000,25818-456,400,557,7.32005E+12,43,"Body of white enamelled RAL 9016 sheet steel. Openings along the entire body, outside the edge of the louvre for flow-through ventilation.",D5020230,100.0,43,597,597,71,1,128.1860465
